Skip to main content
`Ctrl`+`K`

# 6.6. CUPTI PM Sampling API

Functions to enable, disable, start, stop, and decode PM sampling.

## 6.6.1. Data Structures

CUpti_PmSampling_CounterDataImage_Initialize_Params

  Params for cuptiPmSamplingCounterDataImageInitialize.

CUpti_PmSampling_CounterData_GetSampleInfo_Params

  Params for cuptiPmSamplingCounterDataGetSampleInfo.

CUpti_PmSampling_DecodeData_Params

  Params for cuptiPmSamplingDecodeData.

CUpti_PmSampling_Disable_Params

  Params for cuptiPmSamplingDisable.

CUpti_PmSampling_Enable_Params

  Params for cuptiPmSamplingEnable.

CUpti_PmSampling_GetCounterAvailability_Params

  Params for cuptiPmSamplingGetCounterData.

CUpti_PmSampling_GetCounterDataInfo_Params

  Params for cuptiPmSamplingGetCounterDataInfo.

CUpti_PmSampling_GetCounterDataSize_Params

  Params for cuptiPmSamplingGetCounterDataSize.

CUpti_PmSampling_SetConfig_Params

  Params for cuptiPmSamplingSetConfig.

CUpti_PmSampling_Start_Params

  Params for cuptiPmSamplingStart.

CUpti_PmSampling_Stop_Params

  Params for cuptiPmSamplingStop.

## 6.6.2. Macros

CUpti_PmSampling_CounterDataImage_Initialize_Params_STRUCT_SIZE

CUpti_PmSampling_CounterData_GetSampleInfo_Params_STRUCT_SIZE

CUpti_PmSampling_DecodeData_Params_STRUCT_SIZE

CUpti_PmSampling_Disable_Params_STRUCT_SIZE

CUpti_PmSampling_Enable_Params_STRUCT_SIZE

CUpti_PmSampling_GetCounterAvailability_Params_STRUCT_SIZE

CUpti_PmSampling_GetCounterDataInfo_Params_STRUCT_SIZE

CUpti_PmSampling_GetCounterDataSize_Params_STRUCT_SIZE

CUpti_PmSampling_SetConfig_Params_STRUCT_SIZE

CUpti_PmSampling_Start_Params_STRUCT_SIZE

CUpti_PmSampling_Stop_Params_STRUCT_SIZE

## 6.6.3. Enumerations

CUpti_PmSampling_DecodeStopReason

CUpti_PmSampling_HardwareBuffer_AppendMode

CUpti_PmSampling_TriggerMode

## 6.6.4. Functions

CUptiResult cuptiPmSamplingCounterDataGetSampleInfo(CUpti_PmSampling_CounterData_GetSampleInfo_Params *pParams)

  Get the sample info (start and end time stamp) for the given sample index.

CUptiResult cuptiPmSamplingCounterDataImageInitialize(CUpti_PmSampling_CounterDataImage_Initialize_Params *pParams)

  Initialize the counter data to CUPTI record format for storing the metric data.

CUptiResult cuptiPmSamplingDecodeData(CUpti_PmSampling_DecodeData_Params *pParams)

  Decode the metrics data stored in the hardware buffer to the counter data image.

CUptiResult cuptiPmSamplingDisable(CUpti_PmSampling_Disable_Params *pParams)

  Disable PM sampling on the CUDA device and destroy the PM sampling object.

CUptiResult cuptiPmSamplingEnable(CUpti_PmSampling_Enable_Params *pParams)

  Create a PM sampling object and enable PM sampling on the CUDA device.

CUptiResult cuptiPmSamplingGetCounterAvailability(CUpti_PmSampling_GetCounterAvailability_Params *pParams)

  Query counter availibility information in a buffer which can be used to filter unavailable raw metrics on host.

CUptiResult cuptiPmSamplingGetCounterDataInfo(CUpti_PmSampling_GetCounterDataInfo_Params *pParams)

  Get the counter data info like number of samples, number of populated samples and number of completed samples in a counter data image.

CUptiResult cuptiPmSamplingGetCounterDataSize(CUpti_PmSampling_GetCounterDataSize_Params *pParams)

  Query the size of the counter data image which will be used to store the metrics data.

CUptiResult cuptiPmSamplingSetConfig(CUpti_PmSampling_SetConfig_Params *pParams)

  Set the configuration for PM sampling like sampling interval, HW buffer size, trigger mode and the config image which has scheduling info for metric collection.

CUptiResult cuptiPmSamplingStart(CUpti_PmSampling_Start_Params *pParams)

  Start the PM sampling.

CUptiResult cuptiPmSamplingStop(CUpti_PmSampling_Stop_Params *pParams)

  Stop the PM sampling.

## 6.6.5. Typedefs

CUpti_PmSampling_Object

## 6.6.6. Macros

CUpti_PmSampling_CounterDataImage_Initialize_Params_STRUCT_SIZE

CUpti_PmSampling_CounterData_GetSampleInfo_Params_STRUCT_SIZE

CUpti_PmSampling_DecodeData_Params_STRUCT_SIZE

CUpti_PmSampling_Disable_Params_STRUCT_SIZE

CUpti_PmSampling_Enable_Params_STRUCT_SIZE

CUpti_PmSampling_GetCounterAvailability_Params_STRUCT_SIZE

CUpti_PmSampling_GetCounterDataInfo_Params_STRUCT_SIZE

CUpti_PmSampling_GetCounterDataSize_Params_STRUCT_SIZE

CUpti_PmSampling_SetConfig_Params_STRUCT_SIZE

CUpti_PmSampling_Start_Params_STRUCT_SIZE

CUpti_PmSampling_Stop_Params_STRUCT_SIZE

## 6.6.7. Enumerations

enum CUpti_PmSampling_DecodeStopReason

  Values:

  enumerator CUPTI_PM_SAMPLING_DECODE_STOP_REASON_OTHER
  enumerator CUPTI_PM_SAMPLING_DECODE_STOP_REASON_COUNTER_DATA_FULL

    Counter data image is full.

  enumerator CUPTI_PM_SAMPLING_DECODE_STOP_REASON_END_OF_RECORDS

    All the records in the hardware buffer is decoded.

  enumerator CUPTI_PM_SAMPLING_DECODE_STOP_REASON_COUNT

enum CUpti_PmSampling_HardwareBuffer_AppendMode

  Values:

  enumerator CUPTI_PM_SAMPLING_HARDWARE_BUFFER_APPEND_MODE_KEEP_OLDEST

    Keep the oldest records in the hardware buffer. CUPTI will report error for overflow in case hardware buffer is getting filled up.

  enumerator CUPTI_PM_SAMPLING_HARDWARE_BUFFER_APPEND_MODE_KEEP_LATEST

    Keep the latest records in the hardware buffer. Note: This mode is not supported on Turing GPU architecture. It is supported on Ampere and later GPU architectures.

enum CUpti_PmSampling_TriggerMode

  Values:

  enumerator CUPTI_PM_SAMPLING_TRIGGER_MODE_GPU_SYSCLK_INTERVAL

    The trigger is based off of the SYSCLK frequency, note SYS frequency by default is variable. the sample interval (set in the struct CUpti_PmSampling_SetConfig_Params) is in terms of clocks.

  enumerator CUPTI_PM_SAMPLING_TRIGGER_MODE_GPU_TIME_INTERVAL

    The trigger is based off of a fixed frequency source. The sample interval (set in the struct CUpti_PmSampling_SetConfig_Params) is in terms of nanoseconds. Note: This trigger mode is not supported on Turing GPU architecture and GA100 GPU. It is supported on Ampere GA10x and later GPU architectures.

  enumerator CUPTI_PM_SAMPLING_TRIGGER_MODE_COUNT

## 6.6.8. Functions

CUptiResult cuptiPmSamplingCounterDataGetSampleInfo(

  CUpti_PmSampling_CounterData_GetSampleInfo_Params *pParams,

)

  Get the sample info (start and end time stamp) for the given sample index.

  Each sample is distinguished by the start and end time stamp.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_CounterData_GetSampleInfo_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingCounterDataImageInitialize(

  CUpti_PmSampling_CounterDataImage_Initialize_Params *pParams,

)

  Initialize the counter data to CUPTI record format for storing the metric data.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_CounterDataImage_Initialize_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_INVALID_OPERATION – if PM sampling CounterDataInitialize is called without enabling PM sampling

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingDecodeData(

  CUpti_PmSampling_DecodeData_Params *pParams,

)

  Decode the metrics data stored in the hardware buffer to the counter data image.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_DecodeData_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_INVALID_OPERATION – if PM sampling DecodeData is called without enabling PM sampling

    - CUPTI_ERROR_OUT_OF_MEMORY – if there is record overflow in the hardware buffer

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingDisable(

  CUpti_PmSampling_Disable_Params *pParams,

)

  Disable PM sampling on the CUDA device and destroy the PM sampling object.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_Disable_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingEnable(

  CUpti_PmSampling_Enable_Params *pParams,

)

  Create a PM sampling object and enable PM sampling on the CUDA device.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_Enable_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_OUT_OF_MEMORY – if memory allocation fails while creating the PM sampling object

    - CUPTI_ERROR_INVALID_OPERATION – if PM sampling is already enabled on the device

    - CUPTI_ERROR_INSUFFICIENT_PRIVILEGES – if the user does not have sufficient privileges to perform the operation

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingGetCounterAvailability(

  CUpti_PmSampling_GetCounterAvailability_Params *pParams,

)

  Query counter availibility information in a buffer which can be used to filter unavailable raw metrics on host.

  Note: This API may fail, if any profiling or sampling session is active on the specified device.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_GetCounterAvailability_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_INSUFFICIENT_PRIVILEGES – if the user does not have sufficient privileges to perform the operation

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingGetCounterDataInfo(

  CUpti_PmSampling_GetCounterDataInfo_Params *pParams,

)

  Get the counter data info like number of samples, number of populated samples and number of completed samples in a counter data image.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_GetCounterDataInfo_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingGetCounterDataSize(

  CUpti_PmSampling_GetCounterDataSize_Params *pParams,

)

  Query the size of the counter data image which will be used to store the metrics data.

  User need to allocate the memory for the counter data image based on the size returned by this API.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_GetCounterDataSize_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_INVALID_OPERATION – if PM sampling GetCounterDataSize is called without enabling PM sampling

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingSetConfig(

  CUpti_PmSampling_SetConfig_Params *pParams,

)

  Set the configuration for PM sampling like sampling interval, HW buffer size, trigger mode and the config image which has scheduling info for metric collection.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_SetConfig_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_NOT_SUPPORTED – for config image which require multiple passes for data collection

CUptiResult cuptiPmSamplingStart(

  CUpti_PmSampling_Start_Params *pParams,

)

  Start the PM sampling.

  The GPU will start collecting the metrics data periodically based on trigger type and sampling interval passed in CUpti_PmSampling_SetConfig_Params. The collected data will be stored in the hardware buffer.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_Start_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_INVALID_OPERATION – if PM sampling Start is called without enabling PM sampling, and PM sampling is already started

    - CUPTI_ERROR_UNKNOWN – for any internal error

CUptiResult cuptiPmSamplingStop(

  CUpti_PmSampling_Stop_Params *pParams,

)

  Stop the PM sampling.

  The GPU will stop collecting the metrics data.

  Parameters:

    pParams – A pointer to CUpti_PmSampling_Stop_Params

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if any `pParams` is not valid

    - CUPTI_ERROR_INVALID_OPERATION – if PM sampling Stop is called without enabling PM sampling, and PM sampling is already stopped

    - CUPTI_ERROR_UNKNOWN – for any internal error

## 6.6.9. Typedefs

typedef struct CUpti_PmSampling_Object CUpti_PmSampling_Object