Skip to main content
`Ctrl`+`K`

# 6.1. CUPTI Activity API

Functions, types, and enums that implement the CUPTI Activity API.

## 6.1.1. Data Structures

CUpti_Activity

  The base activity record.

CUpti_ActivityAPI

  The activity record for a driver or runtime API invocation.

CUpti_ActivityAutoBoostState

  Device auto boost state structure.

CUpti_ActivityBranch2

  The activity record for source level result branch.

CUpti_ActivityCdpKernel

  The activity record for CDP (CUDA Dynamic Parallelism) kernel.

CUpti_ActivityComputeEngineCtxSwitch

  The activity record for trace of CUDA context switch events.

CUpti_ActivityConfidentialComputeRotation

  Event related to confidential compute encryption rotation.

CUpti_ActivityConfig

  Activity configuration.

CUpti_ActivityContext4

  The activity record for a context.

CUpti_ActivityCudaEvent2

  The activity record for CUDA event.

CUpti_ActivityDevice6

  The activity record for a device.

CUpti_ActivityDeviceAttribute

  The activity record for a device attribute.

CUpti_ActivityDeviceGraphTrace

  The activity record for trace of device graph execution.

CUpti_ActivityEnvironment

  The activity record for CUPTI environmental data.

CUpti_ActivityEnvironmentCooling

  Data returned for CUPTI_ACTIVITY_ENVIRONMENT_COOLING environment kind.

CUpti_ActivityEnvironmentPower

  Data returned for CUPTI_ACTIVITY_ENVIRONMENT_POWER environment kind.

CUpti_ActivityEnvironmentSpeed

  Data returned for CUPTI_ACTIVITY_ENVIRONMENT_SPEED environment kind.

CUpti_ActivityEnvironmentTemperature

  Data returned for CUPTI_ACTIVITY_ENVIRONMENT_TEMPERATURE environment kind.

CUpti_ActivityEvent

  The activity record for a CUPTI event.

CUpti_ActivityEventInstance

  The activity record for a CUPTI event with instance information.

CUpti_ActivityExternalCorrelation

  The activity record for correlation with external records.

CUpti_ActivityFieldLayoutEntry

CUpti_ActivityFieldSelection

CUpti_ActivityFunction

  The activity record for global/device functions.

CUpti_ActivityGlobalAccess3

  The activity record for source-level global access.

CUpti_ActivityGraphHostNode

CUpti_ActivityGraphTrace2

  The activity record for trace of graph execution.

CUpti_ActivityGreenContext2

  The activity record for a green context (version 2).

CUpti_ActivityHostLaunch

  The activity record for host launch functions.

CUpti_ActivityInstantaneousEvent

  The activity record for an instantaneous CUPTI event.

CUpti_ActivityInstantaneousEventInstance

  The activity record for an instantaneous CUPTI event with event domain instance information.

CUpti_ActivityInstantaneousMetric

  The activity record for an instantaneous CUPTI metric.

CUpti_ActivityInstantaneousMetricInstance

  The instantaneous activity record for a CUPTI metric with instance information.

CUpti_ActivityInstructionCorrelation

  The activity record for source-level sass/source line-by-line correlation.

CUpti_ActivityInstructionExecution

  The activity record for source-level instruction execution.

CUpti_ActivityJit2

  The activity record for JIT operations.

CUpti_ActivityKernel12

  The activity record for kernel (version 12).

CUpti_ActivityMarker2

  The activity record providing a marker which is an instantaneous point in time.

CUpti_ActivityMarkerData2

  The activity record providing detailed information for a marker.

CUpti_ActivityMemDecompress

  The activity record for trace of decompression operations.

CUpti_ActivityMemcpy6

  The activity record for memory copies.

CUpti_ActivityMemcpyPtoP4

  The activity record for peer-to-peer memory copies.

CUpti_ActivityMemory

  The activity record for memory.

CUpti_ActivityMemory4

  The activity record for memory.

CUpti_ActivityMemoryPool3

  The activity record for memory pool.

CUpti_ActivityMemset4

  The activity record for memset.

CUpti_ActivityMetric

  The activity record for a CUPTI metric.

CUpti_ActivityMetricInstance

  The activity record for a CUPTI metric with instance information.

CUpti_ActivityModule

  The activity record for a CUDA module.

CUpti_ActivityName

  The activity record providing a name.

CUpti_ActivityNvLink5

  NVLink information.

CUpti_ActivityNvLinkNpu

  NPU identifier for NVLink connections.

CUpti_ActivityObjectKindId

  Identifiers for object kinds as specified by CUpti_ActivityObjectKind.

CUpti_ActivityOpenAcc

  The base activity record for OpenAcc records.

CUpti_ActivityOpenAccData

  The activity record for OpenACC data.

CUpti_ActivityOpenAccLaunch

  The activity record for OpenACC launch.

CUpti_ActivityOpenAccOther

  The activity record for OpenACC other.

CUpti_ActivityOpenMp

  The base activity record for OpenMp records.

CUpti_ActivityOverhead3

  The activity record for CUPTI and driver overheads.

CUpti_ActivityOverheadCommandBufferFullData

  The structure to provide additional data for CUPTI_ACTIVITY_OVERHEAD_COMMAND_BUFFER_FULL.

CUpti_ActivityPCSampling3

  The activity record for PC sampling.

CUpti_ActivityPCSamplingConfig

  PC sampling configuration structure.

CUpti_ActivityPCSamplingRecordInfo

  The activity record for record status for PC sampling.

CUpti_ActivityPcie

  PCI devices information required to construct topology.

CUpti_ActivityPcieBridgeAttr

  Attributes for more information about PCI Bridge (bridgeAttr).

CUpti_ActivityPcieGpuAttr

  Attributes for more information about GPU (gpuAttr).

CUpti_ActivityPreemption

  The activity record for a preemption of a CDP kernel.

CUpti_ActivityRecordLayout

CUpti_ActivitySharedAccess

  The activity record for source-level shared access.

CUpti_ActivitySourceLocator

  The activity record for source locator.

CUpti_ActivityStream

  The activity record for CUDA stream.

CUpti_ActivitySynchronization2

  The activity record for synchronization management.

CUpti_ActivityUnifiedMemoryCounter3

  The activity record for Unified Memory counters (CUDA 7.0 and beyond)

CUpti_ActivityUnifiedMemoryCounterConfig

  Unified Memory counters configuration structure.

CUpti_BufferCallbackCompleteInfo

CUpti_BufferCallbackRequestInfo

CUpti_NvtxExtPayloadAttr

## 6.1.2. Macros

CUPTI_ACTIVITY_STRUCT_SIZE

CUPTI_AUTO_BOOST_INVALID_CLIENT_PID

  An invalid/unknown process id.

CUPTI_CORRELATION_ID_UNKNOWN

  An invalid/unknown correlation ID.

CUPTI_DECOMPRESSED_BYTES_UNKNOWN

  An invalid/unknown value for decompressed bytes.

CUPTI_FUNCTION_INDEX_ID_INVALID

  An invalid function index ID.

CUPTI_GRID_ID_UNKNOWN

  An invalid/unknown grid ID.

CUPTI_MAX_GPUS

CUPTI_NVLINK_INVALID_PORT

  Invalid/unknown NVLink port number.

CUPTI_SOURCE_LOCATOR_ID_UNKNOWN

  The source-locator ID that indicates an unknown source location.

CUPTI_SYNCHRONIZATION_INVALID_VALUE

  An invalid/unknown value.

CUPTI_TIMESTAMP_UNKNOWN

  An invalid/unknown timestamp for a start, end, queued, submitted, or completed time.

CUpti_ActivityConfig_STRUCT_SIZE

## 6.1.3. Enumerations

CUpti_ActivityApiFieldIds

  Enum identifiers for fields in CUpti_ActivityAPI .

CUpti_ActivityAttribute

  Activity attributes.

CUpti_ActivityComputeApiKind

  The kind of a compute API.

CUpti_ActivityComputeEngineCtxSwitchFieldIds

  Enum identifiers for fields in CUpti_ActivityComputeEngineCtxSwitch .

CUpti_ActivityConfidentialComputeRotationFieldIds

  Enum identifiers for fields in CUpti_ActivityConfidentialComputeRotation .

CUpti_ActivityContextFieldIds

  Enum identifiers for fields to trace context.

CUpti_ActivityCudaEventFieldIds

  Enum identifiers for fields to trace CUDA Event operations.

CUpti_ActivityDeviceFieldIds

  Enum identifiers for fields in CUpti_ActivityDevice6 .

CUpti_ActivityDeviceGraphTraceFieldIds

  Enum identifiers for fields in CUpti_ActivityDeviceGraphTrace .

CUpti_ActivityEnvironmentFieldIds

  Enum identifiers for fields in CUpti_ActivityEnvironment .

CUpti_ActivityEnvironmentKind

  The kind of environment data.

CUpti_ActivityExternalCorrelationFieldIds

  Enum identifiers for fields in CUpti_ActivityExternalCorrelation .

CUpti_ActivityFlag

  Flags associated with activity records.

CUpti_ActivityGraphHostNodeFieldIds

  Enum identifiers for fields in CUpti_ActivityGraphHostNode.

CUpti_ActivityGraphTraceFieldIds

  Enum identifiers for fields to trace graph execution.

CUpti_ActivityGreenContextFieldIds

  Enum identifiers for fields to trace green context information.

CUpti_ActivityHostLaunchFieldIds

  Enum identifiers for fields in CUpti_ActivityHostLaunch .

CUpti_ActivityInstructionClass

  SASS instruction classification.

CUpti_ActivityJitEntryType

  The types of JIT entry.

CUpti_ActivityJitFieldIds

  Enum identifiers for fields to trace JIT operations.

CUpti_ActivityJitOperationType

  The types of JIT compilation operations.

CUpti_ActivityKernelFieldIds

  Enum identifiers for fields to trace kernel operations.

CUpti_ActivityKind

  The kinds of activity records.

CUpti_ActivityLaunchType

  The type of the CUDA kernel launch.

CUpti_ActivityMarkerDataFieldIds

  Enum identifiers for fields to trace detailed information for a marker.

CUpti_ActivityMarkerFieldIds

  Enum identifiers for fields to trace NVTX markers/ranges.

CUpti_ActivityMemDecompressFieldIds

  Enum identifiers for fields to trace decompression operations.

CUpti_ActivityMemcpy2FieldIds

  Enum identifiers for fields to trace peer-to-peer memory copies.

CUpti_ActivityMemcpyFieldIds

  Enum identifiers for fields to trace memory copies.

CUpti_ActivityMemcpyKind

  The kind of a memory copy, indicating the source and destination targets of the copy.

CUpti_ActivityMemoryFieldIds

  Enum identifiers for fields to trace memory allocation and free operation.

CUpti_ActivityMemoryKind

  The kinds of memory accessed by a memory operation/copy.

CUpti_ActivityMemoryOperationType

  Memory operation types.

CUpti_ActivityMemoryPoolFieldIds

  Enum identifiers for fields to trace CUDA memory pool creation, destruction and trimming.

CUpti_ActivityMemoryPoolOperationType

  Memory pool operation types.

CUpti_ActivityMemoryPoolType

  Memory pool types.

CUpti_ActivityMemsetFieldIds

  Enum identifiers for fields to trace memset operations.

CUpti_ActivityNameFieldIds

  Enum identifiers for fields in CUpti_ActivityName .

CUpti_ActivityNvLinkFieldIds

  Enum identifiers for fields in CUpti_ActivityNvLink5 .

CUpti_ActivityObjectKind

  The kinds of activity objects.

CUpti_ActivityOpenAccDataFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenAccData .

CUpti_ActivityOpenAccLaunchFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenAccLaunch .

CUpti_ActivityOpenAccOtherFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenAccOther .

CUpti_ActivityOpenMpFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenMp .

CUpti_ActivityOverheadFieldIds

  Enum identifiers for fields to trace CUPTI and driver overhead information.

CUpti_ActivityOverheadKind

  The kinds of activity overhead.

CUpti_ActivityPCSamplingPeriod

  Sampling period for PC sampling method.

CUpti_ActivityPCSamplingStallReason

  The stall reason for PC sampling activity.

CUpti_ActivityPartitionedGlobalCacheConfig

  Partitioned global caching option.

CUpti_ActivityPcieFieldIds

  Enum identifiers for fields in CUpti_ActivityPcie .

CUpti_ActivityPreemptionKind

  The kind of a preemption activity.

CUpti_ActivityStreamFieldIds

  Enum identifiers for fields to trace CUDA Stream operations.

CUpti_ActivityStreamFlag

  stream type.

CUpti_ActivitySynchronizationFieldIds

  Enum identifiers for fields to trace various CUDA synchronization APIs.

CUpti_ActivitySynchronizationType

  Synchronization type.

CUpti_ActivityThreadIdType

  Thread-Id types.

CUpti_ActivityUnifiedMemoryAccessType

  Memory access type for unified memory page faults.

CUpti_ActivityUnifiedMemoryCounterKind

  Kind of the Unified Memory counter.

CUpti_ActivityUnifiedMemoryCounterScope

  Scope of the unified memory counter (deprecated in CUDA 7.0)

CUpti_ActivityUnifiedMemoryMigrationCause

  Migration cause of the Unified Memory counter.

CUpti_ActivityUnifiedMemoryRemoteMapCause

  Remote memory map cause of the Unified Memory counter.

CUpti_ActivityUvmCounterFieldIds

  Enum identifiers for fields in CUpti_ActivityUnifiedMemoryCounter3 .

CUpti_ChannelType

CUpti_ComputeEngineCtxSwitchOperationType

  The operation type of CUDA context switch event records.

CUpti_ConfidentialComputeRotationEventType

CUpti_ContextCigMode

  CIG (CUDA in Graphics) Modes.

CUpti_DevType

  The device type for device connected to NVLink.

CUpti_DeviceGraphLaunchMode

  The launch mode for device graph execution.

CUpti_DeviceVirtualizationMode

  This indicates the virtualization mode in which CUDA device is running.

CUpti_EnvironmentClocksThrottleReason

  Reasons for clock throttling.

CUpti_ExternalCorrelationKind

  The kind of external APIs supported for correlation.

CUpti_FuncExecutionModel

  The execution model of a kernel function.

CUpti_FuncShmemLimitConfig

  The shared memory limit per block config for a kernel This should be used to set 'cudaOccFuncShmemConfig' field in occupancy calculator API.

CUpti_LinkFlag

  Link flags.

CUpti_NvtxExtPayloadType

CUpti_OpenAccConstructKind

  The OpenAcc parent construct kind for OpenAcc activity records.

CUpti_OpenAccEventKind

  The OpenAcc event kind for OpenAcc activity records.

CUpti_OpenMpEventKind

CUpti_PcieDeviceType

  Field to differentiate whether PCIE Activity record is of a GPU or a PCI Bridge.

CUpti_PcieGen

  PCIE Generation.

## 6.1.4. Functions

CUptiResult cuptiActivityConfigurePCSampling(CUcontext ctx, CUpti_ActivityPCSamplingConfig *config)

  Set PC sampling configuration.

CUptiResult cuptiActivityConfigureUnifiedMemoryCounter(CUpti_ActivityUnifiedMemoryCounterConfig *config, uint32_t count)

  Set Unified Memory Counter configuration.

CUptiResult cuptiActivityDisable(CUpti_ActivityKind kind)

  Disable collection of a specific kind of activity record.

CUptiResult cuptiActivityDisableContext(CUcontext context, CUpti_ActivityKind kind)

  Disable collection of a specific kind of activity record for a context.

CUptiResult cuptiActivityDisable_v2(CUpti_SubscriberHandle subscriber, CUpti_ActivityKind kind, CUpti_ActivityConfig *pActivityConfig)

  Disable collection of a specific kind of activity record for the subscriber.

CUptiResult cuptiActivityEnable(CUpti_ActivityKind kind)

  Enable collection of a specific kind of activity record.

CUptiResult cuptiActivityEnableAllSyncRecords(uint8_t enable)

  Enables collecting records for all synchronization operations.

CUptiResult cuptiActivityEnableAndDump(CUpti_ActivityKind kind)

  Enable collection of a specific kind of activity record.

CUptiResult cuptiActivityEnableAndDump_v2(CUpti_SubscriberHandle subscriber, CUpti_ActivityKind kind, CUpti_ActivityConfig *activityConfig)

  Enable collection of a specific kind of activity record.

CUptiResult cuptiActivityEnableContext(CUcontext context, CUpti_ActivityKind kind)

  Enable collection of a specific kind of activity record for a context.

CUptiResult cuptiActivityEnableCudaEventDeviceTimestamps(uint8_t enable)

  Enable/Disable collecting device timestamp for CUPTI_ACTIVITY_KIND_CUDA_EVENT record.

CUptiResult cuptiActivityEnableDeviceGraph(uint8_t enable)

  Controls the collection of records for device launched graphs.

CUptiResult cuptiActivityEnableDriverApi(CUpti_CallbackId cbid, uint8_t enable)

  Controls the collection of activity records for specific CUDA Driver APIs.

CUptiResult cuptiActivityEnableDriverApi_v2(CUpti_SubscriberHandle subscriber, CUpti_CallbackId cbid, uint8_t enable)

  Controls the collection of activity records for specific CUDA Driver APIs for a given subscriber.

CUptiResult cuptiActivityEnableHWTrace(uint8_t enable)

  Enables CUDA kernel timestamp collection via Hardware Event System (HES).

CUptiResult cuptiActivityEnableLatencyTimestamps(uint8_t enable)

  Controls the collection of queued and submitted timestamps for kernels.

CUptiResult cuptiActivityEnableLaunchAttributes(uint8_t enable)

  Controls the collection of launch attributes for kernels.

CUptiResult cuptiActivityEnableRuntimeApi(CUpti_CallbackId cbid, uint8_t enable)

  Controls the collection of activity records for specific CUDA Runtime APIs.

CUptiResult cuptiActivityEnableRuntimeApi_v2(CUpti_SubscriberHandle subscriber, CUpti_CallbackId cbid, uint8_t enable)

  Controls the collection of activity records for specific CUDA Runtime APIs for a given subscriber.

CUptiResult cuptiActivityEnable_v2(CUpti_SubscriberHandle subscriber, CUpti_ActivityKind kind, CUpti_ActivityConfig *pActivityConfig)

  Enable collection of a specific kind of activity record for the subscriber.

CUptiResult cuptiActivityFlush(CUcontext context, uint32_t streamId, uint32_t flag)

  Wait for all activity records to be delivered via the completion callback.

CUptiResult cuptiActivityFlushAll(uint32_t flag)

  Request to deliver activity records via the buffer completion callback.

CUptiResult cuptiActivityFlushPeriod(uint32_t time)

  Sets the flush period for the worker thread.

CUptiResult cuptiActivityGetAttribute(CUpti_ActivityAttribute attr, size_t *valueSize, void *value)

  Read an activity API attribute.

CUptiResult cuptiActivityGetAttribute_v2(CUpti_SubscriberHandle subscriber, CUpti_ActivityAttribute attr, size_t *valueSize, void *value)

  Read an activity API attribute.

CUptiResult cuptiActivityGetEnabledKinds(CUpti_SubscriberHandle subscriber, CUpti_ActivityKind *buffer, uint32_t *bufferSize, uint32_t *enabledKindsCount)

  Get the enabled activity kinds for a subscriber.

CUptiResult cuptiActivityGetNextRecord(uint8_t *buffer, size_t validBufferSizeBytes, CUpti_Activity **record)

  Iterate over the activity records in a buffer.

CUptiResult cuptiActivityGetNextRecord_v2(CUpti_SubscriberHandle subscriber, uint8_t *buffer, size_t validBufferSizeBytes, CUpti_Activity **record)

  Iterate over the activity records in the supplied buffer.

CUptiResult cuptiActivityGetNumDroppedRecords(CUcontext context, uint32_t streamId, size_t *dropped)

  Get the number of activity records that were dropped of insufficient buffer space.

CUptiResult cuptiActivityGetNumDroppedRecords_v2(CUpti_SubscriberHandle subscriber, CUcontext context, uint32_t streamId, size_t *dropped)

  Get the number of dropped activity records for a specific subscriber.

CUptiResult cuptiActivityGetStructSize(CUpti_ActivityKind activityKind, uint32_t version, size_t *activityStructSize)

  Get the size of the activity struct for a given CUPTI version.

CUptiResult cuptiActivityPopExternalCorrelationId(CUpti_ExternalCorrelationKind kind, uint64_t *lastId)

  Pop an external correlation id for the calling thread.

CUptiResult cuptiActivityPopExternalCorrelationId_v2(CUpti_SubscriberHandle subscriber, CUpti_ExternalCorrelationKind kind, uint64_t *lastId)

  Pop an external correlation id for a specific subscriber.

CUptiResult cuptiActivityPushExternalCorrelationId(CUpti_ExternalCorrelationKind kind, uint64_t id)

  Push an external correlation id for the calling thread.

CUptiResult cuptiActivityPushExternalCorrelationId_v2(CUpti_SubscriberHandle subscriber, CUpti_ExternalCorrelationKind kind, uint64_t id)

  Push an external correlation id for a specific subscriber.

CUptiResult cuptiActivityRegisterCallbacks(CUpti_BuffersCallbackRequestFunc funcBufferRequested, CUpti_BuffersCallbackCompleteFunc funcBufferCompleted)

  Registers callback functions with CUPTI for activity buffer handling.

CUptiResult cuptiActivityRegisterCallbacks_v2(CUpti_SubscriberHandle subscriber, CUpti_BuffersCallbackRequestFunc_v2 funcBufferRequested, CUpti_BuffersCallbackCompleteFunc_v2 funcBufferCompleted)

  Registers callback functions with CUPTI for activity buffer handling for the subscriber.

CUptiResult cuptiActivityRegisterTimestampCallback(CUpti_TimestampCallbackFunc funcTimestamp)

  Registers callback function with CUPTI for providing timestamp.

CUptiResult cuptiActivitySetAttribute(CUpti_ActivityAttribute attr, size_t *valueSize, void *value)

  Write an activity API attribute.

CUptiResult cuptiActivitySetAttribute_v2(CUpti_SubscriberHandle subscriber, CUpti_ActivityAttribute attr, size_t *valueSize, void *value)

  Write an activity API attribute.

CUptiResult cuptiComputeCapabilitySupported(int major, int minor, int *support)

  Check support for a compute capability.

CUptiResult cuptiDeviceSupported(CUdevice dev, int *support)

  Check support for a compute device.

CUptiResult cuptiDeviceVirtualizationMode(CUdevice dev, CUpti_DeviceVirtualizationMode *mode)

  Query the virtualization mode of the device.

CUptiResult cuptiFinalize(void)

  Detach CUPTI from the running process.

CUptiResult cuptiGetAutoBoostState(CUcontext context, CUpti_ActivityAutoBoostState *state)

  Get auto boost state.

CUptiResult cuptiGetContextId(CUcontext context, uint32_t *contextId)

  Get the ID of a context.

CUptiResult cuptiGetDeviceId(CUcontext context, uint32_t *deviceId)

  Get the ID of a device.

CUptiResult cuptiGetGraphExecId(CUgraphExec graphExec, uint32_t *pId)

  Get the unique ID of executable graph.

CUptiResult cuptiGetGraphId(CUgraph graph, uint32_t *pId)

  Get the unique ID of graph.

CUptiResult cuptiGetGraphNodeId(CUgraphNode node, uint64_t *nodeId)

  Get the unique ID of a graph node.

CUptiResult cuptiGetLastError(void)

  Returns the last error from a cupti call or callback.

CUptiResult cuptiGetStreamId(CUcontext context, CUstream stream, uint32_t *streamId)

  Get the ID of a stream.

CUptiResult cuptiGetStreamIdEx(CUcontext context, CUstream stream, uint8_t perThreadStream, uint32_t *streamId)

  Get the ID of a stream.

CUptiResult cuptiGetThreadIdType(CUpti_ActivityThreadIdType *type)

  Get the thread-id type.

CUptiResult cuptiGetTimestamp(uint64_t *timestamp)

  Get the CUPTI timestamp.

CUptiResult cuptiGetTimestamp_v2(CUpti_SubscriberHandle subscriber, uint64_t *timestamp)

  Get the CUPTI timestamp (API currently in beta).

CUptiResult cuptiIsTracingSessionRunning(uint8_t *isRunning)

  Check whether a CUPTI tracing session is still running.

CUptiResult cuptiSetThreadIdType(CUpti_ActivityThreadIdType type)

  Set the thread-id type.

## 6.1.5. Typedefs

CUpti_BuffersCallbackCompleteFunc

  Function type for callback used by CUPTI to return a buffer of activity records.

CUpti_BuffersCallbackCompleteFunc_v2

  Function type for callback used by CUPTI to return a buffer of activity records.

CUpti_BuffersCallbackRequestFunc

  Function type for callback used by CUPTI to request an empty buffer for storing activity records.

CUpti_BuffersCallbackRequestFunc_v2

  Function type for callback used by CUPTI to request an empty buffer for storing activity records.

CUpti_TimestampCallbackFunc

  Function type for callback used by CUPTI to request a timestamp to be used in activity records.

## 6.1.6. Macros

CUPTI_ACTIVITY_STRUCT_SIZE(type_, lastfield_)

CUPTI_AUTO_BOOST_INVALID_CLIENT_PID

  An invalid/unknown process id.

CUPTI_CORRELATION_ID_UNKNOWN

  An invalid/unknown correlation ID.

  A correlation ID of this value indicates that there is no correlation for the activity record.

CUPTI_DECOMPRESSED_BYTES_UNKNOWN

  An invalid/unknown value for decompressed bytes.

CUPTI_FUNCTION_INDEX_ID_INVALID

  An invalid function index ID.

CUPTI_GRID_ID_UNKNOWN

  An invalid/unknown grid ID.

CUPTI_MAX_GPUS

CUPTI_NVLINK_INVALID_PORT

  Invalid/unknown NVLink port number.

CUPTI_SOURCE_LOCATOR_ID_UNKNOWN

  The source-locator ID that indicates an unknown source location.

  There is not an actual CUpti_ActivitySourceLocator object corresponding to this value.

CUPTI_SYNCHRONIZATION_INVALID_VALUE

  An invalid/unknown value.

CUPTI_TIMESTAMP_UNKNOWN

  An invalid/unknown timestamp for a start, end, queued, submitted, or completed time.

CUpti_ActivityConfig_STRUCT_SIZE

## 6.1.7. Enumerations

enum CUpti_ActivityApiFieldIds

  Enum identifiers for fields in CUpti_ActivityAPI.

  Each enum value corresponds to a field in CUpti_ActivityAPI and describes the data type and purpose of that field.

  Values:

  enumerator API_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always either CUPTI_ACTIVITY_KIND_DRIVER or CUPTI_ACTIVITY_KIND_RUNTIME.

  enumerator API_FIELD_CBID

    CUpti_CallbackId cbid; Callback ID of the CUDA driver/runtime API function.

  enumerator API_FIELD_START

    uint64_t start; Start timestamp of the CUDA driver/runtime API call (in nanoseconds).

  enumerator API_FIELD_END

    uint64_t end; End timestamp of the CUDA driver/runtime API call (in nanoseconds).

  enumerator API_FIELD_PROCESS_ID

    uint32_t processId; ID of the process executing the CUDA driver/runtime API call.

  enumerator API_FIELD_THREAD_ID

    uint64_t threadId; ID of the thread executing the CUDA driver/runtime API call.

  enumerator API_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this CUDA driver/runtime API invocation.

    This ID matches the correlation ID of the associated kernel, memcpy, or memset activity record that the API call initiated.

  enumerator API_FIELD_RETURN_VALUE

    uint32_t returnValue; Return value of the CUDA driver/runtime API call (CUresult or cudaError_t).

  enumerator API_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityAttribute

  Activity attributes.

  These attributes are used to control the behavior of the activity API.

  Values:

  enumerator CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE

    The device memory size (in bytes) reserved for storing profiling data for concurrent kernels (activity kind CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL), memcopies and memsets for each buffer on a context.

    The value is a size_t.

    There is a limit on how many device buffers can be allocated per context. User can query and set this limit using the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT. CUPTI doesn’t pre-allocate all the buffers, it pre-allocates only those many buffers as set by the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE. When all of the data in a buffer is consumed, it is added in the reuse pool, and CUPTI picks a buffer from this pool when a new buffer is needed. Thus memory footprint does not scale with the kernel count. Applications with the high density of kernels, memcopies and memsets might result in having CUPTI to allocate more device buffers. CUPTI allocates another buffer only when it runs out of the buffers in the reuse pool.

    Since buffer allocation happens in the main application thread, this might result in stalls in the critical path. CUPTI pre-allocates 3 buffers of the same size to mitigate this issue. User can query and set the pre-allocation limit using the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE.

    Having larger buffer size leaves less device memory for the application. Having smaller buffer size increases the risk of dropping timestamps for records if too many kernels or memcopies or memsets are launched at one time.

    This value only applies to new buffer allocations. Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.

    The default value is 3200000 (~3MB) which can accommodate profiling data up to 100,000 kernels, memcopies and memsets combined.

    Note: Starting with the CUDA 12.0 Update 1 release, CUPTI allocates the profiling buffer in the device memory by default, which may improve the performance of the tracing run. To change the preferred location to page-locked host memory, refer to the attribute CUPTI_ACTIVITY_ATTR_MEM_ALLOCATION_TYPE_HOST_PINNED. The size of the memory and maximum number of pools are still controlled by the attributes CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE and CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT.

    Note: The actual amount of device memory per buffer reserved by CUPTI might be larger.

  enumerator CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE_CDP

    The device memory size (in bytes) reserved for storing profiling data for CDP operations for each buffer on a context.

    The value is a size_t.

    Having larger buffer size means less flush operations but consumes more device memory. This value only applies to new allocations.

    Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.

    The default value is 8388608 (8MB).

    Note: The actual amount of device memory per context reserved by CUPTI might be larger.

  enumerator CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT

    The maximum number of device memory buffers per context.

    The value is a size_t.

    For an application with high rate of kernel launches, memcopies and memsets having a bigger pool limit helps in timestamp collection for all these activities at the expense of a larger memory footprint. Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE for more details.

    Setting this value will not modify the number of memory buffers currently stored.

    Set this value before initializing CUDA to ensure the limit is not exceeded.

    The default value is 250.

  enumerator CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_SIZE

    This attribute is not supported starting with CUDA 12.3 CUPTI no longer uses profiling semaphore pool to store profiling data.

    There is a limit on how many semaphore pools can be allocated per context. User can query and set this limit using the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_LIMIT. CUPTI doesn’t pre-allocate all the semaphore pools, it pre-allocates only those many semaphore pools as set by the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_PRE_ALLOCATE_VALUE. When all of the data in a semaphore pool is consumed, it is added in the reuse pool, and CUPTI picks a semaphore pool from the reuse pool when a new semaphore pool is needed. Thus memory footprint does not scale with the kernel count. Applications with the high density of kernels might result in having CUPTI to allocate more semaphore pools. CUPTI allocates another semaphore pool only when it runs out of the semaphore pools in the reuse pool.

    Since semaphore pool allocation happens in the main application thread, this might result in stalls in the critical path. CUPTI pre-allocates 3 semaphore pools of the same size to mitigate this issue. User can query and set the pre-allocation limit using the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_PRE_ALLOCATE_VALUE.

    Having larger semaphore pool size leaves less device memory for the application. Having smaller semaphore pool size increases the risk of dropping timestamps for kernel records if too many kernels are issued/launched at one time.

    This value only applies to new semaphore pool allocations. Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.

    The default value is 25000 which can accommodate profiling data for upto 25,000 kernels.

  enumerator CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_LIMIT

    This attribute is not supported starting with CUDA 12.3 CUPTI no longer uses profiling semaphore pool to store profiling data.

    The maximum number of profiling semaphore pools per context. The value is a size_t.

    Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_SIZE for more details.

    Set this value before initializing CUDA to ensure the limit is not exceeded.

    The default value is 250.

  enumerator CUPTI_ACTIVITY_ATTR_ZEROED_OUT_ACTIVITY_BUFFER

    The flag to indicate whether user should provide activity buffer of zero value.

    The value is a uint8_t.

    If the value of this attribute is non-zero, user should provide a zero value buffer in the CUpti_BuffersCallbackRequestFunc. If the user does not provide a zero value buffer after setting this to non-zero, the activity buffer may contain some uninitialized values when CUPTI returns it in CUpti_BuffersCallbackCompleteFunc

    If the value of this attribute is zero, CUPTI will initialize the user buffer received in the CUpti_BuffersCallbackRequestFunc to zero before filling it. If the user sets this to zero, a few stalls may appear in critical path because CUPTI will zero out the buffer in the main thread. Set this value before returning from CUpti_BuffersCallbackRequestFunc to ensure it is considered for all the subsequent user buffers.

    The default value is 0.

  enumerator CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE

    Number of device buffers to pre-allocate for a context during the initialization phase.

    The value is a size_t.

    Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE for details.

    This value must be less than the maximum number of device buffers set using the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT

    Set this value before initializing CUDA or before creating a context to ensure it is considered by the CUPTI.

    The default value is set to 3 to ping pong between these buffers (if possible).

  enumerator CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_PRE_ALLOCATE_VALUE

    This attribute is not supported starting with CUDA 12.3 CUPTI no longer uses profiling semaphore pool to store profiling data.

    Number of profiling semaphore pools to pre-allocate for a context during the initialization phase. The value is a size_t.

    Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_SIZE for details.

    This value must be less than the maximum number of profiling semaphore pools set using the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_LIMIT

    Set this value before initializing CUDA or before creating a context to ensure it is considered by the CUPTI.

    The default value is set to 3 to ping pong between these pools (if possible).

  enumerator CUPTI_ACTIVITY_ATTR_MEM_ALLOCATION_TYPE_HOST_PINNED

    Allocate page-locked (pinned) host memory for storing profiling data for concurrent kernels, memcopies and memsets for each buffer on a context.

    The value is a uint8_t.

    From CUDA 11.2 through CUDA 12.0 GA releases, CUPTI allocated the profiling buffer in pinned host memory by default. Allocating excessive amounts of pinned memory may degrade system performance, as it reduces the amount of memory available to the system for paging. For this reason user might want to change the location from pinned host memory to device memory by setting value of this attribute to 0.

    Using page-locked (pinned) host memory buffers is not supported on confidential computing devices. If this attribute is set to 1, CUPTI will return error CUPTI_ERROR_NOT_SUPPORTED.

    The default value is 0.

  enumerator CUPTI_ACTIVITY_ATTR_PER_THREAD_ACTIVITY_BUFFER

    Request activity buffers per-thread to store CUPTI activity records in the activity buffer on per-thread basis.

    The value is a uint8_t.

    The attribute should be set before registering the buffer callbacks using cuptiActivityRegisterCallbacks API and before any of the CUPTI activity kinds are enabled. This makes sure that all the records are stored in activity buffers allocated per-thread. Changing this attribute in the middle of the profiling session will result in undefined behavior.

    The default value is 1.

  enumerator CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE_DEVICE_GRAPHS

    The device memory size (in bytes) reserved for storing profiling data for device graph operations for each buffer on a context.

    The value is a size_t.

    Having larger buffer size means less flush operations but consumes more device memory. This value only applies to new allocations.

    Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.

    The default value is 16777216 (16MB).

    Note: The actual amount of device memory per context reserved by CUPTI might be larger.

  enumerator CUPTI_ACTIVITY_ATTR_USER_DEFINED_RECORDS

    Enable user-defined activity records.

    The value is a uint8_t.

    When this attribute is enabled, CUPTI activity records will contain only the fields that are enabled for collection by the user. This can help to reduce the size of each activity record and decrease the overall memory consumption for activity collection.

    This attribute must be set before enabling any CUPTI activity kinds. The activity kinds should be enabled/disabled using CUPTI API cuptiActivityEnable_v2 and cuptiActivityDisable_v2 respectively.

    Minimum CUPTI Version: CUPTI_API_VERSION 130200 (CUDA 13.2). The CUPTI version can be queried using cuptiGetVersion() API.

    Refer these links for online documentation: CUPTI Activity User-Defined Records: https://docs.nvidia.com/cupti/main/main.html#cupti-user-defined-activity-records Tutorial: https://docs.nvidia.com/cupti/tutorial/tutorial.html#tutorial-activity-user-defined-records Refer sample cupti_user_defined_records for usage.

    The default value is 0 i.e. CUPTI will provide records with all fields.

  enumerator CUPTI_ACTIVITY_ATTR_MULTIPLE_SUBSCRIBER_STATE

    Allow multiple subscribers.

    The value is a uint8_t.

    If 0, only a single subscriber is allowed. If 1, multiple subscribers are allowed. If 2, this option has not been set by a prior subscriber, if there were any. In this case, the subscriber is free to set it during cuptiSubscribe_v2 call. Note that this attribute cannot be set by cuptiActivitySetAttribute or cuptiActivitySetAttribute_v2. It can however be queried using cuptiActivityGetAttribute_v2.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_HES

    Get the HES (Hardware Events System) enabled flag.

    The value is a uint8_t.

    If 0, HES (Hardware Events System) is disabled. If 1, HES (Hardware Events System) is enabled. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2. This attribute is not subscriber specific, and the subscriber parameter is ignored. All subscribers will share the same HES enabled flag. However, this attribute must be set before enabling any activity kind by any subscriber. However, it can be queried using cuptiActivityGetAttribute_v2.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_ALLOCATION_SOURCE_TRACKING

    Get the allocation source library tracking enabled flag (for the specified subscriber).

    The value is a uint8_t.

    If 0, allocation source library tracking is disabled. If 1, allocation source library tracking is enabled. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber. Note that the cuptiActivityEnableAllocationSource API cannot be used when multiple subscribers are allowed.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_KERNEL_LATENCY_TIMESTAMPS

    Get the latency timestamp tracking enabled flag (for the specified subscriber).

    The value is a uint8_t.

    This can be used to toggle collecting latency timestamps for kernel records.

    If 0, latency timestamp tracking is disabled. If 1, latency timestamp tracking is enabled. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_ALL_SYNC_RECORDS

    Get the all sync records enabled flag (for the specified subscriber).

    The value is a uint8_t.

    This can be used to toggle collecting sync records for all synchronization operations (whether to include records for synchronization operations which return non-zero CUDA status). By default, this flag is set to 0. If this flag is set to 1, sync records are collected for all synchronization operations (even if they return non-zero CUDA status). Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_CUDA_EVENT_DEVICE_TIMESTAMPS

    Get the event device timestamps enabled flag (for the specified subscriber).

    The value is a uint8_t.

    This can be used to toggle collecting event device timestamps for CUDA event records. By default, this flag is set to 0. If this flag is set to 1, event device timestamps are collected for CUDA event records. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_KERNEL_LAUNCH_ATTRIBUTES

    Get the launch attributes for kernel enabled flag (for the specified subscriber).

    The value is a uint8_t.

    This can be used to toggle collecting launch attributes for kernel records. By default, this flag is set to 0. If this flag is set to 1, launch attributes are collected for kernel records. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_DEVICE_GRAPH_TRACE

    Get the device graph trace enabled flag (for the specified subscriber).

    The value is a uint8_t.

    This can be used to toggle collecting device graph trace for graph records. By default, this flag is set to 0. If this flag is set to 1, device graph trace is collected for graph records. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_MULTI_SUBSCRIBER_GRAPH_TRACE

    Get the multi-subscriber graph level trace enabled flag.

    The value is a uint8_t.

    This attribute is only relevant for multi-subscriber mode. CUPTI currently does not support different subscribers to ask for node level trace and graph level trace concurrently. If this flag is disabled, body nodes of a graph are reported under normal concurrent kernel/ memcpy/ memset records. If this flag is enabled, body nodes of a graph are not reported under normal concurrent kernel/ memcpy/ memset records, but the graph is entirely reported as part of a single graph trace record(if CUPTI_ACTIVITY_KIND_GRAPH_TRACE is enabled for the subscriber). Note that this behavior is consistent across all subscribers, regardless of which activities each subscriber is enabling.

    If 0, multi-subscriber graph level trace is disabled. If 1, multi-subscriber graph level trace is enabled. The default value is 0. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber. However, this attribute must be set before enabling any activity kind by any subscriber. This attribute is not subscriber specific, and the subscriber parameter is ignored. All subscribers will share the same multi-subscriber graph level trace enabled flag.

  enumerator CUPTI_ACTIVITY_ATTR_THREAD_ID_TYPE

    Get or set the thread ID type (for the specified subscriber).

    The value is a CUpti_ActivityThreadIdType.

    This attribute specifies the method used by CUPTI to obtain thread IDs. The default value is CUPTI_ACTIVITY_THREAD_ID_TYPE_DEFAULT. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

  enumerator CUPTI_ACTIVITY_ATTR_TIMESTAMP_CALLBACK

    Get or set the timestamp callback function (for the specified subscriber).

    The value is a CUpti_TimestampCallbackFunc.

    This attribute allows registering a custom timestamp callback function that CUPTI will use instead of its default CPU timer. The value can be NULL to unregister the callback. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2 for the specified subscriber.

    Note

    This attribute is currently in beta. Current behavior is that this cannot be used when multiple subscribers are allowed. Behavior may change in future releases.

  enumerator CUPTI_ACTIVITY_ATTR_ENABLE_CIG_MODE

    Get or set the CIG (CUDA in Graphics) mode.

    The value is a uint8_t.

    This attribute allows enabling or disabling the CIG mode. Note that this attribute can be set by cuptiActivitySetAttribute_v2 and queried using cuptiActivityGetAttribute_v2.

  enumerator CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_FORCE_INT

enum CUpti_ActivityComputeApiKind

  The kind of a compute API.

  Values:

  enumerator CUPTI_ACTIVITY_COMPUTE_API_UNKNOWN

    The compute API is not known.

  enumerator CUPTI_ACTIVITY_COMPUTE_API_CUDA

    The compute APIs are for CUDA.

  enumerator CUPTI_ACTIVITY_COMPUTE_API_CUDA_MPS

    The compute APIs are for CUDA running in MPS (Multi-Process Service) environment.

  enumerator CUPTI_ACTIVITY_COMPUTE_API_FORCE_INT

enum CUpti_ActivityComputeEngineCtxSwitchFieldIds

  Enum identifiers for fields in CUpti_ActivityComputeEngineCtxSwitch.

  Each enum value corresponds to a field in CUpti_ActivityComputeEngineCtxSwitch and describes the data type and purpose of that field.

  Values:

  enumerator COMPUTE_ENGINE_CTX_SWITCH_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_COMPUTE_ENGINE_CTX_SWITCH.

  enumerator COMPUTE_ENGINE_CTX_SWITCH_FIELD_CONTEXT_ID

    uint32_t contextId; ID of the CUDA context.

  enumerator COMPUTE_ENGINE_CTX_SWITCH_FIELD_TIMESTAMP

    uint64_t timestamp; Timestamp at which the context switch operation occurs.

  enumerator COMPUTE_ENGINE_CTX_SWITCH_FIELD_OPERATION_TYPE

    CUpti_ComputeEngineCtxSwitchOperationType operationType; Type of the Compute Engine Context switch operation.

  enumerator COMPUTE_ENGINE_CTX_SWITCH_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityConfidentialComputeRotationFieldIds

  Enum identifiers for fields in CUpti_ActivityConfidentialComputeRotation.

  Each enum value corresponds to a field in CUpti_ActivityConfidentialComputeRotation and describes the data type and purpose of that field.

  Values:

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_CONFIDENTIAL_COMPUTE_ROTATION.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_EVENT_TYPE

    CUpti_ConfidentialComputeRotationEventType eventType; Type of event.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_DEVICE_ID

    uint32_t deviceId; Device ID.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_CONTEXT_ID

    uint32_t contextId; Context ID.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_CHANNEL_ID

    uint32_t channelId; Channel ID.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_CHANNEL_TYPE

    CUpti_ChannelType channelType; Channel Type.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_TIMESTAMP

    uint64_t timestamp; Timestamp in ns.

  enumerator CONFIDENTIAL_COMPUTE_ROTATION_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityContextFieldIds

  Enum identifiers for fields to trace context.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_CONTEXT.

  Values:

  enumerator CONTEXT_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_CONTEXT.

  enumerator CONTEXT_FIELD_CONTEXT_ID

    uint32_t contextId; The ID of the context.

  enumerator CONTEXT_FIELD_DEVICE_ID

    uint32_t deviceId; The ID of the device associated with the context.

  enumerator CONTEXT_FIELD_COMPUTE_API_KIND

    uint16_t computeApiKind; The compute API kind associated with the context.

    CUpti_ActivityComputeApiKind

  enumerator CONTEXT_FIELD_NULL_STREAM_ID

    uint32_t nullStreamId; The ID for the NULL stream in this context.

  enumerator CONTEXT_FIELD_PARENT_CONTEXT_ID

    uint32_t parentContextId; The ID of the parent context.

    It would be 0 if context does not have parent.

  enumerator CONTEXT_FIELD_IS_GREEN_CONTEXT

    uint8_t isGreenContext; Indicates whether the context is a green context.

  enumerator CONTEXT_FIELD_NUM_MULTIPROCESSORS

    uint16_t numMultiprocessors; Number of multiprocessors assigned to the green context.

    Invalid if the field ‘isGreenContext’ is 0.

  enumerator CONTEXT_FIELD_CIG_MODE

    CUpti_ContextCigMode cigMode; The CIG mode of the context.

  enumerator CONTEXT_FIELD_PROCESS_ID

    uint32_t processId; The ID of the process associated with the context.

  enumerator CONTEXT_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityCudaEventFieldIds

  Enum identifiers for fields to trace CUDA Event operations.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_CUDA_EVENT.

  Values:

  enumerator CUDA_EVENT_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_CONTEXT.

  enumerator CUDA_EVENT_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this CUDA Event operation.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator CUDA_EVENT_FIELD_CONTEXT_ID

    uint32_t contextId; The ID of the context where the event was recorded.

  enumerator CUDA_EVENT_FIELD_STREAM_ID

    uint32_t streamId; The compute stream where the event was recorded.

  enumerator CUDA_EVENT_FIELD_EVENT_ID

    uint64_t eventId; A unique event ID to identify the event record.

  enumerator CUDA_EVENT_FIELD_DEVICE_ID

    uint32_t deviceId; The ID of the device where the event was recorded.

  enumerator CUDA_EVENT_FIELD_DEVICE_TIMESTAMP

    uint64_t deviceTimestamp; The device-side timestamp on CUDA event record (in nanoseconds).

    Collection of this field is disabled by default. It can be enabled by calling CUPTI API cuptiActivityEnableCudaEventDeviceTimestamps

  enumerator CUDA_EVENT_FIELD_CUDA_EVENT_SYNC_ID

    uint64_t cudaEventSyncId; A unique ID to associate event synchronization records with the latest CUDA Event record.

    Similar field is added in CUpti_ActivitySynchronization2 to associate CUDA Event record to the synchronization record.

    The same CUDA event can be used multiple times, so the event id will not be unique to correlate the synchronization record with the latest CUDA Event record. This field will be unique and can be used to do the required correlation.

  enumerator CUDA_EVENT_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityDeviceFieldIds

  Enum identifiers for fields in CUpti_ActivityDevice6.

  Each enum value corresponds to a field in CUpti_ActivityDevice6 and describes the data type and purpose of that field.

  Values:

  enumerator DEVICE_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_DEVICE.

  enumerator DEVICE_FIELD_FLAGS

    CUpti_ActivityFlag flags; Flags associated with the device.

  enumerator DEVICE_FIELD_GLOBAL_MEMORY_BANDWIDTH

    uint64_t globalMemoryBandwidth; Global memory bandwidth available on the device (in kBytes/sec).

  enumerator DEVICE_FIELD_GLOBAL_MEMORY_SIZE

    uint64_t globalMemorySize; Amount of global memory on the device (in bytes).

  enumerator DEVICE_FIELD_CONSTANT_MEMORY_SIZE

    uint32_t constantMemorySize; Amount of constant memory on the device (in bytes).

  enumerator DEVICE_FIELD_L2_CACHE_SIZE

    uint32_t l2CacheSize; Size of the L2 cache on the device (in bytes).

  enumerator DEVICE_FIELD_NUM_THREADS_PER_WARP

    uint32_t numThreadsPerWarp; Number of threads per warp on the device.

  enumerator DEVICE_FIELD_CORE_CLOCK_RATE

    uint32_t coreClockRate; Core clock rate of the device (in kHz).

  enumerator DEVICE_FIELD_NUM_MEMCPY_ENGINES

    uint32_t numMemcpyEngines; Number of memory copy engines on the device.

  enumerator DEVICE_FIELD_NUM_MULTIPROCESSORS

    uint32_t numMultiprocessors; Number of multiprocessors on the device.

  enumerator DEVICE_FIELD_MAX_IPC

    uint32_t maxIPC; Maximum instructions per cycle possible on each device multiprocessor.

  enumerator DEVICE_FIELD_MAX_WARPS_PER_MULTIPROCESSOR

    uint32_t maxWarpsPerMultiprocessor; Maximum number of warps that can be present on a multiprocessor.

  enumerator DEVICE_FIELD_MAX_BLOCKS_PER_MULTIPROCESSOR

    uint32_t maxBlocksPerMultiprocessor; Maximum number of blocks that can be present on a multiprocessor.

  enumerator DEVICE_FIELD_MAX_SHARED_MEMORY_PER_MULTIPROCESSOR

    uint32_t maxSharedMemoryPerMultiprocessor; Maximum amount of shared memory available per multiprocessor (in bytes).

  enumerator DEVICE_FIELD_MAX_REGISTERS_PER_MULTIPROCESSOR

    uint32_t maxRegistersPerMultiprocessor; Maximum number of 32-bit registers available per multiprocessor.

  enumerator DEVICE_FIELD_MAX_REGISTERS_PER_BLOCK

    uint32_t maxRegistersPerBlock; Maximum number of registers that can be allocated to a block.

  enumerator DEVICE_FIELD_MAX_SHARED_MEMORY_PER_BLOCK

    uint32_t maxSharedMemoryPerBlock; Maximum amount of shared memory that can be assigned to a block (in bytes).

  enumerator DEVICE_FIELD_MAX_THREADS_PER_BLOCK

    uint32_t maxThreadsPerBlock; Maximum number of threads allowed in a block.

  enumerator DEVICE_FIELD_MAX_BLOCK_DIM_X

    uint32_t maxBlockDimX; Maximum allowed X dimension for a block.

  enumerator DEVICE_FIELD_MAX_BLOCK_DIM_Y

    uint32_t maxBlockDimY; Maximum allowed Y dimension for a block.

  enumerator DEVICE_FIELD_MAX_BLOCK_DIM_Z

    uint32_t maxBlockDimZ; Maximum allowed Z dimension for a block.

  enumerator DEVICE_FIELD_MAX_GRID_DIM_X

    uint32_t maxGridDimX; Maximum allowed X dimension for a grid.

  enumerator DEVICE_FIELD_MAX_GRID_DIM_Y

    uint32_t maxGridDimY; Maximum allowed Y dimension for a grid.

  enumerator DEVICE_FIELD_MAX_GRID_DIM_Z

    uint32_t maxGridDimZ; Maximum allowed Z dimension for a grid.

  enumerator DEVICE_FIELD_COMPUTE_CAPABILITY_MAJOR

    uint32_t computeCapabilityMajor; Compute capability for the device (major number).

  enumerator DEVICE_FIELD_COMPUTE_CAPABILITY_MINOR

    uint32_t computeCapabilityMinor; Compute capability for the device (minor number).

  enumerator DEVICE_FIELD_ID

    uint32_t id; Device ID.

  enumerator DEVICE_FIELD_ECC_ENABLED

    uint32_t eccEnabled; ECC enabled flag for device.

  enumerator DEVICE_FIELD_UUID

    CUuuid uuid; Device UUID.

  enumerator DEVICE_FIELD_NAME

    const char *name; Device name.

  enumerator DEVICE_FIELD_IS_CUDA_VISIBLE

    uint8_t isCudaVisible; Flag to indicate whether the device is visible to CUDA.

  enumerator DEVICE_FIELD_IS_MIG_ENABLED

    uint8_t isMigEnabled; MIG enabled flag for device.

  enumerator DEVICE_FIELD_GPU_INSTANCE_ID

    uint32_t gpuInstanceId; GPU instance ID for MIG enabled devices.

  enumerator DEVICE_FIELD_COMPUTE_INSTANCE_ID

    uint32_t computeInstanceId; Compute instance ID for MIG enabled devices.

  enumerator DEVICE_FIELD_MIG_UUID

    CUuuid migUuid; MIG UUID.

  enumerator DEVICE_FIELD_IS_NUMA_NODE

    uint32_t isNumaNode; NUMA node flag for device.

  enumerator DEVICE_FIELD_NUMA_ID

    uint32_t numaId; NUMA node ID of the GPU memory.

  enumerator DEVICE_FIELD_NUM_TPCS

    uint32_t numTpcs; Number of TPCs on the device.

  enumerator DEVICE_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityDeviceGraphTraceFieldIds

  Enum identifiers for fields in CUpti_ActivityDeviceGraphTrace.

  Each enum value corresponds to a field in CUpti_ActivityDeviceGraphTrace and describes the data type and purpose of that field.

  Values:

  enumerator DEVICE_GRAPH_TRACE_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_DEVICE_GRAPH_TRACE.

  enumerator DEVICE_GRAPH_TRACE_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the device where the first node of the graph is executed.

  enumerator DEVICE_GRAPH_TRACE_FIELD_START

    uint64_t start; Start timestamp for the graph execution (in ns).

  enumerator DEVICE_GRAPH_TRACE_FIELD_END

    uint64_t end; End timestamp for the graph execution (in ns).

  enumerator DEVICE_GRAPH_TRACE_FIELD_GRAPH_ID

    uint32_t graphId; Unique ID of the graph that is launched.

  enumerator DEVICE_GRAPH_TRACE_FIELD_LAUNCHER_GRAPH_ID

    uint32_t launcherGraphId; Unique ID of the graph that has launched this graph.

  enumerator DEVICE_GRAPH_TRACE_FIELD_DEVICE_LAUNCH_MODE

    uint32_t deviceLaunchMode; Type of launch.

  enumerator DEVICE_GRAPH_TRACE_FIELD_CONTEXT_ID

    uint64_t contextId; ID of the context where the first node of the graph is executed.

  enumerator DEVICE_GRAPH_TRACE_FIELD_STREAM_ID

    uint64_t streamId; ID of the stream where the graph is being launched.

    This is the only record that has 64-bit streamId to accommodate device-side created streams.

  enumerator DEVICE_GRAPH_TRACE_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityEnvironmentFieldIds

  Enum identifiers for fields in CUpti_ActivityEnvironment.

  Each enum value corresponds to a field in CUpti_ActivityEnvironment and describes the data type and purpose of that field.

  Values:

  enumerator ENVIRONMENT_FIELD_KIND

    CUpti_ActivityKind kind; Kind of activity record: CUPTI_ACTIVITY_KIND_ENVIRONMENT.

  enumerator ENVIRONMENT_FIELD_DEVICE_ID

    uint32_t deviceId; The ID of the device

  enumerator ENVIRONMENT_FIELD_TIMESTAMP

    uint64_t timestamp; The timestamp when this sample was retrieved, in ns.

    A value of 0 indicates that timestamp information could not be collected for the marker.

  enumerator ENVIRONMENT_FIELD_ENVIRONMENT_KIND

    CUpti_ActivityEnvironmentKind environmentKind; The kind of data reported in this record.

  enumerator ENVIRONMENT_FIELD_ENVIRONMENT_KIND_DATA

    union data; Depending on the value of environmentKind, this field contains additional information about the environment.

    CUpti_ActivityEnvironmentSpeed speed if environmentKind is CUPTI_ACTIVITY_ENVIRONMENT_SPEED CUpti_ActivityEnvironmentTemperature temperature if environmentKind is CUPTI_ACTIVITY_ENVIRONMENT_TEMPERATURE CUpti_ActivityEnvironmentPower power if environmentKind is CUPTI_ACTIVITY_ENVIRONMENT_POWER CUpti_ActivityEnvironmentCooling cooling if environmentKind is CUPTI_ACTIVITY_ENVIRONMENT_COOLING The size of this field is determined by the largest structure among the possible types it can hold.

  enumerator ENVIRONMENT_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityEnvironmentKind

  The kind of environment data.

  Used to indicate what type of data is being reported by an environment activity record.

  Values:

  enumerator CUPTI_ACTIVITY_ENVIRONMENT_UNKNOWN

    Unknown data.

  enumerator CUPTI_ACTIVITY_ENVIRONMENT_SPEED

    The environment data is related to speed.

  enumerator CUPTI_ACTIVITY_ENVIRONMENT_TEMPERATURE

    The environment data is related to temperature.

  enumerator CUPTI_ACTIVITY_ENVIRONMENT_POWER

    The environment data is related to power.

  enumerator CUPTI_ACTIVITY_ENVIRONMENT_COOLING

    The environment data is related to cooling.

  enumerator CUPTI_ACTIVITY_ENVIRONMENT_COUNT
  enumerator CUPTI_ACTIVITY_ENVIRONMENT_KIND_FORCE_INT

enum CUpti_ActivityExternalCorrelationFieldIds

  Enum identifiers for fields in CUpti_ActivityExternalCorrelation.

  This activity record correlates native CUDA records (e.g. CUDA Driver API, kernels, memcpys, …) with records from external APIs such as OpenACC. (CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION).

  Values:

  enumerator EXTERNAL_CORRELATION_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION.

  enumerator EXTERNAL_CORRELATION_FIELD_EXTERNAL_KIND

    CUpti_ExternalCorrelationKind externalKind; Kind of external API this record correlated to.

  enumerator EXTERNAL_CORRELATION_FIELD_EXTERNAL_ID

    uint64_t externalId; Correlation ID of the associated non-CUDA API record.

  enumerator EXTERNAL_CORRELATION_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID of the associated CUDA driver or runtime API record.

  enumerator EXTERNAL_CORRELATION_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityFlag

  Flags associated with activity records.

  Activity record flags. Flags can be combined by bitwise OR to associated multiple flags with an activity record. Each flag is specific to a certain activity kind, as noted below.

  Values:

  enumerator CUPTI_ACTIVITY_FLAG_NONE

    Indicates the activity record has no flags.

  enumerator CUPTI_ACTIVITY_FLAG_DEVICE_CONCURRENT_KERNELS

    Indicates the activity represents a device that supports concurrent kernel execution.

    Valid for CUPTI_ACTIVITY_KIND_DEVICE.

  enumerator CUPTI_ACTIVITY_FLAG_DEVICE_ATTRIBUTE_CUDEVICE

    Indicates if the activity represents a CUdevice_attribute value or a CUpti_DeviceAttribute value.

    Valid for CUPTI_ACTIVITY_KIND_DEVICE_ATTRIBUTE.

  enumerator CUPTI_ACTIVITY_FLAG_MEMCPY_ASYNC

    Indicates the activity represents an asynchronous memcpy operation.

    Valid for CUPTI_ACTIVITY_KIND_MEMCPY.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_INSTANTANEOUS

    Indicates the activity represents an instantaneous marker.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_START

    Indicates the activity represents a region start marker.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_END

    Indicates the activity represents a region end marker.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_SYNC_ACQUIRE

    Indicates the activity represents an attempt to acquire a user defined synchronization object.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_SYNC_ACQUIRE_SUCCESS

    Indicates the activity represents success in acquiring the user defined synchronization object.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_SYNC_ACQUIRE_FAILED

    Indicates the activity represents failure in acquiring the user defined synchronization object.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_SYNC_RELEASE

    Indicates the activity represents releasing a reservation on user defined synchronization object.

    Valid for CUPTI_ACTIVITY_KIND_MARKER.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_COLOR_NONE

    Indicates the activity represents a marker that does not specify a color.

    Valid for CUPTI_ACTIVITY_KIND_MARKER_DATA.

  enumerator CUPTI_ACTIVITY_FLAG_MARKER_COLOR_ARGB

    Indicates the activity represents a marker that specifies a color in alpha-red-green-blue format.

    Valid for CUPTI_ACTIVITY_KIND_MARKER_DATA.

  enumerator CUPTI_ACTIVITY_FLAG_GLOBAL_ACCESS_KIND_SIZE_MASK

    The number of bytes requested by each thread Valid for CUpti_ActivityGlobalAccess3.

  enumerator CUPTI_ACTIVITY_FLAG_GLOBAL_ACCESS_KIND_LOAD

    If bit in this flag is set, the access was load, else it is a store access.

    Valid for CUpti_ActivityGlobalAccess3.

  enumerator CUPTI_ACTIVITY_FLAG_GLOBAL_ACCESS_KIND_CACHED

    If this bit in flag is set, the load access was cached else it is uncached.

    Valid for CUpti_ActivityGlobalAccess3.

  enumerator CUPTI_ACTIVITY_FLAG_METRIC_OVERFLOWED

    If this bit in flag is set, the metric value overflowed.

    Valid for CUpti_ActivityMetric and CUpti_ActivityMetricInstance.

  enumerator CUPTI_ACTIVITY_FLAG_METRIC_VALUE_INVALID

    If this bit in flag is set, the metric value couldn’t be calculated.

    This occurs when a value(s) required to calculate the metric is missing. Valid for CUpti_ActivityMetric and CUpti_ActivityMetricInstance.

  enumerator CUPTI_ACTIVITY_FLAG_INSTRUCTION_VALUE_INVALID

    If this bit in flag is set, the source level metric value couldn’t be calculated.

    This occurs when a value(s) required to calculate the source level metric cannot be evaluated. Valid for CUpti_ActivityInstructionExecution.

  enumerator CUPTI_ACTIVITY_FLAG_INSTRUCTION_CLASS_MASK

    The mask for the instruction class, CUpti_ActivityInstructionClass Valid for CUpti_ActivityInstructionExecution and CUpti_ActivityInstructionCorrelation.

  enumerator CUPTI_ACTIVITY_FLAG_FLUSH_FORCED

    When calling cuptiActivityFlushAll, this flag can be set to force CUPTI to flush all records in the buffer, whether finished or not.

  enumerator CUPTI_ACTIVITY_FLAG_SHARED_ACCESS_KIND_SIZE_MASK

    The number of bytes requested by each thread Valid for CUpti_ActivitySharedAccess.

  enumerator CUPTI_ACTIVITY_FLAG_SHARED_ACCESS_KIND_LOAD

    If bit in this flag is set, the access was load, else it is a store access.

    Valid for CUpti_ActivitySharedAccess.

  enumerator CUPTI_ACTIVITY_FLAG_MEMSET_ASYNC

    Indicates the activity represents an asynchronous memset operation.

    Valid for CUPTI_ACTIVITY_KIND_MEMSET.

  enumerator CUPTI_ACTIVITY_FLAG_THRASHING_IN_CPU

    Indicates the activity represents thrashing in CPU.

    Valid for counter of kind CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THRASHING in CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER

  enumerator CUPTI_ACTIVITY_FLAG_THROTTLING_IN_CPU

    Indicates the activity represents page throttling in CPU.

    Valid for counter of kind CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THROTTLING in CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER

  enumerator CUPTI_ACTIVITY_FLAG_FORCE_INT

enum CUpti_ActivityGraphHostNodeFieldIds

  Enum identifiers for fields in CUpti_ActivityGraphHostNode.

  Each enum value corresponds to a field in CUpti_ActivityGraphHostNode and describes the data type and purpose of that field.

  Values:

  enumerator GRAPH_HOST_NODE_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_GRAPH_HOST_NODE.

  enumerator GRAPH_HOST_NODE_FIELD_STREAM_ID

    uint32_t streamId; ID of the stream that waits for the graph host node to finish.

  enumerator GRAPH_HOST_NODE_FIELD_CONTEXT_ID

    uint32_t contextId; ID of the CUDA context to which the waiting CUDA stream belongs.

  enumerator GRAPH_HOST_NODE_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the CUDA device to which the CUDA context and stream belong.

  enumerator GRAPH_HOST_NODE_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID of the graph host node operation.

  enumerator GRAPH_HOST_NODE_FIELD_GRAPH_ID

    uint32_t graphId; Unique ID of the graph that executed this host node through graph launch.

  enumerator GRAPH_HOST_NODE_FIELD_GRAPH_NODE_ID

    uint64_t graphNodeId; Unique ID of the graph node that executed this host node through graph launch.

  enumerator GRAPH_HOST_NODE_FIELD_PROCESS_ID

    uint32_t processId; ID of the process where the host node is executing.

  enumerator GRAPH_HOST_NODE_FIELD_THREAD_ID

    uint64_t threadId; ID of the thread where the host node is executing.

  enumerator GRAPH_HOST_NODE_FIELD_START

    uint64_t start; Start timestamp.

  enumerator GRAPH_HOST_NODE_FIELD_END

    uint64_t end; End timestamp.

  enumerator GRAPH_HOST_NODE_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityGraphTraceFieldIds

  Enum identifiers for fields to trace graph execution.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_GRAPH_TRACE.

  Values:

  enumerator GRAPH_TRACE_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_GRAPH_TRACE.

  enumerator GRAPH_TRACE_FIELD_CORRELATION_ID

    uint64_t correlationId; The correlation ID of the graph launch.

  enumerator GRAPH_TRACE_FIELD_START

    uint64_t start; The start timestamp for the graph execution, in ns.

  enumerator GRAPH_TRACE_FIELD_END

    uint64_t end; The end timestamp for the graph execution, in ns.

  enumerator GRAPH_TRACE_FIELD_DEVICE_ID

    uint32_t deviceId; The ID of the device where the first node of the graph is executed.

    If this is INT_MAX, then the start is on the host.

  enumerator GRAPH_TRACE_FIELD_GRAPH_ID

    uint32_t graphId; The unique ID of the graph that is launched.

  enumerator GRAPH_TRACE_FIELD_CONTEXT_ID

    uint32_t contextId; The ID of the context where the first node of the graph is executed.

    If this is INT_MAX, then the start is on the host.

  enumerator GRAPH_TRACE_FIELD_STREAM_ID

    uint32_t streamId; The ID of the stream where the graph is being launched.

  enumerator GRAPH_TRACE_FIELD_END_DEVICE_ID

    uint32_t endDeviceId; The ID of the device where last node of the graph is executed.

  enumerator GRAPH_TRACE_FIELD_END_CONTEXT_ID

    uint32_t endContextId; The ID of the context where the last node of the graph is executed.

  enumerator GRAPH_TRACE_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityGreenContextFieldIds

  Enum identifiers for fields to trace green context information.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_GREEN_CONTEXT.

  Values:

  enumerator GREEN_CONTEXT_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_GREEN_CONTEXT.

  enumerator GREEN_CONTEXT_FIELD_CONTEXT_ID

    uint32_t contextId; The context ID of the green context.

  enumerator GREEN_CONTEXT_FIELD_PARENT_CONTEXT_ID

    uint32_t parentContextId; The ID of the parent context.

  enumerator GREEN_CONTEXT_FIELD_DEVICE_ID

    uint32_t deviceId; The device ID associated with the green context.

  enumerator GREEN_CONTEXT_FIELD_NUM_MULTIPROCESSORS

    uint16_t numMultiprocessors; The number of multiprocessors (SMs) allocated to the green context.

  enumerator GREEN_CONTEXT_FIELD_NUM_TPCS

    uint32_t numTpcs; The number of TPCs allocated to the green context.

  enumerator GREEN_CONTEXT_FIELD_LOGICAL_TPC_MASK_SIZE

    uint8_t logicalTpcMaskSize; The size (in 32-bit words) of the logical TPC mask.

  enumerator GREEN_CONTEXT_FIELD_LOGICAL_TPC_MASK

    uint32_t logicalTpcMask[32]; The logical TPC mask for the green context.

  enumerator GREEN_CONTEXT_FIELD_WORKQUEUE_RESOURCE_ID

    uint64_t workqueueResourceId; The work queue resource ID associated with the green context.

    Refer

    Param CUdevWorkqueueConfigScope:

      in cuda.h for possible values.

  enumerator GREEN_CONTEXT_FIELD_WORKQUEUE_CONCURRENCY_LIMIT

    uint32_t workqueueConcurrencyLimit; The concurrency limit for the work queue associated with the green context.

  enumerator GREEN_CONTEXT_FIELD_WORKQUEUE_SHARING_SCOPE

    uint32_t workqueueSharingScope; The sharing scope for the work queue associated with the green context.

  enumerator GREEN_CONTEXT_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityHostLaunchFieldIds

  Enum identifiers for fields in CUpti_ActivityHostLaunch.

  Each enum value corresponds to a field in CUpti_ActivityHostLaunch and describes the data type and purpose of that field.

  Values:

  enumerator HOST_LAUNCH_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_HOST_LAUNCH.

  enumerator HOST_LAUNCH_FIELD_STREAM_ID

    uint32_t streamId; ID of the CUDA stream to which the waiting CUDA stream belongs.

  enumerator HOST_LAUNCH_FIELD_CONTEXT_ID

    uint32_t contextId; ID of the CUDA context to which the waiting CUDA stream belongs.

  enumerator HOST_LAUNCH_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the CUDA device to which the CUDA context and stream belong.

  enumerator HOST_LAUNCH_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID of the host launch operation.

  enumerator HOST_LAUNCH_FIELD_PROCESS_ID

    uint32_t processId; ID of the process where the host function is executing.

  enumerator HOST_LAUNCH_FIELD_THREAD_ID

    uint64_t threadId; ID of the thread where the host function is executing.

  enumerator HOST_LAUNCH_FIELD_START

    uint64_t start; Start timestamp.

  enumerator HOST_LAUNCH_FIELD_END

    uint64_t end; End timestamp.

  enumerator HOST_LAUNCH_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityInstructionClass

  SASS instruction classification.

  The sass instruction are broadly divided into different class. Each enum represents a classification.

  Values:

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_UNKNOWN

    The instruction class is not known.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_FP_32

    Represents a 32 bit floating point operation.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_FP_64

    Represents a 64 bit floating point operation.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_INTEGER

    Represents an integer operation.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_BIT_CONVERSION

    Represents a bit conversion operation.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_CONTROL_FLOW

    Represents a control flow instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_GLOBAL

    Represents a global load-store instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_SHARED

    Represents a shared load-store instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_LOCAL

    Represents a local load-store instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_GENERIC

    Represents a generic load-store instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_SURFACE

    Represents a surface load-store instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_CONSTANT

    Represents a constant load instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_TEXTURE

    Represents a texture load-store instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_GLOBAL_ATOMIC

    Represents a global atomic instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_SHARED_ATOMIC

    Represents a shared atomic instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_SURFACE_ATOMIC

    Represents a surface atomic instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_INTER_THREAD_COMMUNICATION

    Represents a inter-thread communication instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_BARRIER

    Represents a barrier instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_MISCELLANEOUS

    Represents some miscellaneous instructions which do not fit in the above classification.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_FP_16

    Represents a 16 bit floating point operation.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_UNIFORM

    Represents uniform instruction.

  enumerator CUPTI_ACTIVITY_INSTRUCTION_CLASS_KIND_FORCE_INT

enum CUpti_ActivityJitEntryType

  The types of JIT entry.

  To be used in CUpti_ActivityJit.

  Values:

  enumerator CUPTI_ACTIVITY_JIT_ENTRY_INVALID
  enumerator CUPTI_ACTIVITY_JIT_ENTRY_PTX_TO_CUBIN

    PTX to CUBIN.

  enumerator CUPTI_ACTIVITY_JIT_ENTRY_NVVM_IR_TO_PTX

    NVVM-IR to PTX.

  enumerator CUPTI_ACTIVITY_JIT_ENTRY_TYPE_FORCE_INT

enum CUpti_ActivityJitFieldIds

  Enum identifiers for fields to trace JIT operations.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_JIT.

  Values:

  enumerator JIT_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_JIT.

  enumerator JIT_FIELD_ENTRY_TYPE

    CUpti_ActivityJitEntryType jitEntryType; The JIT entry type.

    CUpti_ActivityJitEntryType

  enumerator JIT_FIELD_OPERATION_TYPE

    CUpti_ActivityJitOperationType jitOperationType; The JIT operation type.

    CUpti_ActivityJitOperationType

  enumerator JIT_FIELD_DEVICE_ID

    uint32_t deviceId; The device ID.

  enumerator JIT_FIELD_START

    uint64_t start; The start timestamp for the JIT operation (in nanoseconds).

  enumerator JIT_FIELD_END

    uint64_t end; The end timestamp for the JIT operation (in nanoseconds).

  enumerator JIT_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this JIT operation.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator JIT_FIELD_OPERATION_CORRELATION_ID

    uint64_t jitOperationCorrelationId; The correlation ID to correlate JIT compilation, load and store operations.

    Each JIT compilation unit is assigned a unique correlation ID at the time of the JIT compilation. This correlation id can be used to find the matching JIT cache load/store records.

  enumerator JIT_FIELD_CACHE_SIZE

    uint64_t cacheSize; The size of compute cache.

  enumerator JIT_FIELD_CACHE_PATH

    const char* cachePath; The path where the fat binary is cached.

  enumerator JIT_FIELD_PROCESS_ID

    uint32_t processId; The ID of the process where the JIT operation is executing.

  enumerator JIT_FIELD_THREAD_ID

    uint64_t threadId; The ID of the thread where the JIT operation is executing.

  enumerator JIT_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityJitOperationType

  The types of JIT compilation operations.

  To be used in CUpti_ActivityJit.

  Values:

  enumerator CUPTI_ACTIVITY_JIT_OPERATION_INVALID
  enumerator CUPTI_ACTIVITY_JIT_OPERATION_CACHE_LOAD

    Loaded from the compute cache.

  enumerator CUPTI_ACTIVITY_JIT_OPERATION_CACHE_STORE

    Stored in the compute cache.

  enumerator CUPTI_ACTIVITY_JIT_OPERATION_COMPILE

    JIT compilation.

  enumerator CUPTI_ACTIVITY_JIT_OPERATION_TYPE_FORCE_INT

enum CUpti_ActivityKernelFieldIds

  Enum identifiers for fields to trace kernel operations.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL.

  Values:

  enumerator KERNEL_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always either CUPTI_ACTIVITY_KIND_KERNEL or CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL.

  enumerator KERNEL_FIELD_CACHE_CONFIG_REQUESTED

    uint8_t requested; Indicates the cache configuration requested by the kernel.

    Values are from CUfunc_cache enumeration.

  enumerator KERNEL_FIELD_CACHE_CONFIG_EXECUTED

    uint8_t executed; Indicates the cache configuration actually used during kernel execution.

    Values are from CUfunc_cache enumeration.

  enumerator KERNEL_FIELD_SHARED_MEMORY_CONFIG

    uint8_t sharedMemoryConfig; Specifies the shared memory configuration used for the kernel.

    Values are from CUsharedconfig enumeration.

  enumerator KERNEL_FIELD_REGISTERS_PER_THREAD

    uint16_t registersPerThread; Number of registers required for each thread executing the kernel.

  enumerator KERNEL_FIELD_PARTITIONED_GLOBAL_CACHE_REQUESTED

    CUpti_ActivityPartitionedGlobalCacheConfig requested; Partitioned global caching requested for the kernel.

    Relevant for devices requiring this to enable caching.

  enumerator KERNEL_FIELD_PARTITIONED_GLOBAL_CACHE_EXECUTED

    CUpti_ActivityPartitionedGlobalCacheConfig executed; Partitioned global caching actually used during kernel execution.

  enumerator KERNEL_FIELD_START

    uint64_t start; Start timestamp for the kernel execution (in nanoseconds).

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator KERNEL_FIELD_END

    uint64_t end; End timestamp for the kernel execution (in nanoseconds).

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator KERNEL_FIELD_COMPLETED

    uint64_t completed; Completion timestamp for the kernel execution, including all child kernels (in nanoseconds).

    CUPTI_TIMESTAMP_UNKNOWN if unknown.

  enumerator KERNEL_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the device where the kernel is executing.

  enumerator KERNEL_FIELD_CONTEXT_ID

    uint64_t contextId; ID of the context where the kernel is executing.

  enumerator KERNEL_FIELD_STREAM_ID

    uint64_t streamId; ID of the stream where the kernel is executing.

  enumerator KERNEL_FIELD_GRID_X

    int32_t gridX; X-dimension of the grid size for the kernel.

  enumerator KERNEL_FIELD_GRID_Y

    int32_t gridY; Y-dimension of the grid size for the kernel.

  enumerator KERNEL_FIELD_GRID_Z

    int32_t gridZ; Z-dimension of the grid size for the kernel.

  enumerator KERNEL_FIELD_BLOCK_X

    int32_t blockX; X-dimension of the block size for the kernel.

  enumerator KERNEL_FIELD_BLOCK_Y

    int32_t blockY; Y-dimension of the block size for the kernel.

  enumerator KERNEL_FIELD_BLOCK_Z

    int32_t blockZ; Z-dimension of the block size for the kernel.

  enumerator KERNEL_FIELD_STATIC_SHARED_MEMORY

    int32_t staticSharedMemory; Amount of static shared memory allocated for the kernel, in bytes.

  enumerator KERNEL_FIELD_DYNAMIC_SHARED_MEMORY

    int32_t dynamicSharedMemory; Amount of dynamic shared memory reserved for the kernel, in bytes.

  enumerator KERNEL_FIELD_LOCAL_MEMORY_PER_THREAD

    uint32_t localMemoryPerThread; Amount of local memory reserved per thread, in bytes.

  enumerator KERNEL_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID of the kernel, Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator KERNEL_FIELD_GRID_ID

    int64_t gridId; Unique grid ID assigned to the kernel at runtime.

  enumerator KERNEL_FIELD_NAME

    const char* name; Name of the kernel.

    Shared across all activity records for the same kernel.

  enumerator KERNEL_FIELD_QUEUED

    uint64_t queued; Timestamp when the kernel was queued in the command buffer (in nanoseconds).

    CUPTI_TIMESTAMP_UNKNOWN if not collected.

  enumerator KERNEL_FIELD_SUBMITTED

    uint64_t submitted; Timestamp when the command buffer containing the kernel launch was submitted to the GPU (in nanoseconds).

    CUPTI_TIMESTAMP_UNKNOWN if not collected.

  enumerator KERNEL_FIELD_LAUNCH_TYPE

    uint8_t launchType; Indicates if the kernel was executed via a regular launch or a cooperative launch.

    See CUpti_ActivityLaunchType.

  enumerator KERNEL_FIELD_IS_SHARED_MEMORY_CARVEOUT_REQUESTED

    uint8_t isSharedMemoryCarveoutRequested; Indicates if CU_FUNC_ATTRIBUTE_PREFERRED_SHARED_MEMORY_CARVEOUT was updated for the kernel launch.

  enumerator KERNEL_FIELD_SHARED_MEMORY_CARVEOUT_REQUESTED

    uint8_t sharedMemoryCarveoutRequested; Shared memory carveout value requested for the function, as a percentage of the total resource.

  enumerator KERNEL_FIELD_SHARED_MEMORY_EXECUTED

    uint32_t sharedMemoryExecuted; Shared memory size set by the driver, in bytes.

  enumerator KERNEL_FIELD_GRAPH_NODE_ID

    uint64_t graphNodeId; Unique ID of the graph node that launched this kernel through graph launch APIs.

    0 if not launched through graph APIs.

  enumerator KERNEL_FIELD_SHMEM_LIMIT_CONFIG

    CUpti_FuncShmemLimitConfig shmemLimitConfig; Shared memory limit configuration for the kernel, indicating if a higher per-block dynamic shared memory limit was opted.

  enumerator KERNEL_FIELD_GRAPH_ID

    uint32_t graphId; Unique ID of the graph that launched this kernel through graph launch APIs.

    0 if not launched through graph APIs.

  enumerator KERNEL_FIELD_ACCESS_POLICY_WINDOW

    CUaccessPolicyWindow* pAccessPolicyWindow; Pointer to the access policy window structure.

    Defined in cuda.h.

  enumerator KERNEL_FIELD_CHANNEL_ID

    uint32_t channelID; ID of the hardware channel on which the kernel is launched.

  enumerator KERNEL_FIELD_CHANNEL_TYPE

    CUpti_ChannelType channelType; Type of the channel used for kernel launch.

  enumerator KERNEL_FIELD_CLUSTER_X

    int32_t clusterX; X-dimension of the cluster size for the kernel.

    Valid for devices with compute capability 9.0 and higher.

  enumerator KERNEL_FIELD_CLUSTER_Y

    int32_t clusterY; Y-dimension of the cluster size for the kernel.

    Valid for devices with compute capability 9.0 and higher.

  enumerator KERNEL_FIELD_CLUSTER_Z

    int32_t clusterZ; Z-dimension of the cluster size for the kernel.

    Valid for devices with compute capability 9.0 and higher.

  enumerator KERNEL_FIELD_CLUSTER_SCHEDULING_POLICY

    uint32_t clusterSchedulingPolicy; Cluster scheduling policy for the kernel.

    Refer to CUclusterSchedulingPolicy. Valid for devices with compute capability 9.0 and higher.

  enumerator KERNEL_FIELD_LOCAL_MEMORY_TOTAL

    uint64_t localMemoryTotal_v2; Total amount of local memory reserved for the kernel, in bytes.

  enumerator KERNEL_FIELD_MAX_POTENTIAL_CLUSTER_SIZE

    uint32_t maxPotentialClusterSize; Maximum cluster size for the kernel.

  enumerator KERNEL_FIELD_MAX_ACTIVE_CLUSTERS

    uint32_t maxActiveClusters; Maximum number of clusters that could co-exist on the target device for the kernel.

  enumerator KERNEL_FIELD_IS_DEVICE_LAUNCHED

    uint8_t isDeviceLaunched; This field is set to 1 if the kernel is part of a device launched graph.

  enumerator KERNEL_FIELD_LAUNCH_PRIORITY

    int32_t priority; The launch priority of the kernel.

  enumerator KERNEL_FIELD_EXECUTION_MODEL

    uint32_t executionModel; The execution model of the kernel function.

    See also

    CUpti_FuncExecutionModel for possible values.

  enumerator KERNEL_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityKind

  The kinds of activity records.

  Each activity record kind represents information about a GPU or an activity occurring on a CPU or GPU. Each kind is associated with a activity record structure that holds the information associated with the kind.

  See also

  CUpti_Activity

  See also

  CUpti_ActivityAPI

  See also

  CUpti_ActivityContext

  See also

  CUpti_ActivityContext2

  See also

  CUpti_ActivityContext3

  See also

  CUpti_ActivityContext4

  See also

  CUpti_ActivityDevice

  See also

  CUpti_ActivityDevice2

  See also

  CUpti_ActivityDevice3

  See also

  CUpti_ActivityDevice4

  See also

  CUpti_ActivityDevice5

  See also

  CUpti_ActivityDevice6

  See also

  CUpti_ActivityDeviceAttribute

  See also

  CUpti_ActivityEvent

  See also

  CUpti_ActivityEventInstance

  See also

  CUpti_ActivityKernel

  See also

  CUpti_ActivityKernel2

  See also

  CUpti_ActivityKernel3

  See also

  CUpti_ActivityKernel4

  See also

  CUpti_ActivityKernel5

  See also

  CUpti_ActivityKernel6

  See also

  CUpti_ActivityKernel7

  See also

  CUpti_ActivityKernel8

  See also

  CUpti_ActivityKernel9

  See also

  CUpti_ActivityKernel10

  See also

  CUpti_ActivityKernel11

  See also

  CUpti_ActivityKernel12

  See also

  CUpti_ActivityCdpKernel

  See also

  CUpti_ActivityPreemption

  See also

  CUpti_ActivityMemcpy

  See also

  CUpti_ActivityMemcpy3

  See also

  CUpti_ActivityMemcpy4

  See also

  CUpti_ActivityMemcpy5

  See also

  CUpti_ActivityMemcpy6

  See also

  CUpti_ActivityMemcpyPtoP

  See also

  CUpti_ActivityMemcpyPtoP2

  See also

  CUpti_ActivityMemcpyPtoP3

  See also

  CUpti_ActivityMemcpyPtoP4

  See also

  CUpti_ActivityMemset

  See also

  CUpti_ActivityMemset2

  See also

  CUpti_ActivityMemset3

  See also

  CUpti_ActivityMemset4

  See also

  CUpti_ActivityMemory

  See also

  CUpti_ActivityMemory2

  See also

  CUpti_ActivityMemory3

  See also

  CUpti_ActivityMemory4

  See also

  CUpti_ActivityMemoryPool

  See also

  CUpti_ActivityMemoryPool2

  See also

  CUpti_ActivityMemoryPool3

  See also

  CUpti_ActivityMetric

  See also

  CUpti_ActivityMetricInstance

  See also

  CUpti_ActivityName

  See also

  CUpti_ActivityMarker

  See also

  CUpti_ActivityMarker2

  See also

  CUpti_ActivityMarkerData

  See also

  CUpti_ActivitySourceLocator

  See also

  CUpti_ActivityGlobalAccess

  See also

  CUpti_ActivityGlobalAccess2

  See also

  CUpti_ActivityGlobalAccess3

  See also

  CUpti_ActivityBranch

  See also

  CUpti_ActivityBranch2

  See also

  CUpti_ActivityOverhead3

  See also

  CUpti_ActivityEnvironment

  See also

  CUpti_ActivityInstructionExecution

  See also

  CUpti_ActivityUnifiedMemoryCounter

  See also

  CUpti_ActivityFunction

  See also

  CUpti_ActivityModule

  See also

  CUpti_ActivitySharedAccess

  See also

  CUpti_ActivityPCSampling

  See also

  CUpti_ActivityPCSampling2

  See also

  CUpti_ActivityPCSampling3

  See also

  CUpti_ActivityPCSamplingRecordInfo

  See also

  CUpti_ActivityCudaEvent2

  See also

  CUpti_ActivityStream

  See also

  CUpti_ActivitySynchronization2

  See also

  CUpti_ActivityInstructionCorrelation

  See also

  CUpti_ActivityExternalCorrelation

  See also

  CUpti_ActivityUnifiedMemoryCounter3

  See also

  CUpti_ActivityOpenAccData

  See also

  CUpti_ActivityOpenAccLaunch

  See also

  CUpti_ActivityOpenAccOther

  See also

  CUpti_ActivityOpenMp

  See also

  CUpti_ActivityNvLink

  See also

  CUpti_ActivityNvLink2

  See also

  CUpti_ActivityNvLink3

  See also

  CUpti_ActivityNvLink4

  See also

  CUpti_ActivityNvLink5

  See also

  CUpti_ActivityPcie

  See also

  CUpti_ActivityConfidentialComputeRotation

  See also

  CUpti_ActivityComputeEngineCtxSwitch

  Values:

  enumerator CUPTI_ACTIVITY_KIND_INVALID

    The activity record is invalid.

  enumerator CUPTI_ACTIVITY_KIND_MEMCPY

    A host<->host, host<->device, or device<->device memory copy.

    For peer to peer memory copy, use the kind CUPTI_ACTIVITY_KIND_MEMCPY2. The corresponding activity record structure is CUpti_ActivityMemcpy6.

  enumerator CUPTI_ACTIVITY_KIND_MEMSET

    A memory set executing on the GPU.

    The corresponding activity record structure is CUpti_ActivityMemset4.

  enumerator CUPTI_ACTIVITY_KIND_KERNEL

    A kernel executing on the GPU.

    This activity kind may significantly change the overall performance characteristics of the application because all kernel executions are serialized on the GPU. Other activity kind for kernel CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL doesn’t break kernel concurrency. The corresponding activity record structure is CUpti_ActivityKernel12

  enumerator CUPTI_ACTIVITY_KIND_DRIVER

    A CUDA driver API function execution.

    The corresponding activity record structure is CUpti_ActivityAPI.

  enumerator CUPTI_ACTIVITY_KIND_RUNTIME

    A CUDA runtime API function execution.

    The corresponding activity record structure is CUpti_ActivityAPI.

  enumerator CUPTI_ACTIVITY_KIND_EVENT

    A performance counter (aka event) value.

    The corresponding activity record structure is CUpti_ActivityEvent. This activity cannot be directly enabled or disabled. Information collected using the Event API. can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_METRIC

    A performance metric value.

    The corresponding activity record structure is CUpti_ActivityMetric. This activity cannot be directly enabled or disabled. Information collected using the Metric API. can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_DEVICE

    Information about a CUDA device.

    The corresponding activity record structure is CUpti_ActivityDevice6.

  enumerator CUPTI_ACTIVITY_KIND_CONTEXT

    Information about a CUDA context.

    The corresponding activity record structure is CUpti_ActivityContext4.

  enumerator CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL

    A kernel executing on the GPU.

    This activity kind doesn’t break kernel concurrency. The corresponding activity record structure is CUpti_ActivityKernel12.

  enumerator CUPTI_ACTIVITY_KIND_NAME

    Resource naming done via NVTX APIs for thread, device, context, etc.

    The corresponding activity record structure is CUpti_ActivityName.

  enumerator CUPTI_ACTIVITY_KIND_MARKER

    Instantaneous, start, or end NVTX marker.

    The corresponding activity record structure is CUpti_ActivityMarker2.

  enumerator CUPTI_ACTIVITY_KIND_MARKER_DATA

    Extended, optional, data about a NVTX marker.

    User must enable CUPTI_ACTIVITY_KIND_MARKER as well to get records for marker data. The corresponding activity record structure is CUpti_ActivityMarkerData2.

  enumerator CUPTI_ACTIVITY_KIND_SOURCE_LOCATOR

    Source information about source level result.

    The corresponding activity record structure is CUpti_ActivitySourceLocator. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the SASS Metric APIs from the cupti_sass_metrics.h header.

  enumerator CUPTI_ACTIVITY_KIND_GLOBAL_ACCESS

    Results for source-level global access.

    The corresponding activity record structure is CUpti_ActivityGlobalAccess3. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the SASS Metric APIs from the cupti_sass_metrics.h header.

  enumerator CUPTI_ACTIVITY_KIND_BRANCH

    Results for source-level branch.

    The corresponding activity record structure is CUpti_ActivityBranch2. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the SASS Metric APIs from the cupti_sass_metrics.h header.

  enumerator CUPTI_ACTIVITY_KIND_OVERHEAD

    Overhead added by CUPTI, Compiler, CUDA driver etc.

    The corresponding activity record structure is CUpti_ActivityOverhead3.

  enumerator CUPTI_ACTIVITY_KIND_CDP_KERNEL

    A CDP (CUDA Dynamic Parallel) kernel executing on the GPU.

    The corresponding activity record structure is CUpti_ActivityCdpKernel. This activity cannot be directly enabled or disabled. It is enabled and disabled through concurrent kernel activity i.e. _CONCURRENT_KERNEL.

  enumerator CUPTI_ACTIVITY_KIND_PREEMPTION

    Preemption activity record indicating a preemption of a CDP (CUDA Dynamic Parallel) kernel executing on the GPU.

    The corresponding activity record structure is CUpti_ActivityPreemption.

  enumerator CUPTI_ACTIVITY_KIND_ENVIRONMENT

    Environment activity records indicating power, clock, thermal, etc.

    levels of the GPU. The corresponding activity record structure is CUpti_ActivityEnvironment.

  enumerator CUPTI_ACTIVITY_KIND_EVENT_INSTANCE

    An performance counter value associated with a specific event domain instance.

    The corresponding activity record structure is CUpti_ActivityEventInstance. This activity cannot be directly enabled or disabled. Information collected using the Event API. can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_MEMCPY2

    A peer to peer memory copy.

    The corresponding activity record structure is CUpti_ActivityMemcpyPtoP4.

  enumerator CUPTI_ACTIVITY_KIND_METRIC_INSTANCE

    A performance metric value associated with a specific metric domain instance.

    The corresponding activity record structure is CUpti_ActivityMetricInstance. This activity cannot be directly enabled or disabled. Information collected using the Metric API. can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_INSTRUCTION_EXECUTION

    Results for source-level instruction execution.

    The corresponding activity record structure is CUpti_ActivityInstructionExecution. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the SASS Metric APIs from the cupti_sass_metrics.h header.

  enumerator CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER

    Unified Memory counter record.

    The corresponding activity record structure is CUpti_ActivityUnifiedMemoryCounter3.

  enumerator CUPTI_ACTIVITY_KIND_FUNCTION

    Device global/function record.

    The corresponding activity record structure is CUpti_ActivityFunction.

  enumerator CUPTI_ACTIVITY_KIND_MODULE

    CUDA Module record.

    The corresponding activity record structure is CUpti_ActivityModule. This activity cannot be directly enabled or disabled. Information collected using the module callback can be be stored in the corresponding activity record.

  enumerator CUPTI_ACTIVITY_KIND_DEVICE_ATTRIBUTE

    A device attribute value.

    The corresponding activity record structure is CUpti_ActivityDeviceAttribute. This activity cannot be directly enabled or disabled. Information collected using attributes CUpti_DeviceAttribute or CUdevice_attribute can be stored in the corresponding activity record.

  enumerator CUPTI_ACTIVITY_KIND_SHARED_ACCESS

    Results for source-level shared access.

    The corresponding activity record structure is CUpti_ActivitySharedAccess. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the SASS Metric APIs from the cupti_sass_metrics.h header.

  enumerator CUPTI_ACTIVITY_KIND_PC_SAMPLING

    PC sampling information for kernels.

    This will serialize kernels. The corresponding activity record structure is CUpti_ActivityPCSampling3. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the PC Sampling API from the cupti_pcsampling.h header, which allows concurrent kernel execution.

  enumerator CUPTI_ACTIVITY_KIND_PC_SAMPLING_RECORD_INFO

    Summary information about PC sampling records.

    The corresponding activity record structure is CUpti_ActivityPCSamplingRecordInfo. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the PC Sampling API from the cupti_pcsampling.h header.

  enumerator CUPTI_ACTIVITY_KIND_INSTRUCTION_CORRELATION

    SASS/Source line-by-line correlation record.

    This will generate sass/source correlation for functions that have source level analysis or pc sampling results. The records will be generated only when either of source level analysis or pc sampling activity is enabled. The corresponding activity record structure is CUpti_ActivityInstructionCorrelation. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used. Enabling it will return the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED. Instead, use the SASS Metric APIs from the cupti_sass_metrics.h header.

  enumerator CUPTI_ACTIVITY_KIND_OPENACC_DATA

    OpenACC data events.

    The corresponding activity record structure is CUpti_ActivityOpenAccData.

  enumerator CUPTI_ACTIVITY_KIND_OPENACC_LAUNCH

    OpenACC launch events.

    The corresponding activity record structure is CUpti_ActivityOpenAccLaunch.

  enumerator CUPTI_ACTIVITY_KIND_OPENACC_OTHER

    OpenACC other events.

    The corresponding activity record structure is CUpti_ActivityOpenAccOther.

  enumerator CUPTI_ACTIVITY_KIND_CUDA_EVENT

    Information about a CUDA event (cudaEvent).

    The corresponding activity record structure is CUpti_ActivityCudaEvent2.

  enumerator CUPTI_ACTIVITY_KIND_STREAM

    Information about a CUDA stream.

    The corresponding activity record structure is CUpti_ActivityStream.

  enumerator CUPTI_ACTIVITY_KIND_SYNCHRONIZATION

    Records for CUDA synchronization primitives.

    The corresponding activity record structure is CUpti_ActivitySynchronization2.

  enumerator CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION

    Records for correlation of different programming APIs.

    The corresponding activity record structure is CUpti_ActivityExternalCorrelation.

  enumerator CUPTI_ACTIVITY_KIND_NVLINK

    NVLink topology information.

    The corresponding activity record structure is CUpti_ActivityNvLink5.

  enumerator CUPTI_ACTIVITY_KIND_INSTANTANEOUS_EVENT

    Instantaneous Event information.

    The corresponding activity record structure is CUpti_ActivityInstantaneousEvent. This activity can not be directly enabled or disabled. Information collected using the Event API can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_INSTANTANEOUS_EVENT_INSTANCE

    Instantaneous Event information for a specific event domain instance.

    The corresponding activity record structure is CUpti_ActivityInstantaneousEventInstance. This activity can not be directly enabled or disabled. Information collected using the Event API can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_INSTANTANEOUS_METRIC

    Instantaneous Metric information The corresponding activity record structure is CUpti_ActivityInstantaneousMetric.

    This activity cannot be directly enabled or disabled. Information collected using the Metric API can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_INSTANTANEOUS_METRIC_INSTANCE

    Instantaneous Metric information for a specific metric domain instance.

    The corresponding activity record structure is CUpti_ActivityInstantaneousMetricInstance. This activity cannot be directly enabled or disabled. Information collected using the Metric API can be stored in the corresponding activity record. Starting with the CUDA 13.0 release, this enum is unsupported and should no longer be used.

  enumerator CUPTI_ACTIVITY_KIND_MEMORY

    Memory activity tracking allocation and freeing of the memory The corresponding activity record structure is CUpti_ActivityMemory.

  enumerator CUPTI_ACTIVITY_KIND_PCIE

    PCI devices information used for PCI topology.

    The corresponding activity record structure is CUpti_ActivityPcie.

  enumerator CUPTI_ACTIVITY_KIND_OPENMP

    OpenMP parallel events.

    The corresponding activity record structure is CUpti_ActivityOpenMp.

  enumerator CUPTI_ACTIVITY_KIND_INTERNAL_LAUNCH_API

    A CUDA driver kernel launch occurring outside of any public API function execution.

    Tools can handle these like records for driver API launch functions, although the cbid field is not used here. The corresponding activity record structure is CUpti_ActivityAPI.

  enumerator CUPTI_ACTIVITY_KIND_MEMORY2

    Memory activity tracking allocation and freeing of the memory The corresponding activity record structure is CUpti_ActivityMemory4.

  enumerator CUPTI_ACTIVITY_KIND_MEMORY_POOL

    Memory pool activity tracking creation, destruction and trimming of the memory pool.

    The corresponding activity record structure is CUpti_ActivityMemoryPool3.

  enumerator CUPTI_ACTIVITY_KIND_GRAPH_TRACE

    Activity record for graph-level information.

    The corresponding activity record structure is CUpti_ActivityGraphTrace2.

  enumerator CUPTI_ACTIVITY_KIND_JIT

    JIT (Just-in-time) operation tracking.

    The corresponding activity record structure is CUpti_ActivityJit2.

  enumerator CUPTI_ACTIVITY_KIND_DEVICE_GRAPH_TRACE

    This activity can not be directly enabled or disabled.

    It is enabled when CUPTI_ACTIVITY_KIND_GRAPH_TRACE is enabled and device graph trace is enabled through API cuptiActivityEnableDeviceGraph(). The corresponding activity record structure is CUpti_ActivityDeviceGraphTrace.

  enumerator CUPTI_ACTIVITY_KIND_MEM_DECOMPRESS

    Tracing batches of copies that are to be decompressed.

    The corresponding activity record structure is CUpti_ActivityMemDecompress.

  enumerator CUPTI_ACTIVITY_KIND_CONFIDENTIAL_COMPUTE_ROTATION

    Tracing new overheads introduced on some hardware due when confidential computing is enabled.

    The corresponding activity record structure is CUpti_ActivityConfidentialComputeRotation.

  enumerator CUPTI_ACTIVITY_KIND_GRAPH_HOST_NODE

    Tracing of host execution nodes of the CUDA graph, i.e.

    nodes of type CU_GRAPH_NODE_TYPE_HOST. The corresponding activity record structure is CUpti_ActivityGraphHostNode.

  enumerator CUPTI_ACTIVITY_KIND_COMPUTE_ENGINE_CTX_SWITCH

    An activity denoting the switching of Compute Engine contexts in/out of the GPU.

    The corresponding activity record structure is CUpti_ActivityComputeEngineCtxSwitch.

  enumerator CUPTI_ACTIVITY_KIND_HOST_LAUNCH

    An activity kind denoting the launch of a host function through cu(da)LaunchHostFunc API.

    The corresponding activity record structure is CUpti_ActivityHostLaunch.

  enumerator CUPTI_ACTIVITY_KIND_GREEN_CONTEXT

    An activity kind denoting the allocation of a green context.

    The corresponding activity record structure is CUpti_ActivityGreenContext2.

  enumerator CUPTI_ACTIVITY_KIND_COUNT

    Count of supported activity kinds.

  enumerator CUPTI_ACTIVITY_KIND_FORCE_INT

enum CUpti_ActivityLaunchType

  The type of the CUDA kernel launch.

  Values:

  enumerator CUPTI_ACTIVITY_LAUNCH_TYPE_REGULAR

    The kernel was launched via a regular kernel call.

  enumerator CUPTI_ACTIVITY_LAUNCH_TYPE_COOPERATIVE_SINGLE_DEVICE

    The kernel was launched via API cudaLaunchCooperativeKernel() or cuLaunchCooperativeKernel()

  enumerator CUPTI_ACTIVITY_LAUNCH_TYPE_COOPERATIVE_MULTI_DEVICE

    The kernel was launched via API cudaLaunchCooperativeKernelMultiDevice() or cuLaunchCooperativeKernelMultiDevice()

  enumerator CUPTI_ACTIVITY_LAUNCH_TYPE_CBL_COMMANDLIST

    The kernel was launched as a CBL commandlist.

enum CUpti_ActivityMarkerDataFieldIds

  Enum identifiers for fields to trace detailed information for a marker.

  User must enable CUPTI_ACTIVITY_KIND_MARKER as well to get records for marker data. These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MARKER_DATA.

  Values:

  enumerator MARKER_DATA_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MARKER_DATA.

  enumerator MARKER_DATA_FIELD_FLAGS

    CUpti_ActivityFlag flags; Flags associated with the marker.

  enumerator MARKER_DATA_FIELD_ID

    uint32_t id; Marker ID.

  enumerator MARKER_DATA_FIELD_PAYLOAD_KIND

    CUpti_MetricValueKind payloadKind; Defines the payload format for the value associated with the marker.

  enumerator MARKER_DATA_FIELD_PAYLOAD

    CUpti_MetricValue payload; The payload value.

  enumerator MARKER_DATA_FIELD_COLOR

    uint32_t color; The color for the marker.

  enumerator MARKER_DATA_FIELD_CATEGORY

    uint32_t category; The category for the marker.

  enumerator MARKER_DATA_FIELD_CUPTI_DOMAIN_ID

    uint32_t cuptiDomainId; CUPTI maintained domain id required for NVTX extended payloads.

  enumerator MARKER_DATA_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMarkerFieldIds

  Enum identifiers for fields to trace NVTX markers/ranges.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MARKER.

  Values:

  enumerator MARKER_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MARKER.

  enumerator MARKER_FIELD_FLAGS

    CUpti_ActivityFlag flags; Flags associated with the marker.

  enumerator MARKER_FIELD_TIMESTAMP

    uint64_t timestamp; Timestamp for the marker (in ns).

  enumerator MARKER_FIELD_ID

    uint32_t id; Marker ID.

  enumerator MARKER_FIELD_PROCESS_ID

    uint32_t processId; The process ID of the process where the overhead is occurring.

  enumerator MARKER_FIELD_THREAD_ID

    uint64_t threadId; The thread ID of the process where the overhead is occurring.

  enumerator MARKER_FIELD_NAME

    const char *name; Marker name for an instantaneous or start marker.

  enumerator MARKER_FIELD_DOMAIN

    const char *domain; Name of the domain to which this marker belongs.

  enumerator MARKER_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMemDecompressFieldIds

  Enum identifiers for fields to trace decompression operations.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MEM_DECOMPRESS.

  Values:

  enumerator MEM_DECOMPRESS_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MEM_DECOMPRESS.

  enumerator MEM_DECOMPRESS_FIELD_DEVICE_ID

    uint32_t deviceId; The ID of the device where the decompression operation was recorded.

  enumerator MEM_DECOMPRESS_FIELD_CONTEXT_ID

    uint32_t contextId; The ID of the context where the decompression operation was recorded.

  enumerator MEM_DECOMPRESS_FIELD_STREAM_ID

    uint32_t streamId; The compute stream where the decompression operation was recorded.

  enumerator MEM_DECOMPRESS_FIELD_CHANNEL_ID

    uint32_t channelId; The ID of the HW channel on which the decompression operation was recorded.

  enumerator MEM_DECOMPRESS_FIELD_CHANNEL_TYPE

    CUpti_ChannelType channelType; The type of the channel on which the decompression operation was recorded.

  enumerator MEM_DECOMPRESS_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this decompression operation.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator MEM_DECOMPRESS_FIELD_NUMBER_OF_OPERATIONS

    uint32_t numberOfOperations; The number of decompression operations in this batch.

  enumerator MEM_DECOMPRESS_FIELD_SOURCE_BYTES

    uint64_t sourceBytes; The total number of bytes to be read and decompressed in the batch operation.

  enumerator MEM_DECOMPRESS_FIELD_START

    uint64_t start; Start timestamp of the decompression operation, in nanoseconds.

  enumerator MEM_DECOMPRESS_FIELD_END

    uint64_t end; End timestamp of the decompression operation, in nanoseconds.

  enumerator MEM_DECOMPRESS_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMemcpy2FieldIds

  Enum identifiers for fields to trace peer-to-peer memory copies.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MEMCPY2.

  Values:

  enumerator MEMCPY2_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MEMCPY2.

  enumerator MEMCPY2_FIELD_COPY_KIND

    uint8_t copyKind; Type of memory copy.

    ALways CUPTI_ACTIVITY_MEMCPY_KIND_P2P.

    See also

    CUpti_ActivityMemcpyKind

  enumerator MEMCPY2_FIELD_SRC_KIND

    uint8_t srcKind; Kind of source memory used in the copy.

    See also

    CUpti_ActivityMemoryKind

  enumerator MEMCPY2_FIELD_DST_KIND

    uint8_t dstKind; Kind of destination memory used in the copy.

    See also

    CUpti_ActivityMemoryKind

  enumerator MEMCPY2_FIELD_FLAGS

    uint8_t flags; Flags associated with the memory copy.

    See also

    CUpti_ActivityFlag

  enumerator MEMCPY2_FIELD_BYTES

    uint64_t bytes; Number of bytes transferred during the memory copy.

  enumerator MEMCPY2_FIELD_START

    uint64_t start; Start timestamp for the memory copy (in nanoseconds).

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator MEMCPY2_FIELD_END

    uint64_t end; End timestamp for the memory copy (in nanoseconds).

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator MEMCPY2_FIELD_DEVICE_ID

    uint32_t deviceId; Device where the memory copy is occurring.

  enumerator MEMCPY2_FIELD_CONTEXT_ID

    uint32_t contextId; CUDA context where the memory copy is occurring.

  enumerator MEMCPY2_FIELD_STREAM_ID

    uint32_t streamId; Stream in which the memory copy is occurring.

  enumerator MEMCPY2_FIELD_SRC_DEVICE_ID

    uint32_t srcDeviceId; Device from which memory is being copied.

  enumerator MEMCPY2_FIELD_SRC_CONTEXT_ID

    uint32_t srcContextId; CUDA context owning the source memory.

  enumerator MEMCPY2_FIELD_DST_DEVICE_ID

    uint32_t dstDeviceId; Device to which memory is being copied.

  enumerator MEMCPY2_FIELD_DST_CONTEXT_ID

    uint32_t dstContextId; CUDA context owning the destination memory.

  enumerator MEMCPY2_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this memory copy.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator MEMCPY2_FIELD_GRAPH_NODE_ID

    uint64_t graphNodeId; ID of the graph node that launched this memcpy.

    0 if not launched via a CUDA Graph.

  enumerator MEMCPY2_FIELD_GRAPH_ID

    uint32_t graphId; ID of the CUDA Graph associated with this memory copy.

    0 if not launched via a CUDA Graph.

  enumerator MEMCPY2_FIELD_CHANNEL_ID

    uint32_t channelID; Hardware channel ID used for the memory copy.

  enumerator MEMCPY2_FIELD_CHANNEL_TYPE

    CUpti_ChannelType channelType; Type of the hardware channel.

  enumerator MEMCPY2_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMemcpyFieldIds

  Enum identifiers for fields to trace memory copies.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MEMCPY.

  Values:

  enumerator MEMCPY_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MEMCPY.

  enumerator MEMCPY_FIELD_COPY_KIND

    uint8_t copyKind; Type of memory copy operation.

    See also

    CUpti_ActivityMemcpyKind

  enumerator MEMCPY_FIELD_SRC_KIND

    uint8_t srcKind; Memory kind of the source location.

    See also

    CUpti_ActivityMemoryKind

  enumerator MEMCPY_FIELD_DST_KIND

    uint8_t dstKind; Memory kind of the destination location.

    See also

    CUpti_ActivityMemoryKind

  enumerator MEMCPY_FIELD_FLAGS

    uint8_t flags; Flags associated with the memory copy.

    See also

    CUpti_ActivityFlag

  enumerator MEMCPY_FIELD_BYTES

    uint64_t bytes; Number of bytes copied during the memory operation.

  enumerator MEMCPY_FIELD_START

    uint64_t start; Start timestamp of the memory copy, in nanoseconds.

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator MEMCPY_FIELD_END

    uint64_t end; End timestamp of the memory copy, in nanoseconds.

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator MEMCPY_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the device where the memory copy occurred.

  enumerator MEMCPY_FIELD_CONTEXT_ID

    uint32_t contextId; ID of the CUDA context where the memory copy occurred.

  enumerator MEMCPY_FIELD_STREAM_ID

    uint32_t streamId; ID of the stream where the memory copy occurred.

  enumerator MEMCPY_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this memory copy.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator MEMCPY_FIELD_GRAPH_NODE_ID

    uint64_t graphNodeId; ID of the CUDA Graph node that launched this memory copy.

    0 if not launched via a CUDA Graph.

  enumerator MEMCPY_FIELD_GRAPH_ID

    uint32_t graphId; ID of the CUDA Graph that launched this memory copy.

    0 if not launched via a CUDA Graph.

  enumerator MEMCPY_FIELD_CHANNEL_ID

    uint32_t channelID; ID of the hardware channel on which this memory copy was executed.

  enumerator MEMCPY_FIELD_CHANNEL_TYPE

    CUpti_ChannelType channelType; Type of the hardware channel used.

  enumerator MEMCPY_FIELD_IS_DEVICE_LAUNCHED

    uint8_t isDeviceLaunched; This field is set to 1 if the kernel is part of a device launched graph.

  enumerator MEMCPY_FIELD_COPY_COUNT

    uint64_t copyCount; Number of individual memcpy operations traced in this record.

    >1 if batched using MemcpyBatchAsync; otherwise 1.

  enumerator MEMCPY_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMemcpyKind

  The kind of a memory copy, indicating the source and destination targets of the copy.

  Each kind represents the source and destination targets of a memory copy. Targets are host, device, and array.

  Values:

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_UNKNOWN

    The memory copy kind is not known.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_HTOD

    A host to device memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_DTOH

    A device to host memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_HTOA

    A host to device array memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_ATOH

    A device array to host memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_ATOA

    A device array to device array memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_ATOD

    A device array to device memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_DTOA

    A device to device array memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_DTOD

    A device to device memory copy on the same device.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_HTOH

    A host to host memory copy.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_PTOP

    A peer to peer memory copy across different devices.

  enumerator CUPTI_ACTIVITY_MEMCPY_KIND_FORCE_INT

enum CUpti_ActivityMemoryFieldIds

  Enum identifiers for fields to trace memory allocation and free operation.

  This activity record provides separate records for memory allocation and memory release operations. This allows to correlate the corresponding driver and runtime API activity record with the memory operation.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MEMORY2.

  Values:

  enumerator MEMORY_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MEMORY2.

  enumerator MEMORY_FIELD_OPERATION_TYPE

    CUpti_ActivityMemoryOperationType memoryOperationType; The memory operation requested by the user.

  enumerator MEMORY_FIELD_MEMORY_KIND

    CUpti_ActivityMemoryKind memoryKind; The memory kind requested by the user.

  enumerator MEMORY_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID of the memory operation.

  enumerator MEMORY_FIELD_ADDRESS

    uint64_t address; Virtual address of the allocation.

  enumerator MEMORY_FIELD_BYTES

    uint64_t bytes; Number of bytes of memory allocated.

  enumerator MEMORY_FIELD_TIMESTAMP

    uint64_t timestamp; Start timestamp for the memory operation (in ns).

  enumerator MEMORY_FIELD_PROCESS_ID

    uint32_t processId; ID of the process to which this record belongs.

  enumerator MEMORY_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the device where the memory operation is taking place.

  enumerator MEMORY_FIELD_CONTEXT_ID

    uint32_t contextId; ID of the context.

  enumerator MEMORY_FIELD_STREAM_ID

    uint32_t streamId; ID of the stream.

  enumerator MEMORY_FIELD_IS_ASYNC

    uint32_t isAsync; Whether the memory operation happens through async memory APIs.

  enumerator MEMORY_FIELD_POOL_TYPE

    CUpti_ActivityMemoryPoolType memoryPoolConfig.memoryPoolType; Type of the memory pool.

  enumerator MEMORY_FIELD_POOL_ADDRESS

    uint64_t memoryPoolConfig.address; Base address of the memory pool.

  enumerator MEMORY_FIELD_POOL_RELEASE_THRESHOLD

    uint64_t memoryPoolConfig.releaseThreshold; Release threshold of the memory pool in bytes.

  enumerator MEMORY_FIELD_POOL_SIZE

    uint64_t memoryPoolConfig.pool.size; Size of memory pool in bytes.

  enumerator MEMORY_FIELD_POOL_PROCESS_ID

    uint64_t memoryPoolConfig.pool.processId; Process ID of the memory pools.

  enumerator MEMORY_FIELD_POOL_UTILIZED_SIZE

    uint64_t memoryPoolConfig.utilizedSize; Utilized size of the memory pool.

  enumerator MEMORY_FIELD_SOURCE

    const char* source; Shared object or binary that the memory allocation request comes from.

  enumerator MEMORY_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMemoryKind

  The kinds of memory accessed by a memory operation/copy.

  Each kind represents the type of the memory accessed by a memory operation/copy.

  Values:

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_UNKNOWN

    The memory kind is unknown.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_PAGEABLE

    The memory is pageable.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_PINNED

    The memory is pinned.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_DEVICE

    The memory is on the device.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_ARRAY

    The memory is an array.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_MANAGED

    The memory is managed.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_DEVICE_STATIC

    The memory is device static.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_MANAGED_STATIC

    The memory is managed static.

  enumerator CUPTI_ACTIVITY_MEMORY_KIND_FORCE_INT

enum CUpti_ActivityMemoryOperationType

  Memory operation types.

  Describes the type of memory operation, to be used with CUpti_ActivityMemory4.

  Values:

  enumerator CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_INVALID

    The operation is invalid.

  enumerator CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_ALLOCATION

    Memory is allocated.

  enumerator CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_RELEASE

    Memory is released.

  enumerator CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_FORCE_INT

enum CUpti_ActivityMemoryPoolFieldIds

  Enum identifiers for fields to trace CUDA memory pool creation, destruction and trimming.

  This activity record provides separate records for memory pool creation, destruction and trimming operations. This allows to correlate the corresponding driver and runtime API activity record with the memory pool operation.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MEMORY_POOL.

  Values:

  enumerator MEMORY_POOL_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MEMORY_POOL.

  enumerator MEMORY_POOL_FIELD_OPERATION_TYPE

    CUpti_ActivityMemoryPoolOperationType memoryPoolOperationType; The memory operation requested by the user.

  enumerator MEMORY_POOL_FIELD_POOL_TYPE

    CUpti_ActivityMemoryPoolType memoryPoolType; The type of the memory pool.

  enumerator MEMORY_POOL_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this memory pool operation.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator MEMORY_POOL_FIELD_PROCESS_ID

    uint32_t processId; ID of the process to which this record belongs.

  enumerator MEMORY_POOL_FIELD_DEVICE_ID

    uint32_t deviceId; ID of the device where the memory pool is created.

  enumerator MEMORY_POOL_FIELD_MIN_BYTES_TO_KEEP

    size_t minBytesToKeep; Minimum bytes to keep of the memory pool.

  enumerator MEMORY_POOL_FIELD_ADDRESS

    uint64_t address; Virtual address of the allocation.

  enumerator MEMORY_POOL_FIELD_SIZE

    uint64_t size; Size of the memory pool operation in bytes.

  enumerator MEMORY_POOL_FIELD_RELEASE_THRESHOLD

    uint64_t releaseThreshold; Release threshold of the memory pool.

  enumerator MEMORY_POOL_FIELD_TIMESTAMP

    uint64_t timestamp; Start timestamp for the memory operation (in ns).

  enumerator MEMORY_POOL_FIELD_UTILIZED_SIZE

    uint64_t utilizedSize; Utilized size of the memory pool.

  enumerator MEMORY_POOL_FIELD_IS_MANAGED_POOL

    uint8_t isManagedPool; Whether the pool is of managed memory allocation or pinned memory allocation.

  enumerator MEMORY_POOL_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityMemoryPoolOperationType

  Memory pool operation types.

  Describes the type of memory pool operation, to be used with CUpti_ActivityMemoryPool2.

  Values:

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_INVALID

    The operation is invalid.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_CREATED

    Memory pool is created.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_DESTROYED

    Memory pool is destroyed.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_TRIMMED

    Memory pool is trimmed.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_FORCE_INT

enum CUpti_ActivityMemoryPoolType

  Memory pool types.

  Describes the type of memory pool, to be used with CUpti_ActivityMemory4.

  Values:

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_TYPE_INVALID

    The operation is invalid.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_TYPE_LOCAL

    Memory pool is local to the process.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_TYPE_IMPORTED

    Memory pool is imported by the process.

  enumerator CUPTI_ACTIVITY_MEMORY_POOL_TYPE_FORCE_INT

enum CUpti_ActivityMemsetFieldIds

  Enum identifiers for fields to trace memset operations.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_MEMSET.

  Values:

  enumerator MEMSET_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_MEMSET.

  enumerator MEMSET_FIELD_VALUE

    uint32_t value; Value being written to memory by the memset.

  enumerator MEMSET_FIELD_BYTES

    uint64_t bytes; Number of bytes being set.

  enumerator MEMSET_FIELD_START

    uint64_t start; Start timestamp for the memset operation (in nanoseconds).

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator MEMSET_FIELD_END

    uint64_t end; End timestamp for the memset operation (in nanoseconds).

    A value of 0 indicates timestamp couldn’t be collected.

  enumerator MEMSET_FIELD_DEVICE_ID

    uint32_t deviceId; Device on which the memset is occurring.

  enumerator MEMSET_FIELD_CONTEXT_ID

    uint32_t contextId; CUDA context where the memset is occurring.

  enumerator MEMSET_FIELD_STREAM_ID

    uint32_t streamId; Stream where the memset is occurring.

  enumerator MEMSET_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this memset operation.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator MEMSET_FIELD_FLAGS

    uint16_t flags; Flags associated with the memset.

    See also

    CUpti_ActivityFlag

  enumerator MEMSET_FIELD_MEMORY_KIND

    uint16_t memoryKind; Kind of memory being set.

    See also

    CUpti_ActivityMemoryKind

  enumerator MEMSET_FIELD_GRAPH_NODE_ID

    uint64_t graphNodeId; CUDA Graph node ID that executed this memset.

  enumerator MEMSET_FIELD_GRAPH_ID

    uint32_t graphId; CUDA Graph ID that executed this memset.

  enumerator MEMSET_FIELD_CHANNEL_ID

    uint32_t channelID; Hardware channel ID used by the memset.

  enumerator MEMSET_FIELD_CHANNEL_TYPE

    CUpti_ChannelType channelType; Type of hardware channel used by the memset.

  enumerator MEMSET_FIELD_IS_DEVICE_LAUNCHED

    uint8_t isDeviceLaunched; This field is set to 1 if the kernel is part of a device launched graph.

  enumerator MEMSET_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityNameFieldIds

  Enum identifiers for fields in CUpti_ActivityName.

  Each enum value corresponds to a field in CUpti_ActivityName and describes the data type and purpose of that field.

  Values:

  enumerator NAME_FIELD_KIND

    CUpti_ActivityKind kind; Kind of activity record: CUPTI_ACTIVITY_KIND_NAME.

  enumerator NAME_FIELD_OBJECT_KIND

    CUpti_ActivityObjectKind objectKind; Kind of activity object being named.

  enumerator NAME_FIELD_OBJECT_ID

    CUpti_ActivityObjectKindId objectId; Identifier for the activity object being named.

  enumerator NAME_FIELD_NAME

    const char *name; The name.

  enumerator NAME_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityNvLinkFieldIds

  Enum identifiers for fields in CUpti_ActivityNvLink5.

  Each enum value corresponds to a field in CUpti_ActivityNvLink5 and describes the data type and purpose of that field.

  Values:

  enumerator NVLINK_FIELD_KIND

    CUpti_ActivityKind kind; Kind of activity record: CUPTI_ACTIVITY_KIND_NVLINK.

  enumerator NVLINK_FIELD_NVLINK_VERSION

    uint32_t nvlinkVersion; NvLink version.

  enumerator NVLINK_FIELD_TYPE_DEV0

    CUpti_DevType typeDev0; Type of device 0.

  enumerator NVLINK_FIELD_TYPE_DEV1

    CUpti_DevType typeDev1; Type of device 1.

  enumerator NVLINK_FIELD_ID_DEV0

    union idDev0; If typeDev0 is CUPTI_DEV_TYPE_GPU, UUID for device 0.

    If typeDev0 is CUPTI_DEV_TYPE_NPU, CUpti_ActivityNvLinkNpu for NPU.

  enumerator NVLINK_FIELD_ID_DEV1

    union idDev1; If typeDev1 is CUPTI_DEV_TYPE_GPU, UUID for device 1.

    If typeDev1 is CUPTI_DEV_TYPE_NPU, CUpti_ActivityNvLinkNpu for NPU.

  enumerator NVLINK_FIELD_FLAG

    uint32_t flag; Flag gives capabilities of the link (CUpti_LinkFlag).

  enumerator NVLINK_FIELD_PHYSICAL_NVLINK_COUNT

    uint32_t physicalNvLinkCount; Number of physical NVLinks present between two devices.

  enumerator NVLINK_FIELD_PORT_DEV0

    uint32_t* portDev0; Port numbers for NVLinks connected to device 0.

  enumerator NVLINK_FIELD_PORT_DEV1

    uint32_t* portDev1; Port numbers for NVLinks connected to device 1.

  enumerator NVLINK_FIELD_BANDWIDTH

    uint64_t bandwidth; Bandwidth of NVLink in kbytes/sec.

  enumerator NVLINK_FIELD_NVSWITCH_CONNECTED

    uint8_t nvswitchConnected; NVSwitch is connected as an intermediate node.

  enumerator NVLINK_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityObjectKind

  The kinds of activity objects.

  See also

  CUpti_ActivityObjectKindId

  Values:

  enumerator CUPTI_ACTIVITY_OBJECT_UNKNOWN

    The object kind is not known.

  enumerator CUPTI_ACTIVITY_OBJECT_PROCESS

    A process.

  enumerator CUPTI_ACTIVITY_OBJECT_THREAD

    A thread.

  enumerator CUPTI_ACTIVITY_OBJECT_DEVICE

    A device.

  enumerator CUPTI_ACTIVITY_OBJECT_CONTEXT

    A context.

  enumerator CUPTI_ACTIVITY_OBJECT_STREAM

    A stream.

  enumerator CUPTI_ACTIVITY_OBJECT_FORCE_INT

enum CUpti_ActivityOpenAccDataFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenAccData.

  Each enum value corresponds to a field in CUpti_ActivityOpenAccData and documents the exact meaning of that field.

  Values:

  enumerator OPENACC_DATA_FIELD_KIND

    CUpti_ActivityKind kind; The activity record kind.

    Must be CUPTI_ACTIVITY_KIND_OPENACC_DATA.

  enumerator OPENACC_DATA_FIELD_EVENT_KIND

    CUpti_OpenAccEventKind eventKind; CUPTI OpenACC event kind.

  enumerator OPENACC_DATA_FIELD_PARENT_CONSTRUCT

    CUpti_OpenAccConstructKind parentConstruct; Parent OpenACC construct kind.

    For PGI OpenACC runtime < 16.1, this is always CUPTI_OPENACC_CONSTRUCT_KIND_UNKNOWN.

  enumerator OPENACC_DATA_FIELD_VERSION

    uint32_t version; Version number.

  enumerator OPENACC_DATA_FIELD_IMPLICIT

    uint32_t implicit; 1 if this is an implicit event (e.g.

    implicit wait), 0 otherwise.

  enumerator OPENACC_DATA_FIELD_DEVICE_TYPE

    uint32_t deviceType; OpenACC device type.

  enumerator OPENACC_DATA_FIELD_DEVICE_NUMBER

    uint32_t deviceNumber; OpenACC device number.

  enumerator OPENACC_DATA_FIELD_THREAD_ID

    uint32_t threadId; Thread ID.

  enumerator OPENACC_DATA_FIELD_ASYNC

    uint64_t async; Value of the async() clause of the corresponding directive.

  enumerator OPENACC_DATA_FIELD_ASYNC_MAP

    uint64_t asyncMap; Internal asynchronous queue number used.

  enumerator OPENACC_DATA_FIELD_LINE_NO

    uint32_t lineNo; Line number of the directive or construct start.

    A non-positive value indicates unknown.

  enumerator OPENACC_DATA_FIELD_END_LINE_NO

    uint32_t endLineNo; Line number of the end of the OpenACC construct.

    A non-positive value indicates unknown.

  enumerator OPENACC_DATA_FIELD_FUNC_LINE_NO

    uint32_t funcLineNo; First line number of the function in which the event occurred.

    A non-positive value indicates unknown.

  enumerator OPENACC_DATA_FIELD_FUNC_END_LINE_NO

    uint32_t funcEndLineNo; Last line number of the function in which the event occurred.

    A non-positive value indicates unknown.

  enumerator OPENACC_DATA_FIELD_START

    uint64_t start; CUPTI start timestamp (in ns).

  enumerator OPENACC_DATA_FIELD_END

    uint64_t end; CUPTI end timestamp (in ns).

  enumerator OPENACC_DATA_FIELD_CU_DEVICE_ID

    uint32_t cuDeviceId; CUDA device ID.

    Valid only if deviceType is acc_device_nvidia.

  enumerator OPENACC_DATA_FIELD_CU_CONTEXT_ID

    uint32_t cuContextId; CUDA context ID.

    Valid only if deviceType is acc_device_nvidia.

  enumerator OPENACC_DATA_FIELD_CU_STREAM_ID

    uint32_t cuStreamId; CUDA stream ID.

    Valid only if deviceType is acc_device_nvidia.

  enumerator OPENACC_DATA_FIELD_CU_PROCESS_ID

    uint32_t cuProcessId; Process ID where the OpenACC activity is executing.

  enumerator OPENACC_DATA_FIELD_CU_THREAD_ID

    uint64_t cuThreadId; Thread ID where the OpenACC activity is executing.

  enumerator OPENACC_DATA_FIELD_EXTERNAL_ID

    uint32_t externalId; OpenACC correlation ID.

    Matches the externalId from the corresponding CUPTI_EXTERNAL_CORRELATION_KIND_OPENACC record.

  enumerator OPENACC_DATA_FIELD_SRC_FILE

    const char* srcFile; Pointer to a null-terminated string containing the source file name or path, if known.

  enumerator OPENACC_DATA_FIELD_FUNC_NAME

    const char* funcName; Pointer to a null-terminated string containing the function name.

  enumerator OPENACC_DATA_FIELD_BYTES

    uint64_t bytes; Number of bytes involved in the operation.

  enumerator OPENACC_DATA_FIELD_HOST_PTR

    uint64_t hostPtr; Host pointer, if available.

  enumerator OPENACC_DATA_FIELD_DEVICE_PTR

    uint64_t devicePtr; Device pointer, if available.

  enumerator OPENACC_DATA_FIELD_VAR_NAME

    const char* varName; Pointer to a null-terminated string containing the variable name for which this event is triggered.

  enumerator OPENACC_DATA_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityOpenAccLaunchFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenAccLaunch.

  Each enum value corresponds to a field in CUpti_ActivityOpenAccLaunch and documents the exact meaning of that field.

  Values:

  enumerator OPENACC_LAUNCH_FIELD_KIND

    CUpti_ActivityKind kind; The activity record kind, must be CUPTI_ACTIVITY_KIND_OPENACC_LAUNCH.

  enumerator OPENACC_LAUNCH_FIELD_EVENT_KIND

    CUpti_OpenAccEventKind eventKind; CUPTI OpenACC event kind.

  enumerator OPENACC_LAUNCH_FIELD_PARENT_CONSTRUCT

    CUpti_OpenAccConstructKind parentConstruct; CUPTI OpenACC parent construct kind.

  enumerator OPENACC_LAUNCH_FIELD_VERSION

    uint32_t version; Version number.

  enumerator OPENACC_LAUNCH_FIELD_IMPLICIT

    uint32_t implicit; 1 for implicit event, 0 otherwise.

  enumerator OPENACC_LAUNCH_FIELD_DEVICE_TYPE

    uint32_t deviceType; Device type.

  enumerator OPENACC_LAUNCH_FIELD_DEVICE_NUMBER

    uint32_t deviceNumber; Device number.

  enumerator OPENACC_LAUNCH_FIELD_THREAD_ID

    uint32_t threadId; Thread identifier.

  enumerator OPENACC_LAUNCH_FIELD_ASYNC

    uint64_t async; Value of async() clause of the corresponding directive.

  enumerator OPENACC_LAUNCH_FIELD_ASYNC_MAP

    uint64_t asyncMap; Internal asynchronous queue number used.

  enumerator OPENACC_LAUNCH_FIELD_LINE_NO

    uint32_t lineNo; Line number of the directive or construct.

  enumerator OPENACC_LAUNCH_FIELD_END_LINE_NO

    uint32_t endLineNo; Line number of the end of the construct.

  enumerator OPENACC_LAUNCH_FIELD_FUNC_LINE_NO

    uint32_t funcLineNo; Starting line number of the function.

  enumerator OPENACC_LAUNCH_FIELD_FUNC_END_LINE_NO

    uint32_t funcEndLineNo; Ending line number of the function.

  enumerator OPENACC_LAUNCH_FIELD_START

    uint64_t start; CUPTI start timestamp.

  enumerator OPENACC_LAUNCH_FIELD_END

    uint64_t end; CUPTI end timestamp.

  enumerator OPENACC_LAUNCH_FIELD_CU_DEVICE_ID

    uint32_t cuDeviceId; CUDA device id.

  enumerator OPENACC_LAUNCH_FIELD_CU_CONTEXT_ID

    uint32_t cuContextId; CUDA context id.

  enumerator OPENACC_LAUNCH_FIELD_CU_STREAM_ID

    uint32_t cuStreamId; CUDA stream id.

  enumerator OPENACC_LAUNCH_FIELD_CU_PROCESS_ID

    uint32_t cuProcessId; Process id where the activity is executing.

  enumerator OPENACC_LAUNCH_FIELD_CU_THREAD_ID

    uint64_t cuThreadId; Thread id where the activity is executing.

  enumerator OPENACC_LAUNCH_FIELD_EXTERNAL_ID

    uint32_t externalId; OpenACC correlation id.

  enumerator OPENACC_LAUNCH_FIELD_SRC_FILE

    const char *srcFile; Pointer to null-terminated string containing source file name or path.

  enumerator OPENACC_LAUNCH_FIELD_FUNC_NAME

    const char *funcName; Pointer to null-terminated string containing function name.

  enumerator OPENACC_LAUNCH_FIELD_NUM_GANGS

    uint64_t numGangs; Number of gangs created for this kernel launch.

  enumerator OPENACC_LAUNCH_FIELD_NUM_WORKERS

    uint64_t numWorkers; Number of workers created for this kernel launch.

  enumerator OPENACC_LAUNCH_FIELD_VECTOR_LENGTH

    uint64_t vectorLength; Number of vector lanes created for this kernel launch.

  enumerator OPENACC_LAUNCH_FIELD_KERNEL_NAME

    const char *kernelName; Pointer to null-terminated string containing kernel name.

  enumerator OPENACC_LAUNCH_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityOpenAccOtherFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenAccOther.

  Each enum value corresponds to a field in CUpti_ActivityOpenAccOther and documents the exact meaning of that field.

  Values:

  enumerator OPENACC_OTHER_FIELD_KIND

    CUpti_ActivityKind kind; The activity record kind, must be CUPTI_ACTIVITY_KIND_OPENACC_OTHER.

  enumerator OPENACC_OTHER_FIELD_EVENT_KIND

    CUpti_OpenAccEventKind eventKind; CUPTI OpenACC event kind.

  enumerator OPENACC_OTHER_FIELD_PARENT_CONSTRUCT

    CUpti_OpenAccConstructKind parentConstruct; CUPTI OpenACC parent construct kind.

  enumerator OPENACC_OTHER_FIELD_VERSION

    uint32_t version; Version number.

  enumerator OPENACC_OTHER_FIELD_IMPLICIT

    uint32_t implicit; 1 for implicit event, 0 otherwise.

  enumerator OPENACC_OTHER_FIELD_DEVICE_TYPE

    uint32_t deviceType; Device type.

  enumerator OPENACC_OTHER_FIELD_DEVICE_NUMBER

    uint32_t deviceNumber; Device number.

  enumerator OPENACC_OTHER_FIELD_THREAD_ID

    uint32_t threadId; Thread identifier.

  enumerator OPENACC_OTHER_FIELD_ASYNC

    uint64_t async; Value of async() clause of the corresponding directive.

  enumerator OPENACC_OTHER_FIELD_ASYNC_MAP

    uint64_t asyncMap; Internal asynchronous queue number used.

  enumerator OPENACC_OTHER_FIELD_LINE_NO

    uint32_t lineNo; Line number of the directive or construct.

  enumerator OPENACC_OTHER_FIELD_END_LINE_NO

    uint32_t endLineNo; Line number of the end of the construct.

  enumerator OPENACC_OTHER_FIELD_FUNC_LINE_NO

    uint32_t funcLineNo; Starting line number of the function.

  enumerator OPENACC_OTHER_FIELD_FUNC_END_LINE_NO

    uint32_t funcEndLineNo; Ending line number of the function.

  enumerator OPENACC_OTHER_FIELD_START

    uint64_t start; CUPTI start timestamp.

  enumerator OPENACC_OTHER_FIELD_END

    uint64_t end; CUPTI end timestamp.

  enumerator OPENACC_OTHER_FIELD_CU_DEVICE_ID

    uint32_t cuDeviceId; CUDA device id.

  enumerator OPENACC_OTHER_FIELD_CU_CONTEXT_ID

    uint32_t cuContextId; CUDA context id.

  enumerator OPENACC_OTHER_FIELD_CU_STREAM_ID

    uint32_t cuStreamId; CUDA stream id.

  enumerator OPENACC_OTHER_FIELD_CU_PROCESS_ID

    uint32_t cuProcessId; Process id where the activity is executing.

  enumerator OPENACC_OTHER_FIELD_CU_THREAD_ID

    uint64_t cuThreadId; Thread id where the activity is executing.

  enumerator OPENACC_OTHER_FIELD_EXTERNAL_ID

    uint32_t externalId; OpenACC correlation id.

  enumerator OPENACC_OTHER_FIELD_SRC_FILE

    const char *srcFile; Pointer to null-terminated string containing source file name or path.

  enumerator OPENACC_OTHER_FIELD_FUNC_NAME

    const char *funcName; Pointer to null-terminated string containing function name.

  enumerator OPENACC_OTHER_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityOpenMpFieldIds

  Enum identifiers for fields in CUpti_ActivityOpenMp.

  This activity record records OpenMP activity information.

  Values:

  enumerator OPENMP_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_OPENMP.

  enumerator OPENMP_FIELD_EVENT_KIND

    CUpti_OpenMpEventKind eventKind; CUPTI OpenMP event kind (.

    See also

    CUpti_OpenMpEventKind)

  enumerator OPENMP_FIELD_START

    uint64_t start; CUPTI start timestamp

  enumerator OPENMP_FIELD_END

    uint64_t end; CUPTI end timestamp

  enumerator OPENMP_FIELD_CU_THREAD_ID

    uint64_t cuThreadId; The ID of the thread where the OpenMP activity is executing.

  enumerator OPENMP_FIELD_CU_PROCESS_ID

    uint32_t cuProcessId; The ID of the process where the OpenMP activity is executing.

  enumerator OPENMP_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityOverheadFieldIds

  Enum identifiers for fields to trace CUPTI and driver overhead information.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_OVERHEAD.

  Values:

  enumerator OVERHEAD_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_OVERHEAD.

  enumerator OVERHEAD_FIELD_OVERHEAD_KIND

    CUpti_ActivityOverheadKind overheadKind; The kind of overhead, CUPTI, DRIVER, COMPILER etc.

  enumerator OVERHEAD_FIELD_PROCESS_ID

    uint32_t processId; The process ID of the process where the overhead is occurring.

  enumerator OVERHEAD_FIELD_THREAD_ID

    uint64_t threadId; The thread ID of the process where the overhead is occurring.

  enumerator OVERHEAD_FIELD_START

    uint64_t start; The start timestamp for the overhead, in nanoseconds.

  enumerator OVERHEAD_FIELD_END

    uint64_t end; The end timestamp for the overhead, in nanoseconds.

  enumerator OVERHEAD_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this overhead record.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator OVERHEAD_FIELD_OVERHEAD_DATA

    void *overheadData; Pointer to the struct with additional details about the overhead.

    Refer CUpti_ActivityOverheadKind enum and the corresponding structure to typecast and access additional overhead data. Client is responsible for freeing this memory using the free function when done.

  enumerator OVERHEAD_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityOverheadKind

  The kinds of activity overhead.

  Values:

  enumerator CUPTI_ACTIVITY_OVERHEAD_UNKNOWN

    The overhead kind is not known.

  enumerator CUPTI_ACTIVITY_OVERHEAD_DRIVER_COMPILER

    Compiler overhead.

  enumerator CUPTI_ACTIVITY_OVERHEAD_CUPTI_BUFFER_FLUSH

    Activity buffer flush overhead.

  enumerator CUPTI_ACTIVITY_OVERHEAD_CUPTI_INSTRUMENTATION

    CUPTI instrumentation overhead.

  enumerator CUPTI_ACTIVITY_OVERHEAD_CUPTI_RESOURCE

    CUPTI resource creation and destruction overhead.

  enumerator CUPTI_ACTIVITY_OVERHEAD_RUNTIME_TRIGGERED_MODULE_LOADING

    CUDA Runtime triggered module loading overhead.

  enumerator CUPTI_ACTIVITY_OVERHEAD_LAZY_FUNCTION_LOADING

    Lazy function loading overhead.

  enumerator CUPTI_ACTIVITY_OVERHEAD_COMMAND_BUFFER_FULL

    Overhead due to lack of command buffer space.

    Refer CUpti_ActivityOverheadCommandBufferFullData for more details.

  enumerator CUPTI_ACTIVITY_OVERHEAD_ACTIVITY_BUFFER_REQUEST

    Overhead due to activity buffer request.

  enumerator CUPTI_ACTIVITY_OVERHEAD_UVM_ACTIVITY_INIT

    Overhead due to UVM activity initialization.

  enumerator CUPTI_ACTIVITY_OVERHEAD_FORCE_INT

enum CUpti_ActivityPCSamplingPeriod

  Sampling period for PC sampling method.

  Sampling period can be set using cuptiActivityConfigurePCSampling

  Values:

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_INVALID

    The PC sampling period is not set.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_MIN

    Minimum sampling period available on the device.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_LOW

    Sampling period in lower range.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_MID

    Medium sampling period.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_HIGH

    Sampling period in higher range.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_MAX

    Maximum sampling period available on the device.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_FORCE_INT

enum CUpti_ActivityPCSamplingStallReason

  The stall reason for PC sampling activity.

  Values:

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_INVALID

    Invalid reason.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_NONE

    No stall, instruction is selected for issue.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_INST_FETCH

    Warp is blocked because next instruction is not yet available, because of instruction cache miss, or because of branching effects.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_EXEC_DEPENDENCY

    Instruction is waiting on an arithmetic dependency.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_MEMORY_DEPENDENCY

    Warp is blocked because it is waiting for a memory access to complete.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_TEXTURE

    Texture sub-system is fully utilized or has too many outstanding requests.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_SYNC

    Warp is blocked as it is waiting at __syncthreads() or at memory barrier.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_CONSTANT_MEMORY_DEPENDENCY

    Warp is blocked waiting for constant memory and immediate memory access to complete.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_PIPE_BUSY

    Compute operation cannot be performed due to the required resources not being available.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_MEMORY_THROTTLE

    Warp is blocked because there are too many pending memory operations.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_NOT_SELECTED

    Warp was ready to issue, but some other warp issued instead.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_OTHER

    Miscellaneous reasons.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_SLEEPING

    Sleeping.

  enumerator CUPTI_ACTIVITY_PC_SAMPLING_STALL_FORCE_INT

enum CUpti_ActivityPartitionedGlobalCacheConfig

  Partitioned global caching option.

  Values:

  enumerator CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_UNKNOWN

    Partitioned global cache config unknown.

  enumerator CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_NOT_SUPPORTED

    Partitioned global cache not supported.

  enumerator CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_OFF

    Partitioned global cache config off.

  enumerator CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_ON

    Partitioned global cache config on.

  enumerator CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_FORCE_INT

enum CUpti_ActivityPcieFieldIds

  Enum identifiers for fields in CUpti_ActivityPcie.

  Each enum value corresponds to a field in CUpti_ActivityPcie and describes the data type and purpose of that field.

  Values:

  enumerator PCIE_FIELD_KIND

    CUpti_ActivityKind kind; Kind of activity record: CUPTI_ACTIVITY_KIND_PCIE.

  enumerator PCIE_FIELD_TYPE

    CUpti_PcieDeviceType type; Type of device in topology, CUpti_PcieDeviceType.

  enumerator PCIE_FIELD_ID

    union id; A unique identifier for GPU or Bridge in Topology.

    CUdevice devId if type is CUPTI_PCIE_DEVICE_TYPE_GPU uint32_t bridgeId if type is CUPTI_PCIE_DEVICE_TYPE_BRIDGE

  enumerator PCIE_FIELD_DOMAIN

    uint32_t domain; Domain for the GPU or Bridge, required to identify which PCIE bus it belongs to in multiple NUMA systems.

  enumerator PCIE_FIELD_PCIE_GENERATION

    uint16_t pcieGeneration; PCIE Generation of GPU or Bridge.

  enumerator PCIE_FIELD_LINK_RATE

    uint16_t linkRate; Link rate of the GPU or bridge in gigatransfers per second (GT/s).

  enumerator PCIE_FIELD_LINK_WIDTH

    uint16_t linkWidth; Link width of the GPU or bridge.

  enumerator PCIE_FIELD_UPSTREAM_BUS

    uint16_t upstreamBus; Upstream bus ID for the GPU or PCI bridge.

    Required to identify which bus it is connected to in the topology.

  enumerator PCIE_FIELD_ATTR

    union attr; Attributes for more information about GPU (gpuAttr) or PCI Bridge (bridgeAttr).

    CUpti_ActivityPcieGpuAttr gpuAttr if type is CUPTI_PCIE_DEVICE_TYPE_GPU CUpti_ActivityPcieBridgeAttr bridgeAttr if type is CUPTI_PCIE_DEVICE_TYPE_BRIDGE The size of this field is determined by the largest structure among the possible types it can hold.

  enumerator PCIE_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityPreemptionKind

  The kind of a preemption activity.

  Values:

  enumerator CUPTI_ACTIVITY_PREEMPTION_KIND_UNKNOWN

    The preemption kind is not known.

  enumerator CUPTI_ACTIVITY_PREEMPTION_KIND_SAVE

    Preemption to save CDP block.

  enumerator CUPTI_ACTIVITY_PREEMPTION_KIND_RESTORE

    Preemption to restore CDP block.

  enumerator CUPTI_ACTIVITY_PREEMPTION_KIND_FORCE_INT

enum CUpti_ActivityStreamFieldIds

  Enum identifiers for fields to trace CUDA Stream operations.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_STREAM.

  Values:

  enumerator STREAM_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_STREAM.

  enumerator STREAM_FIELD_CONTEXT_ID

    uint32_t contextId; The ID of the context where the stream was created.

  enumerator STREAM_FIELD_STREAM_ID

    uint32_t streamId; A unique stream ID to identify the stream.

  enumerator STREAM_FIELD_PRIORITY

    int32_t priority; The clamped priority for the stream.

  enumerator STREAM_FIELD_FLAG

    CUpti_ActivityStreamFlag flag; Flags associated with the stream.

  enumerator STREAM_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this CUDA Stream operation.

  enumerator STREAM_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivityStreamFlag

  stream type.

  The types of stream to be used with CUpti_ActivityStream.

  Values:

  enumerator CUPTI_ACTIVITY_STREAM_CREATE_FLAG_UNKNOWN

    Unknown data.

  enumerator CUPTI_ACTIVITY_STREAM_CREATE_FLAG_DEFAULT

    Default stream.

  enumerator CUPTI_ACTIVITY_STREAM_CREATE_FLAG_NON_BLOCKING

    Non-blocking stream.

  enumerator CUPTI_ACTIVITY_STREAM_CREATE_FLAG_NULL

    Null stream.

  enumerator CUPTI_ACTIVITY_STREAM_CREATE_MASK

    Stream create Mask.

  enumerator CUPTI_ACTIVITY_STREAM_CREATE_FLAG_FORCE_INT

enum CUpti_ActivitySynchronizationFieldIds

  Enum identifiers for fields to trace various CUDA synchronization APIs.

  These field IDs are used to reference specific fields when dynamically selecting or parsing activity records of CUPTI_ACTIVITY_KIND_SYNCHRONIZATION.

  Values:

  enumerator SYNCHRONIZATION_FIELD_KIND

    CUpti_ActivityKind kind; Kind of this activity record.

    Always CUPTI_ACTIVITY_KIND_SYNCHRONIZATION.

  enumerator SYNCHRONIZATION_FIELD_TYPE

    CUpti_ActivitySynchronizationType type; The type of synchronization operation.

  enumerator SYNCHRONIZATION_FIELD_START

    uint64_t start; The start timestamp for the synchronization operation (in nanoseconds).

  enumerator SYNCHRONIZATION_FIELD_END

    uint64_t start; The start timestamp for the synchronization operation (in nanoseconds).

  enumerator SYNCHRONIZATION_FIELD_CORRELATION_ID

    uint64_t correlationId; Correlation ID assigned to this synchronization operation.

    Matches the correlation ID in the CUDA driver/runtime API activity record that launched it.

  enumerator SYNCHRONIZATION_FIELD_CONTEXT_ID

    uint32_t contextId; CUDA context where the operation is occurring.

  enumerator SYNCHRONIZATION_FIELD_STREAM_ID

    uint32_t streamId; The compute stream where the synchronization operation is occurring.

    CUPTI_SYNCHRONIZATION_INVALID_VALUE indicates that the field is not applicable for this record.

  enumerator SYNCHRONIZATION_FIELD_CUDA_EVENT_ID

    uint64_t cudaEventId; The CUDA event ID for which the synchronization operation is called.

    CUPTI_SYNCHRONIZATION_INVALID_VALUE indicates that the field is not applicable for this record.

  enumerator SYNCHRONIZATION_FIELD_CUDA_EVENT_SYNC_ID

    uint64_t cudaEventSyncId; A unique ID to associate event synchronization records with the latest CUDA Event record.

    Similar field is added in CUpti_ActivityCudaEventFieldIds to associate synchronization record to the CUDA Event record.

    The same CUDA event can be used multiple times, so the event id will not be unique to correlate the synchronization record with the latest CUDA Event record. This field will be unique and can be used to do the required correlation.

    A CUPTI_SYNCHRONIZATION_INVALID_VALUE value indicates that the field is not applicable for this record. Valid only for synchronization records related to CUDA Events.

  enumerator SYNCHRONIZATION_FIELD_RETURN_VALUE

    uint32_t returnValue; The return value for the synchronization operation.

    Use cuptiActivityEnableAllSyncRecords API to enable/disable collection of synchronization records with return value being non-zero. This will be a CUresult value.

  enumerator SYNCHRONIZATION_FIELD_MAX

    Total number of defined fields.

enum CUpti_ActivitySynchronizationType

  Synchronization type.

  The types of synchronization to be used with CUpti_ActivitySynchronization2.

  Values:

  enumerator CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_UNKNOWN

    Unknown data.

  enumerator CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_EVENT_SYNCHRONIZE

    Event synchronize API.

  enumerator CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_STREAM_WAIT_EVENT

    Stream wait event API.

  enumerator CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_STREAM_SYNCHRONIZE

    Stream synchronize API.

  enumerator CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_CONTEXT_SYNCHRONIZE

    Context synchronize API.

  enumerator CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_FORCE_INT

enum CUpti_ActivityThreadIdType

  Thread-Id types.

  CUPTI uses different methods to obtain the thread-id depending on the support and the underlying platform. This enum documents these methods for each type. APIs cuptiSetThreadIdType and cuptiGetThreadIdType can be used to set and get the thread-id type.

  Values:

  enumerator CUPTI_ACTIVITY_THREAD_ID_TYPE_DEFAULT

    Default type Windows uses API GetCurrentThreadId() Linux/Mac/Android/QNX use POSIX pthread API pthread_self()

  enumerator CUPTI_ACTIVITY_THREAD_ID_TYPE_SYSTEM

    This type is based on the system API available on the underlying platform and thread-id obtained is supposed to be unique for the process lifetime.

    Windows uses API GetCurrentThreadId() Linux uses syscall SYS_gettid Mac uses syscall SYS_thread_selfid Android/QNX use gettid()

  enumerator CUPTI_ACTIVITY_THREAD_ID_TYPE_SIZE

    Add new enums before this field.

  enumerator CUPTI_ACTIVITY_THREAD_ID_TYPE_FORCE_INT

enum CUpti_ActivityUnifiedMemoryAccessType

  Memory access type for unified memory page faults.

  This is valid for CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_GPU_PAGE_FAULT and CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_CPU_PAGE_FAULT_COUNT

  Values:

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_UNKNOWN

    The unified memory access type is not known.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_READ

    The page fault was triggered by read memory instruction.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_WRITE

    The page fault was triggered by write memory instruction.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_ATOMIC

    The page fault was triggered by atomic memory instruction.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_PREFETCH

    The page fault was triggered by memory prefetch operation.

enum CUpti_ActivityUnifiedMemoryCounterKind

  Kind of the Unified Memory counter.

  Many activities are associated with Unified Memory mechanism; among them are transfers from host to device, device to host, page fault at host side.

  Values:

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_UNKNOWN

    The unified memory counter kind is not known.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_HTOD

    Number of bytes transferred from host to device.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOH

    Number of bytes transferred from device to host.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_CPU_PAGE_FAULT_COUNT

    Number of CPU page faults, this is only supported on 64 bit Linux and Mac platforms.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_GPU_PAGE_FAULT

    Number of GPU page faults, this is only supported on devices with compute capability 6.0 and higher and 64 bit Linux platforms.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THRASHING

    Thrashing occurs when data is frequently accessed by multiple processors and has to be constantly migrated around to achieve data locality.

    In this case the overhead of migration may exceed the benefits of locality. This is only supported on 64 bit Linux platforms.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THROTTLING

    Throttling is a prevention technique used by the driver to avoid further thrashing.

    Here, the driver doesn’t service the fault for one of the contending processors for a specific period of time, so that the other processor can run at full-speed. This is only supported on 64 bit Linux platforms.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_REMOTE_MAP

    In case throttling does not help, the driver tries to pin the memory to a processor for a specific period of time.

    One of the contending processors will have slow access to the memory, while the other will have fast access. This is only supported on 64 bit Linux platforms.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOD

    Number of bytes transferred from one device to another device.

    This is only supported on 64 bit Linux platforms.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_COUNT
  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_FORCE_INT

enum CUpti_ActivityUnifiedMemoryCounterScope

  Scope of the unified memory counter (deprecated in CUDA 7.0)

  Values:

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_UNKNOWN

    The unified memory counter scope is not known.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_PROCESS_SINGLE_DEVICE

    Collect unified memory counter for single process on one device.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_PROCESS_ALL_DEVICES

    Collect unified memory counter for single process across all devices.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_COUNT
  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_FORCE_INT

enum CUpti_ActivityUnifiedMemoryMigrationCause

  Migration cause of the Unified Memory counter.

  This is valid for CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_HTOD and CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOH and CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOD

  Values:

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_UNKNOWN

    The unified memory migration cause is not known.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_USER

    The unified memory migrated due to an explicit call from the user e.g.

    cudaMemPrefetchAsync

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_COHERENCE

    The unified memory migrated to guarantee data coherence e.g.

    CPU/GPU faults on Pascal+ and kernel launch on pre-Pascal GPUs

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_PREFETCH

    The unified memory was speculatively migrated by the UVM driver before being accessed by the destination processor to improve performance.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_EVICTION

    The unified memory migrated to the CPU because it was evicted to make room for another block of memory on the GPU.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_ACCESS_COUNTERS

    The unified memory migrated to another processor because of access counter notifications.

    Only frequently accessed pages are migrated between CPU and GPU, or between peer GPUs.

enum CUpti_ActivityUnifiedMemoryRemoteMapCause

  Remote memory map cause of the Unified Memory counter.

  This is valid for CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_REMOTE_MAP

  Values:

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_UNKNOWN

    The cause of mapping to remote memory was unknown.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_COHERENCE

    Mapping to remote memory was added to maintain data coherence.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_THRASHING

    Mapping to remote memory was added to prevent further thrashing.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_POLICY

    Mapping to remote memory was added to enforce the hints specified by the programmer or by performance heuristics of the UVM driver.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_OUT_OF_MEMORY

    Mapping to remote memory was added because there is no more memory available on the processor and eviction was not possible.

  enumerator CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_EVICTION

    Mapping to remote memory was added after the memory was evicted to make room for another block of memory on the GPU.

enum CUpti_ActivityUvmCounterFieldIds

  Enum identifiers for fields in CUpti_ActivityUnifiedMemoryCounter3.

  Each enum value corresponds to a field in CUpti_ActivityUnifiedMemoryCounter3 and describes the data type and purpose of that field.

  Values:

  enumerator UVM_COUNTER_FIELD_KIND

    CUpti_ActivityKind kind; Kind of activity record: CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER.

  enumerator UVM_COUNTER_FIELD_COUNTER_KIND

    CUpti_ActivityUnifiedMemoryCounterKind counterKind; The Unified Memory counter kind.

  enumerator UVM_COUNTER_FIELD_VALUE

    uint64_t value; Value of the counter.

  enumerator UVM_COUNTER_FIELD_START

    uint64_t start; Start timestamp of the counter (in ns).

  enumerator UVM_COUNTER_FIELD_END

    uint64_t end; End timestamp of the counter (in ns).

  enumerator UVM_COUNTER_FIELD_ADDRESS

    uint64_t address; Virtual base address of the page/s being transferred.

  enumerator UVM_COUNTER_FIELD_SRC_ID

    uint32_t srcId; ID of the source CPU/device.

  enumerator UVM_COUNTER_FIELD_DST_ID

    uint32_t dstId; ID of the destination CPU/device.

  enumerator UVM_COUNTER_FIELD_STREAM_ID

    uint32_t streamId; ID of the stream causing the transfer.

  enumerator UVM_COUNTER_FIELD_PROCESS_ID

    uint32_t processId; ID of the process to which this record belongs.

  enumerator UVM_COUNTER_FIELD_FLAGS

    uint32_t flags; Flags associated with this record.

  enumerator UVM_COUNTER_FIELD_PROCESSORS

    uint64_t processors[5]; Bitmask of devices involved in the operation.

  enumerator UVM_COUNTER_FIELD_MAX

    Total number of defined fields.

enum CUpti_ChannelType

  Values:

  enumerator CUPTI_CHANNEL_TYPE_INVALID
  enumerator CUPTI_CHANNEL_TYPE_COMPUTE

    Channel is used for standard work launch and tracking.

  enumerator CUPTI_CHANNEL_TYPE_ASYNC_MEMCPY

    Channel is used by an asynchronous copy engine For confidential compute configurations, work launch and completion are done using the copy engines.

  enumerator CUPTI_CHANNEL_TYPE_DECOMP

    Channel is used for memory decompression operations.

  enumerator CUPTI_CHANNEL_TYPE_FORCE_INT

enum CUpti_ComputeEngineCtxSwitchOperationType

  The operation type of CUDA context switch event records.

  Values:

  enumerator CUPTI_COMPUTE_ENGINE_CTX_SWITCH_OPERATION_INVALID
  enumerator CUPTI_COMPUTE_ENGINE_CTX_SWITCH_OPERATION_START

    The start of the CUDA context switch operation.

  enumerator CUPTI_COMPUTE_ENGINE_CTX_SWITCH_OPERATION_END

    The end of the CUDA context switch operation.

  enumerator CUPTI_COMPUTE_ENGINE_CTX_SWITCH_OPERATION_COUNT

enum CUpti_ConfidentialComputeRotationEventType

  Values:

  enumerator CUPTI_CONFIDENTIAL_COMPUTE_INVALID_ROTATION_EVENT
  enumerator CUPTI_CONFIDENTIAL_COMPUTE_KEY_ROTATION_CHANNEL_BLOCKED

    This channel has been blocked from accepting new CUDA work so a key rotation can be done.

  enumerator CUPTI_CONFIDENTIAL_COMPUTE_KEY_ROTATION_CHANNEL_DRAINED

    This channel remains blocked and all queued CUDA work has completed.

    Other clients or channels may cause delays in starting the key rotation.

  enumerator CUPTI_CONFIDENTIAL_COMPUTE_KEY_ROTATION_CHANNEL_UNBLOCKED

    Key rotations have completed and this channel is unblocked.

  enumerator CUPTI_CONFIDENTIAL_COMPUTE_EVENT_TYPE_FORCE_INT

enum CUpti_ContextCigMode

  CIG (CUDA in Graphics) Modes.

  Describes the CIG modes associated with the CUDA context.

  Values:

  enumerator CUPTI_CONTEXT_CIG_MODE_NONE

    Regular (non-CIG) mode.

  enumerator CUPTI_CONTEXT_CIG_MODE_CIG

    CIG mode.

  enumerator CUPTI_CONTEXT_CIG_MODE_CIG_FALLBACK

    CIG fallback mode.

  enumerator CUPTI_CONTEXT_CIG_MODE_FORCE_INT

enum CUpti_DevType

  The device type for device connected to NVLink.

  Values:

  enumerator CUPTI_DEV_TYPE_INVALID
  enumerator CUPTI_DEV_TYPE_GPU

    The device type is GPU.

  enumerator CUPTI_DEV_TYPE_NPU

    The device type is NVLink processing unit in CPU.

  enumerator CUPTI_DEV_TYPE_FORCE_INT

enum CUpti_DeviceGraphLaunchMode

  The launch mode for device graph execution.

  Values:

  enumerator CUPTI_DEVICE_GRAPH_LAUNCH_MODE_INVALID
  enumerator CUPTI_DEVICE_GRAPH_LAUNCH_MODE_FIRE_AND_FORGET
  enumerator CUPTI_DEVICE_GRAPH_LAUNCH_MODE_TAIL
  enumerator CUPTI_DEVICE_GRAPH_LAUNCH_MODE_FIRE_AND_FORGET_AS_SIBLING

enum CUpti_DeviceVirtualizationMode

  This indicates the virtualization mode in which CUDA device is running.

  Values:

  enumerator CUPTI_DEVICE_VIRTUALIZATION_MODE_NONE

    No virtualization mode is associated with the device i.e.

    it’s a baremetal GPU

  enumerator CUPTI_DEVICE_VIRTUALIZATION_MODE_PASS_THROUGH

    The device is associated with the pass-through GPU.

    In this mode, an entire physical GPU is directly assigned to one virtual machine (VM).

  enumerator CUPTI_DEVICE_VIRTUALIZATION_MODE_VIRTUAL_GPU

    The device is associated with the virtual GPU (vGPU).

    In this mode multiple virtual machines (VMs) have simultaneous, direct access to a single physical GPU.

  enumerator CUPTI_DEVICE_VIRTUALIZATION_MODE_FORCE_INT

enum CUpti_EnvironmentClocksThrottleReason

  Reasons for clock throttling.

  The possible reasons that a clock can be throttled. There can be more than one reason that a clock is being throttled so these types can be combined by bitwise OR. These are used in the clocksThrottleReason field in the Environment Activity Record.

  Values:

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_GPU_IDLE

    Nothing is running on the GPU and the clocks are dropping to idle state.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_USER_DEFINED_CLOCKS

    The GPU clocks are limited by a user specified limit.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_SW_POWER_CAP

    A software power scaling algorithm is reducing the clocks below requested clocks.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_HW_SLOWDOWN

    Hardware slowdown to reduce the clock by a factor of two or more is engaged.

    This is an indicator of one of the following: 1) Temperature is too high, 2) External power brake assertion is being triggered (e.g. by the system power supply), 3) Change in power state.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_UNKNOWN

    Some unspecified factor is reducing the clocks.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_UNSUPPORTED

    Throttle reason is not supported for this GPU.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_NONE

    No clock throttling.

  enumerator CUPTI_CLOCKS_THROTTLE_REASON_FORCE_INT

enum CUpti_ExternalCorrelationKind

  The kind of external APIs supported for correlation.

  Custom correlation kinds are reserved for usage in external tools.

  See also

  CUpti_ActivityExternalCorrelation

  Values:

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_INVALID
  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_UNKNOWN

    The external API is unknown to CUPTI.

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_OPENACC

    The external API is OpenACC.

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_CUSTOM0

    The external API is custom0.

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_CUSTOM1

    The external API is custom1.

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_CUSTOM2

    The external API is custom2.

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_SIZE

    Add new kinds before this line.

  enumerator CUPTI_EXTERNAL_CORRELATION_KIND_FORCE_INT

enum CUpti_FuncExecutionModel

  The execution model of a kernel function.

  This should be used to set executionModel field in kernel records.

  Values:

  enumerator CUPTI_FUNC_EXECUTION_MODEL_UNKNOWN
  enumerator CUPTI_FUNC_EXECUTION_MODEL_SIMT
  enumerator CUPTI_FUNC_EXECUTION_MODEL_TILE
  enumerator CUPTI_FUNC_EXECUTION_MODEL_SIZE
  enumerator CUPTI_FUNC_EXECUTION_MODEL_FORCE_INT

enum CUpti_FuncShmemLimitConfig

  The shared memory limit per block config for a kernel This should be used to set ‘cudaOccFuncShmemConfig’ field in occupancy calculator API.

  Values:

  enumerator CUPTI_FUNC_SHMEM_LIMIT_DEFAULT

    The shared memory limit config is default.

  enumerator CUPTI_FUNC_SHMEM_LIMIT_OPTIN

    User has opted for a higher dynamic shared memory limit using function attribute ‘cudaFuncAttributeMaxDynamicSharedMemorySize’ for runtime API or CU_FUNC_ATTRIBUTE_MAX_DYNAMIC_SHARED_SIZE_BYTES for driver API.

  enumerator CUPTI_FUNC_SHMEM_LIMIT_FORCE_INT

enum CUpti_LinkFlag

  Link flags.

  Describes link properties, to be used with CUpti_ActivityNvLink.

  Values:

  enumerator CUPTI_LINK_FLAG_INVALID

    The flag is invalid.

  enumerator CUPTI_LINK_FLAG_PEER_ACCESS

    Is peer to peer access supported by this link.

  enumerator CUPTI_LINK_FLAG_SYSMEM_ACCESS

    Is system memory access supported by this link.

  enumerator CUPTI_LINK_FLAG_PEER_ATOMICS

    Is peer atomic access supported by this link.

  enumerator CUPTI_LINK_FLAG_SYSMEM_ATOMICS

    Is system memory atomic access supported by this link.

  enumerator CUPTI_LINK_FLAG_FORCE_INT

enum CUpti_NvtxExtPayloadType

  Values:

  enumerator CUPTI_NVTX_EXT_PAYLOAD_TYPE_UNKNOWN

    The payload type is not known.

  enumerator CUPTI_NVTX_EXT_PAYLOAD_TYPE_SCHEMA

    The payload type is a schema.

  enumerator CUPTI_NVTX_EXT_PAYLOAD_TYPE_ENUM

    The payload type is an enum.

  enumerator CUPTI_NVTX_EXT_PAYLOAD_TYPE_FORCE_INT

enum CUpti_OpenAccConstructKind

  The OpenAcc parent construct kind for OpenAcc activity records.

  Values:

  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_UNKNOWN
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_PARALLEL
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_KERNELS
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_LOOP
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_DATA
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_ENTER_DATA
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_EXIT_DATA
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_HOST_DATA
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_ATOMIC
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_DECLARE
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_INIT
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_SHUTDOWN
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_SET
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_UPDATE
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_ROUTINE
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_WAIT
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_RUNTIME_API
  enumerator CUPTI_OPENACC_CONSTRUCT_KIND_FORCE_INT

enum CUpti_OpenAccEventKind

  The OpenAcc event kind for OpenAcc activity records.

  See also

  CUpti_ActivityKindOpenAcc

  Values:

  enumerator CUPTI_OPENACC_EVENT_KIND_INVALID
  enumerator CUPTI_OPENACC_EVENT_KIND_DEVICE_INIT
  enumerator CUPTI_OPENACC_EVENT_KIND_DEVICE_SHUTDOWN
  enumerator CUPTI_OPENACC_EVENT_KIND_RUNTIME_SHUTDOWN
  enumerator CUPTI_OPENACC_EVENT_KIND_ENQUEUE_LAUNCH
  enumerator CUPTI_OPENACC_EVENT_KIND_ENQUEUE_UPLOAD
  enumerator CUPTI_OPENACC_EVENT_KIND_ENQUEUE_DOWNLOAD
  enumerator CUPTI_OPENACC_EVENT_KIND_WAIT
  enumerator CUPTI_OPENACC_EVENT_KIND_IMPLICIT_WAIT
  enumerator CUPTI_OPENACC_EVENT_KIND_COMPUTE_CONSTRUCT
  enumerator CUPTI_OPENACC_EVENT_KIND_UPDATE
  enumerator CUPTI_OPENACC_EVENT_KIND_ENTER_DATA
  enumerator CUPTI_OPENACC_EVENT_KIND_EXIT_DATA
  enumerator CUPTI_OPENACC_EVENT_KIND_CREATE
  enumerator CUPTI_OPENACC_EVENT_KIND_DELETE
  enumerator CUPTI_OPENACC_EVENT_KIND_ALLOC
  enumerator CUPTI_OPENACC_EVENT_KIND_FREE
  enumerator CUPTI_OPENACC_EVENT_KIND_FORCE_INT

enum CUpti_OpenMpEventKind

  Values:

  enumerator CUPTI_OPENMP_EVENT_KIND_INVALID
  enumerator CUPTI_OPENMP_EVENT_KIND_PARALLEL
  enumerator CUPTI_OPENMP_EVENT_KIND_TASK
  enumerator CUPTI_OPENMP_EVENT_KIND_THREAD
  enumerator CUPTI_OPENMP_EVENT_KIND_IDLE
  enumerator CUPTI_OPENMP_EVENT_KIND_WAIT_BARRIER
  enumerator CUPTI_OPENMP_EVENT_KIND_WAIT_TASKWAIT
  enumerator CUPTI_OPENMP_EVENT_KIND_FORCE_INT

enum CUpti_PcieDeviceType

  Field to differentiate whether PCIE Activity record is of a GPU or a PCI Bridge.

  Values:

  enumerator CUPTI_PCIE_DEVICE_TYPE_GPU

    PCIE GPU record.

  enumerator CUPTI_PCIE_DEVICE_TYPE_BRIDGE

    PCIE Bridge record.

  enumerator CUPTI_PCIE_DEVICE_TYPE_FORCE_INT

enum CUpti_PcieGen

  PCIE Generation.

  Enumeration of PCIE Generation for pcie activity attribute pcieGeneration

  Values:

  enumerator CUPTI_PCIE_GEN_GEN1

    PCIE Generation 1.

  enumerator CUPTI_PCIE_GEN_GEN2

    PCIE Generation 2.

  enumerator CUPTI_PCIE_GEN_GEN3

    PCIE Generation 3.

  enumerator CUPTI_PCIE_GEN_GEN4

    PCIE Generation 4.

  enumerator CUPTI_PCIE_GEN_GEN5

    PCIE Generation 5.

  enumerator CUPTI_PCIE_GEN_GEN6

    PCIE Generation 6.

  enumerator CUPTI_PCIE_GEN_FORCE_INT

## 6.1.8. Functions

CUptiResult cuptiActivityConfigurePCSampling(

  CUcontext ctx,
  CUpti_ActivityPCSamplingConfig *config,

)

  Set PC sampling configuration.

  For Pascal and older GPU architectures this API must be called before enabling activity kind CUPTI_ACTIVITY_KIND_PC_SAMPLING. There is no such requirement for Volta and newer GPU architectures.

  For Volta and newer GPU architectures if this API is called in the middle of execution, PC sampling configuration will be updated for subsequent kernel launches.

  Starting with CUDA 13.0, this function is unsupported and should not be used. It always returns the error code CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED.

  Parameters:

    - ctx – The context

    - config – A pointer to CUpti_ActivityPCSamplingConfig structure containing PC sampling configuration.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_OPERATION – if this api is called while some valid event collection method is set.

    - CUPTI_ERROR_INVALID_PARAMETER – if `config` is NULL or any parameter in the `config` structures is not a valid value

    - CUPTI_ERROR_NOT_SUPPORTED – Indicates that the system/device does not support the unified memory counters

CUptiResult cuptiActivityConfigureUnifiedMemoryCounter(

  CUpti_ActivityUnifiedMemoryCounterConfig *config,
  uint32_t count,

)

  Set Unified Memory Counter configuration.

  Set the configuration before enabling the corresponding activity kind CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER. The API should be called after CUDA driver initialization.

  Parameters:

    - config – A pointer to CUpti_ActivityUnifiedMemoryCounterConfig structures containing Unified Memory counter configuration.

    - count – Number of Unified Memory counter configuration structures

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `config` is NULL or any parameter in the `config` structures is not a valid value

    - CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED – One potential reason is that platform (OS/arch) does not support the unified memory counters

    - CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_ON_DEVICE – Indicates that the device does not support the unified memory counters

    - CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_ON_NON_P2P_DEVICES – Indicates that multi-GPU configuration without P2P support between any pair of devices does not support the unified memory counters

CUptiResult cuptiActivityDisable(CUpti_ActivityKind kind)

  Disable collection of a specific kind of activity record.

  Disable collection of a specific kind of activity record. Multiple kinds can be disabled by calling this function multiple times. By default all activity kinds are disabled for collection.

  Parameters:

    kind – The kind of activity record to stop collecting

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityDisableContext(

  CUcontext context,
  CUpti_ActivityKind kind,

)

  Disable collection of a specific kind of activity record for a context.

  Disable collection of a specific kind of activity record for a context. This setting done by this API will supersede the global settings for activity records. Multiple kinds can be enabled by calling this function multiple times.

  Parameters:

    - context – The context for which activity is to be disabled

    - kind – The kind of activity record to stop collecting

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityDisable_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ActivityKind kind,
  CUpti_ActivityConfig *pActivityConfig,

)

  Disable collection of a specific kind of activity record for the subscriber.

  Disable collection of a specific kind of activity record. Multiple kinds can be disabled by calling this function multiple times. By default all activity kinds are disabled for collection.

  Parameters:

    - subscriber – The subscriber handle.

    - kind – The kind of activity record to stop collecting

    - pActivityConfig – The activity config. It can be NULL.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityEnable(CUpti_ActivityKind kind)

  Enable collection of a specific kind of activity record.

  Enable collection of a specific kind of activity record. Multiple kinds can be enabled by calling this function multiple times. By default all activity kinds are disabled for collection.

  Parameters:

    kind – The kind of activity record to collect

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_NOT_COMPATIBLE – if the activity kind cannot be enabled

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityEnableAllSyncRecords(uint8_t enable)

  Enables collecting records for all synchronization operations.

  CUPTI provides CUDA event query and stream query records via CUPTI_ACTIVITY_KIND_SYNCHRONIZATION. Using this API, CUPTI client can disable to record CUDA event query and stream query records for queries for which the operations have not yet been completed on the CUDA event/stream.

  By default, the record is generated for all CUDA events and stream irrespective of whether the operations have been completed on the CUDA event/stream.

  Parameters:

    enable – is a boolean, denoting whether to enable or disable the collection of all CUDA event query and stream query records

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityEnableAndDump(CUpti_ActivityKind kind)

  Enable collection of a specific kind of activity record.

  For certain activity kinds it dumps existing records.

  In general, the behavior of this API is similar to the API cuptiActivityEnable i.e. it enables the collection of a specific kind of activity record. Additionally, this API can help in dumping the records for activities which happened in the past before enabling the corresponding activity kind. The API allows to get records for the current resource allocations done in CUDA For CUPTI_ACTIVITY_KIND_DEVICE, existing device records are dumped For CUPTI_ACTIVITY_KIND_CONTEXT, existing context records are dumped For CUPTI_ACTIVITY_KIND_STREAM, existing stream records are dumped For CUPTI_ACTIVITY_KIND_ NVLINK, existing NVLINK records are dumped For CUPTI_ACTIVITY_KIND_PCIE, existing PCIE records are dumped For other activities, the behavior is similar to the API cuptiActivityEnable

  Device records are emitted in CUPTI on CUDA driver initialization. Those records can only be retrieved by the user if CUPTI is attached before CUDA initialization. Context and stream records are emitted on context and stream creation. The use case of the API is to provide the records for CUDA resources (contexts/streams/devices) that are currently active if user late attaches CUPTI.

  Before calling this function, the user must register buffer callbacks to get the activity records by calling cuptiActivityRegisterCallbacks. If the user does not register the buffers and calls API cuptiActivityEnableAndDump, then CUPTI will enable the activity kind but not provide any records for that activity kind.

  Parameters:

    kind – The kind of activity record to collect

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_UNKNOWN – if buffer is not initialized.

    - CUPTI_ERROR_NOT_COMPATIBLE – if the activity kind cannot be enabled

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityEnableAndDump_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ActivityKind kind,
  CUpti_ActivityConfig *activityConfig,

)

  Enable collection of a specific kind of activity record.

  For certain activity kinds it dumps existing records.

  In general, the behavior of this API is similar to the API cuptiActivityEnable_v2 i.e. it enables the collection of a specific kind of activity record. Additionally, this API can help in dumping the records for activities which happened in the past before enabling the corresponding activity kind. The API allows to get records for the current resource allocations done in CUDA For CUPTI_ACTIVITY_KIND_DEVICE, existing device records are dumped For CUPTI_ACTIVITY_KIND_CONTEXT, existing context records are dumped For CUPTI_ACTIVITY_KIND_STREAM, existing stream records are dumped For CUPTI_ACTIVITY_KIND_ NVLINK, existing NVLINK records are dumped For CUPTI_ACTIVITY_KIND_PCIE, existing PCIE records are dumped For other activities, the behavior is similar to the API cuptiActivityEnable

  Device records are emitted in CUPTI on CUDA driver initialization. Those records can only be retrieved by the user if CUPTI is attached before CUDA initialization. Context and stream records are emitted on context and stream creation. The use case of the API is to provide the records for CUDA resources (contexts/streams/devices) that are currently active if user late attaches CUPTI.

  Before calling this function, the user must register buffer callbacks to get the activity records by calling cuptiActivityRegisterCallbacks_v2. If the user does not register the buffers and calls API cuptiActivityEnableAndDump_v2, then CUPTI will enable the activity kind but not provide any records for that activity kind.

  Parameters:

    - subscriber – The subscriber handle.

    - kind – The kind of activity record to collect

    - activityConfig – The activity config. It can be NULL.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_UNKNOWN – if buffer is not initialized.

    - CUPTI_ERROR_NOT_COMPATIBLE – if the activity kind cannot be enabled

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityEnableContext(

  CUcontext context,
  CUpti_ActivityKind kind,

)

  Enable collection of a specific kind of activity record for a context.

  Enable collection of a specific kind of activity record for a context. This setting done by this API will supersede the global settings for activity records enabled by cuptiActivityEnable. Multiple kinds can be enabled by calling this function multiple times.

  Parameters:

    - context – The context for which activity is to be enabled

    - kind – The kind of activity record to collect

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_NOT_COMPATIBLE – if the activity kind cannot be enabled

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityEnableCudaEventDeviceTimestamps(

  uint8_t enable,

)

  Enable/Disable collecting device timestamp for CUPTI_ACTIVITY_KIND_CUDA_EVENT record.

  CUPTI provides device timestamps via ‘deviceTimestamp’ field in CUPTI_ACTIVITY_KIND_CUDA_EVENT records. Using this API, CUPTI client can enable or disable the collection of CUDA event device timestamps. By default, the collection of CUDA event device timestamps is disabled.

  Parameters:

    enable – is a boolean, denoting whether to enable or disable the collection of CUDA event device timestamps

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityEnableDeviceGraph(uint8_t enable)

  Controls the collection of records for device launched graphs.

  This API is used to control the collection of records for device launched graphs. Default value is 0, i.e. these records are not collected. This API needs to be called before initialization of CUDA and this setting should not be changed during the profiling session.

  Parameters:

    enable – is a boolean, denoting whether these records should be collected

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityEnableDriverApi(

  CUpti_CallbackId cbid,
  uint8_t enable,

)

  Controls the collection of activity records for specific CUDA Driver APIs.

  Activity kind CUPTI_ACTIVITY_KIND_DRIVER controls the collection of either all CUDA Driver APIs or none. API cuptiActivityEnableDriverApi can be used for fine-grained control, it allows enabling/disabling tracing of a specific set of CUDA Driver APIs. To disable collection of a small set of CUDA Driver APIs, user can first enable the collection of all Driver APIs using the activity kind CUPTI_ACTIVITY_KIND_DRIVER and call this API to disable specific Driver APIs. And to enable the collection of a small set of CUDA Driver APIs, user can call this API without using the activity kind CUPTI_ACTIVITY_KIND_DRIVER.

  Note: Activity kind CUPTI_ACTIVITY_KIND_DRIVER overrides the settings done by this API if it is called after the API.

  Parameters:

    - cbid – callback id of the CUDA Driver API. This can be found in the header cupti_driver_cbid.h.

    - enable – is a boolean, denoting whether to enable or disable the collection

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityEnableDriverApi_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_CallbackId cbid,
  uint8_t enable,

)

  Controls the collection of activity records for specific CUDA Driver APIs for a given subscriber.

  This is the per-subscriber version of cuptiActivityEnableDriverApi. It allows each subscriber to independently enable or disable tracing of specific CUDA Driver APIs.

  Parameters:

    - subscriber – Handle to the subscriber. Must have been previously created via cuptiSubscribe_v2.

    - cbid – callback id of the CUDA Driver API.

    - enable – is a boolean, denoting whether to enable or disable the collection

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if the subscriber handle is invalid or cbid is out of range

CUptiResult cuptiActivityEnableHWTrace(uint8_t enable)

  Enables CUDA kernel timestamp collection via Hardware Event System (HES).

  This API enables hardware-based collection of CUDA kernel timestamps as an alternative to the traditional software instrumentation and semaphore-based approach. HES-based collection provides lower overhead and more accurate timing measurements.

  This API must be called after CUDA driver initialization but before creating the CUDA context. As a generic solution, this API can be called from the CUPTI_CBID_RESOURCE_CU_INIT_FINISHED callback. Once enabled, HES-based tracing persists for the entire profiling session and cannot be disabled.

  This API can also be called before CUDA driver initialization. After driver initialization, CUPTI may switch to traditional semaphore-based tracing and return error through callback with domain CUPTI_CB_DOMAIN_STATE if HES-based tracing cannot be supported.

  Note

  This feature is only available on NVIDIA Blackwell architecture and later.

  Parameters:

    enable – is a boolean flag to enable (true) HES-based timestamp collection.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_SUPPORTED – if HW trace cannot be enabled on the current platform

    - CUPTI_ERROR_VIRTUALIZED_DEVICE_NOT_SUPPORTED –

    - CUPTI_ERROR_CONFIDENTIAL_COMPUTING_NOT_SUPPORTED –

    - CUPTI_ERROR_CMP_DEVICE_NOT_SUPPORTED –

    - CUPTI_ERROR_MIG_DEVICE_NOT_SUPPORTED –

    - CUPTI_ERROR_SLI_DEVICE_NOT_SUPPORTED –

    - CUPTI_ERROR_WSL_DEVICE_NOT_SUPPORTED –

    - CUPTI_ERROR_HES_TRACE_NOT_SUPPORTED_ON_MPS –

CUptiResult cuptiActivityEnableLatencyTimestamps(uint8_t enable)

  Controls the collection of queued and submitted timestamps for kernels.

  This API is used to control the collection of queued and submitted timestamps for kernels whose records are provided through the struct CUpti_ActivityKernel12. Default value is 0, i.e. these timestamps are not collected. This API needs to be called before initialization of CUDA and this setting should not be changed during the profiling session.

  This API is not supported if the HW trace is enabled through the API cuptiActivityEnableHWTrace.

  Parameters:

    enable – is a boolean, denoting whether these timestamps should be collected

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityEnableLaunchAttributes(uint8_t enable)

  Controls the collection of launch attributes for kernels.

  This API is used to control the collection of launch attributes for kernels whose records are provided through the struct CUpti_ActivityKernel12. Default value is 0, i.e. these attributes are not collected.

  Parameters:

    enable – is a boolean denoting whether these launch attributes should be collected

CUptiResult cuptiActivityEnableRuntimeApi(

  CUpti_CallbackId cbid,
  uint8_t enable,

)

  Controls the collection of activity records for specific CUDA Runtime APIs.

  Activity kind CUPTI_ACTIVITY_KIND_RUNTIME controls the collection of either all CUDA Runtime APIs or none. API cuptiActivityEnableRuntimeApi can be used for fine-grained control, it allows enabling/disabling tracing of a specific set of CUDA Runtime APIs. To disable collection of a small set of CUDA Runtime APIs, user can first enable the collection of all Runtime APIs using the activity kind CUPTI_ACTIVITY_KIND_RUNTIME and call this API to disable specific Runtime APIs. And to enable the collection of a small set of CUDA Runtime APIs, user can call this API without using the activity kind CUPTI_ACTIVITY_KIND_RUNTIME.

  Note: Activity kind CUPTI_ACTIVITY_KIND_RUNTIME overrides the settings done by this API if it is called after the API.

  Parameters:

    - cbid – callback id of the CUDA Runtime API. This can be found in the header cupti_runtime_cbid.h.

    - enable – is a boolean, denoting whether to enable or disable the collection

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityEnableRuntimeApi_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_CallbackId cbid,
  uint8_t enable,

)

  Controls the collection of activity records for specific CUDA Runtime APIs for a given subscriber.

  This is the per-subscriber version of cuptiActivityEnableRuntimeApi. It allows each subscriber to independently enable or disable tracing of specific CUDA Runtime APIs.

  Parameters:

    - subscriber – Handle to the subscriber. Must have been previously created via cuptiSubscribe_v2.

    - cbid – callback id of the CUDA Runtime API.

    - enable – is a boolean, denoting whether to enable or disable the collection

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if the subscriber handle is invalid or cbid is out of range

CUptiResult cuptiActivityEnable_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ActivityKind kind,
  CUpti_ActivityConfig *pActivityConfig,

)

  Enable collection of a specific kind of activity record for the subscriber.

  Enable collection of a specific kind of activity record. Multiple kinds can be enabled by calling this function multiple times. By default all activity kinds are disabled for collection.

  Parameters:

    - subscriber – The subscriber handle.

    - kind – The kind of activity record to collect

    - pActivityConfig – The activity config. It can be NULL.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_NOT_COMPATIBLE – if the activity kind cannot be enabled

    - CUPTI_ERROR_INVALID_KIND – if the activity kind is not supported

CUptiResult cuptiActivityFlush(

  CUcontext context,
  uint32_t streamId,
  uint32_t flag,

)

  Wait for all activity records to be delivered via the completion callback.

  This function does not return until all activity records associated with the specified context/stream are returned to the CUPTI client using the callback registered in cuptiActivityRegisterCallbacks. To ensure that all activity records are complete, the requested stream(s), if any, are synchronized.

  If `context` is NULL, the global activity records (i.e. those not associated with a particular stream) are flushed (in this case no streams are synchronized). If `context` is a valid CUcontext and `streamId` is 0, the buffers of all streams of this context are flushed. Otherwise, the buffers of the specified stream in this context is flushed.

  Before calling this function, the buffer handling callback api must be activated by calling cuptiActivityRegisterCallbacks.

  DEPRECATED This method is deprecated CONTEXT and STREAMID will be ignored. Use cuptiActivityFlushAll to flush all data.

  Parameters:

    - context – A valid CUcontext or NULL.

    - streamId – The stream ID.

    - flag – The flag can be set to indicate a forced flush. See CUpti_ActivityFlag

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_CUPTI_ERROR_INVALID_OPERATION – if not preceded by a successful call to cuptiActivityRegisterCallbacks

    - CUPTI_ERROR_UNKNOWN – an internal error occurred

CUptiResult cuptiActivityFlushAll(uint32_t flag)

  Request to deliver activity records via the buffer completion callback.

  This function returns the activity records associated with all contexts/streams (and the global buffers not associated with any stream) to the CUPTI client using the callback registered in cuptiActivityRegisterCallbacks.

  This is a blocking call but it doesn’t issue any CUDA synchronization calls implicitly thus it’s not guaranteed that all activities are completed on the underlying devices. Activity record is considered as completed if it has all the information filled up including the timestamps if any. It is the client’s responsibility to issue necessary CUDA synchronization calls before calling this function if all activity records with complete information are expected to be delivered.

  Behavior of the function based on the input flag: (-) ::For default flush i.e. when flag is set as 0, it returns all the activity buffers which have all the activity records completed, buffers need not to be full though. It doesn’t return buffers which have one or more incomplete records. Default flush can be done at a regular interval in a separate thread. (-) ::For forced flush i.e. when flag CUPTI_ACTIVITY_FLAG_FLUSH_FORCED is passed to the function, it returns all the activity buffers including the ones which have one or more incomplete activity records. It’s suggested for clients to do the force flush before the termination of the profiling session to allow remaining buffers to be delivered. In general, it can be done in the at-exit handler.

  Before calling this function, the buffer handling callback api must be activated by calling cuptiActivityRegisterCallbacks.

  When multiple subscribers are allowed, the buffers of all subscribers are flushed with the same flag. It is not possible to flush the buffers of only a specific subscriber.

  See also

  cuptiActivityFlushPeriod

  Parameters:

    flag – The flag can be set to indicate a forced flush. See CUpti_ActivityFlag

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_OPERATION – if not preceded by a successful call to cuptiActivityRegisterCallbacks

    - CUPTI_ERROR_UNKNOWN – an internal error occurred

CUptiResult cuptiActivityFlushPeriod(uint32_t time)

  Sets the flush period for the worker thread.

  CUPTI creates a worker thread to minimize the perturbance for the application created threads. CUPTI offloads certain operations from the application threads to the worker thread, this includes synchronization of profiling resources between host and device, delivery of the activity buffers to the client using the callback registered in cuptiActivityRegisterCallbacks. For performance reasons, CUPTI wakes up the worker thread based on certain heuristics.

  This API is used to control the flush period of the worker thread. This setting will override the CUPTI heuristics. Setting time to zero disables the periodic flush and restores the default behavior.

  Periodic flush can return only those activity buffers which are full and have all the activity records completed.

  It’s allowed to use the API cuptiActivityFlushAll to flush the data on-demand, even when client sets the periodic flush.

  See also

  cuptiActivityFlushAll

  Parameters:

    time – flush period in milliseconds (ms)

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivityGetAttribute(

  CUpti_ActivityAttribute attr,
  size_t *valueSize,
  void *value,

)

  Read an activity API attribute.

  Read an activity API attribute and return it in `*value`. In case of multiple subscribers, use cuptiActivityGetAttribute_v2 to read the attribute for the subscriber.

  Parameters:

    - attr – The attribute to read

    - valueSize – Size of buffer pointed by the value, and returns the number of bytes written to `value`

    - value – Returns the value of the attribute

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `valueSize` or `value` is NULL, or if `attr` is not an activity attribute

    - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT – Indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiActivityGetAttribute_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ActivityAttribute attr,
  size_t *valueSize,
  void *value,

)

  Read an activity API attribute.

  This function is similar to cuptiActivityGetAttribute. Note that in case of multiple subscribers, only cuptiActivityGetAttribute_v2 can be used to read the attribute for the subscriber.

  Read an activity API attribute and return it in `*value`.

  Parameters:

    - subscriber – The subscriber handle.

    - attr – The attribute to read

    - valueSize – Size of buffer pointed by the value, and returns the number of bytes written to `value`

    - value – Returns the value of the attribute

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `valueSize` or `value` is NULL, or if `attr` is not an activity attribute

    - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT – Indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiActivityGetEnabledKinds(

  CUpti_SubscriberHandle subscriber,
  CUpti_ActivityKind *buffer,
  uint32_t *bufferSize,
  uint32_t *enabledKindsCount,

)

  Get the enabled activity kinds for a subscriber.

  Note

  If the provided buffer size is not sufficient to store all the enabled activity kinds, we populate the buffer with as much as we can, but return the true value of the number of enabled activity kinds in `enabledKindsCount`.

  Parameters:

    - subscriber – The subscriber handle. If NULL, the union of activity kinds enabled across all subscribers is returned.

    - buffer – The buffer to store the enabled activity kinds. If NULL, the number of enabled activity kinds is returned in `enabledKindsCount`.

    - bufferSize – The size of the buffer. If NULL, only the number of enabled activity kinds is returned in `enabledKindsCount`. If NULL and `buffer` is not NULL, CUPTI_ERROR_INVALID_PARAMETER is returned.

    - enabledKindsCount – The number of enabled activity kinds. If NULL, CUPTI_ERROR_INVALID_PARAMETER is returned.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `enabledKindsCount` is NULL or if `subscriber` is invalid.

CUptiResult cuptiActivityGetNextRecord(

  uint8_t *buffer,
  size_t validBufferSizeBytes,
  CUpti_Activity **record,

)

  Iterate over the activity records in a buffer.

  This is a helper function to iterate over the activity records in a buffer. A buffer of activity records is typically obtained by receiving a CUpti_BuffersCallbackCompleteFunc callback. Stop iterating the buffer when an error occurs.

  An example of typical usage:

      CUpti_Activity *record = NULL;
      CUptiResult status = CUPTI_SUCCESS;
        do {
           status = cuptiActivityGetNextRecord(buffer, validSize, &record);
           if(status == CUPTI_SUCCESS) {
                // Use record here...
           }
           else if (status == CUPTI_ERROR_MAX_LIMIT_REACHED)
               break;
           else if (status == CUPTI_ERROR_INVALID_KIND)
               break;
           else {
               goto Error;
           }
         } while (1);

  Parameters:

    - buffer – The buffer containing activity records

    - record – Inputs the previous record returned by cuptiActivityGetNextRecord and returns the next activity record from the buffer. If input value is NULL, returns the first activity record in the buffer. Records of certain kinds like CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL may contain invalid (0) timestamps, indicating that no timing information could be collected for lack of device memory.

    - validBufferSizeBytes – The number of valid bytes in the buffer.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_MAX_LIMIT_REACHED – if no more records in the buffer

    - CUPTI_ERROR_INVALID_PARAMETER – if `buffer` is NULL.

    - CUPTI_ERROR_INVALID_KIND – if activity record is either incomplete or invalid

CUptiResult cuptiActivityGetNextRecord_v2(

  CUpti_SubscriberHandle subscriber,
  uint8_t *buffer,
  size_t validBufferSizeBytes,
  CUpti_Activity **record,

)

  Iterate over the activity records in the supplied buffer.

  This function is similar to cuptiActivityGetNextRecord and accepts a subscriber handle. It should be used instead of cuptiActivityGetNextRecord when using subscriber-aware V2 APIs.

  An example of typical usage:

      CUpti_Activity *record = NULL;
      CUptiResult status = CUPTI_SUCCESS;
        do {
           status = cuptiActivityGetNextRecord_v2(subscriber, buffer, validSize, &record);
           if(status == CUPTI_SUCCESS) {
                // Use record here...
           }
           else if (status == CUPTI_ERROR_MAX_LIMIT_REACHED)
               break;
           else if (status == CUPTI_ERROR_INVALID_KIND)
               break;
           else {
               goto Error;
           }
         } while (1);

  Parameters:

    - subscriber – Handle to the subscriber whose record layout should be used.

    - buffer – The buffer containing activity records

    - validBufferSizeBytes – The number of valid bytes in the buffer.

    - record – Inputs the previous record returned by cuptiActivityGetNextRecord_v2 and returns the next activity record from the buffer. If input value is NULL, returns the first activity record in the buffer.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_MAX_LIMIT_REACHED – if no more records in the buffer

    - CUPTI_ERROR_INVALID_PARAMETER – if `subscriber`, `buffer` or `record` is NULL.

    - CUPTI_ERROR_INVALID_KIND – if activity record is either incomplete or invalid

CUptiResult cuptiActivityGetNumDroppedRecords(

  CUcontext context,
  uint32_t streamId,
  size_t *dropped,

)

  Get the number of activity records that were dropped of insufficient buffer space.

  Get the number of records that were dropped because of insufficient buffer space. The dropped count includes records that could not be recorded because CUPTI did not have activity buffer space available for the record (because the CUpti_BuffersCallbackRequestFunc callback did not return an empty buffer of sufficient size) and also CDP records that could not be record because the device-size buffer was full (size is controlled by the CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE_CDP attribute). The dropped count maintained for the queue is reset to zero when this function is called.

  Parameters:

    - context – The context, or NULL to get dropped count from global queue

    - streamId – The stream ID

    - dropped – The number of records that were dropped since the last call to this function.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `dropped` is NULL

CUptiResult cuptiActivityGetNumDroppedRecords_v2(

  CUpti_SubscriberHandle subscriber,
  CUcontext context,
  uint32_t streamId,
  size_t *dropped,

)

  Get the number of dropped activity records for a specific subscriber.

  This is the per-subscriber version of cuptiActivityGetNumDroppedRecords.

  Note

  This API resets the subscriber’s dropped record count to 0 after reading.

  Parameters:

    - subscriber – The subscriber handle

    - context – CUDA context (reserved for future use)

    - streamId – Stream ID (reserved for future use)

    - dropped – Returns the number of dropped records

  Return values:

    - CUPTI_SUCCESS – on success

    - CUPTI_ERROR_INVALID_PARAMETER – if `subscriber` or `dropped` is NULL

CUptiResult cuptiActivityGetStructSize(

  CUpti_ActivityKind activityKind,
  uint32_t version,
  size_t *activityStructSize,

)

  Get the size of the activity struct for a given CUPTI version.

  This API is applicable only for predefined activity structs.

  Parameters:

    - activityKind – The activity kind to get the size for.

    - activityStructSize – The size of the activity struct.

    - version – The version of the CUPTI API. If 0, returns size for current version. If non-zero, returns size for the specified version. The version format is xxyyzz, e.g., 130000 for CUPTI 13.0, 130100 for CUPTI 13.1. The version of CUPTI can be queried using cuptiGetVersion API. Only versions >= 130000 are supported.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `activityStructSize` is NULL

    - CUPTI_ERROR_INVALID_KIND – if `activityKind` is invalid.

    - CUPTI_ERROR_NOT_SUPPORTED – if `version` is non-zero and is less than 130000.

CUptiResult cuptiActivityPopExternalCorrelationId(

  CUpti_ExternalCorrelationKind kind,
  uint64_t *lastId,

)

  Pop an external correlation id for the calling thread.

  This function notifies CUPTI that the calling thread is leaving an external API region.

  Parameters:

    - kind – The kind of external API activities should be correlated with.

    - lastId – If the function returns successful, contains the last external correlation id for this `kind`, can be NULL.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – The external API kind is invalid.

    - CUPTI_ERROR_QUEUE_EMPTY – No external id is currently associated with `kind`.

CUptiResult cuptiActivityPopExternalCorrelationId_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ExternalCorrelationKind kind,
  uint64_t *lastId,

)

  Pop an external correlation id for a specific subscriber.

  Subscriber aware V2 version of cuptiActivityPopExternalCorrelationId. This allows each subscriber to maintain its own external correlation context.

  Parameters:

    - subscriber – The subscriber handle.

    - kind – The kind of external API to pop correlation for.

    - lastId – Returns the last external correlation id popped, can be NULL.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if subscriber or kind is invalid.

    - CUPTI_ERROR_QUEUE_EMPTY – No external id is currently associated with `kind` for this subscriber.

CUptiResult cuptiActivityPushExternalCorrelationId(

  CUpti_ExternalCorrelationKind kind,
  uint64_t id,

)

  Push an external correlation id for the calling thread.

  This function notifies CUPTI that the calling thread is entering an external API region. When a CUPTI activity API record is created while within an external API region and CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION is enabled, the activity API record will be preceded by a CUpti_ActivityExternalCorrelation record for each CUpti_ExternalCorrelationKind.

  Parameters:

    - kind – The kind of external API activities should be correlated with.

    - id – External correlation id.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – The external API kind is invalid

CUptiResult cuptiActivityPushExternalCorrelationId_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ExternalCorrelationKind kind,
  uint64_t id,

)

  Push an external correlation id for a specific subscriber.

  Subscriber aware V2 version of cuptiActivityPushExternalCorrelationId. This allows each subscriber to maintain its own external correlation context.

  Parameters:

    - subscriber – The subscriber handle.

    - kind – The kind of external API activities should be correlated with.

    - id – External correlation id.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if subscriber or kind is invalid.

CUptiResult cuptiActivityRegisterCallbacks(

  CUpti_BuffersCallbackRequestFunc funcBufferRequested,
  CUpti_BuffersCallbackCompleteFunc funcBufferCompleted,

)

  Registers callback functions with CUPTI for activity buffer handling.

  This function registers two callback functions to be used in asynchronous buffer handling. If registered, activity record buffers are handled using asynchronous requested/completed callbacks from CUPTI.

  Registering these callbacks prevents the client from using CUPTI’s blocking enqueue/dequeue functions.

  Parameters:

    - funcBufferRequested – callback which is invoked when an empty buffer is requested by CUPTI

    - funcBufferCompleted – callback which is invoked when a buffer containing activity records is available from CUPTI

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if either `funcBufferRequested` or `funcBufferCompleted` is NULL

CUptiResult cuptiActivityRegisterCallbacks_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_BuffersCallbackRequestFunc_v2 funcBufferRequested,
  CUpti_BuffersCallbackCompleteFunc_v2 funcBufferCompleted,

)

  Registers callback functions with CUPTI for activity buffer handling for the subscriber.

  This function registers two callback functions to be used in asynchronous buffer handling. If registered, activity record buffers are handled using asynchronous requested/completed callbacks from CUPTI.

  Registering these callbacks prevents the client from using CUPTI’s blocking enqueue/dequeue functions.

  Parameters:

    - subscriber – The subscriber handle.

    - funcBufferRequested – callback which is invoked when an empty buffer is requested by CUPTI

    - funcBufferCompleted – callback which is invoked when a buffer containing activity records is available from CUPTI

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if either `funcBufferRequested` or `funcBufferCompleted_v2` is NULL

CUptiResult cuptiActivityRegisterTimestampCallback(

  CUpti_TimestampCallbackFunc funcTimestamp,

)

  Registers callback function with CUPTI for providing timestamp.

  This function registers a callback function to obtain timestamp of user’s choice instead of using CUPTI provided timestamp. By default CUPTI uses different methods, based on the underlying platform, to retrieve the timestamp Linux (x86_64, aarch64 sbsa, aarch64) uses clock_gettime(CLOCK_REALTIME) Windows uses QueryPerformanceCounter() WSL (Windows Subsystem for Linux) uses clock_gettime(CLOCK_MONOTONIC_RAW) as CLOCK_REALTIME can cause backward jumps. QNX uses ClockCycles() Timestamps retrieved using these methods are converted to nanosecond if needed before usage.

  Timestamps for GPU activities such as kernels, memory copies and memset operations are recorded directly on the GPU. To provide a unified and normalized view of these timestamps in relation to CPU time, CUPTI performs a linear interpolation to convert GPU timestamps into CPU timestamps during post-processing. For activities where timestamps are captured on the GPU, the timestamp callback is invoked during the post-processing phase, while converting GPU timestamps into CPU timestamps. For activities for which timestamps are captured directly on the CPU, the timestamp callback is invoked immediately at the time of the activity.

  The registration of timestamp callback should be done before any of the CUPTI activity kinds are enabled to make sure that all the records report the timestamp using the callback function registered through cuptiActivityRegisterTimestampCallback API.

  Changing the timestamp callback function in CUPTI through cuptiActivityRegisterTimestampCallback API in the middle of the profiling session can cause records generated prior to the change to report timestamps through previous timestamp method.

  Parameters:

    funcTimestamp – callback which is invoked when a timestamp is needed by CUPTI

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `funcTimestamp` is NULL

    - CUPTI_ERROR_NOT_INITIALIZED –

CUptiResult cuptiActivitySetAttribute(

  CUpti_ActivityAttribute attr,
  size_t *valueSize,
  void *value,

)

  Write an activity API attribute.

  Write an activity API attribute. In case of multiple subscribers, use cuptiActivitySetAttribute_v2 to write the attribute for the subscriber.

  Parameters:

    - attr – The attribute to write

    - valueSize – The size, in bytes, of the value

    - value – The attribute value to write

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_NOT_SUPPORTED – if multiple subscribers are not allowed.

    - CUPTI_ERROR_INVALID_PARAMETER – if `valueSize` or `value` is NULL, or if `attr` is not an activity attribute

    - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT – Indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiActivitySetAttribute_v2(

  CUpti_SubscriberHandle subscriber,
  CUpti_ActivityAttribute attr,
  size_t *valueSize,
  void *value,

)

  Write an activity API attribute.

  Write an activity API attribute. In case of multiple subscribers, use cuptiActivitySetAttribute_v2 to write the attribute for the subscriber.

  Parameters:

    - subscriber – The subscriber handle.

    - attr – The attribute to write

    - valueSize – The size, in bytes, of the value

    - value – The attribute value to write

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `valueSize` or `value` is NULL, or if `attr` is not an activity attribute

    - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT – Indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiComputeCapabilitySupported(

  int major,
  int minor,
  int *support,

)

  Check support for a compute capability.

  This function is used to check the support for a device based on it’s compute capability. It sets the `support` when the compute capability is supported by the current version of CUPTI, and clears it otherwise. This version of CUPTI might not support all GPUs sharing the same compute capability. It is suggested to use API cuptiDeviceSupported which provides correct information.

  See also

  cuptiDeviceSupported

  Parameters:

    - major – The major revision number of the compute capability

    - minor – The minor revision number of the compute capability

    - support – Pointer to an integer to return the support status

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `support` is NULL

CUptiResult cuptiDeviceSupported(CUdevice dev, int *support)

  Check support for a compute device.

  This function is used to check the support for a compute device. It sets the `support` when the device is supported by the current version of CUPTI, and clears it otherwise.

  See also

  cuptiComputeCapabilitySupported

  Parameters:

    - dev – The device handle returned by CUDA Driver API cuDeviceGet

    - support – Pointer to an integer to return the support status

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `support` is NULL

    - CUPTI_ERROR_INVALID_DEVICE – if `dev` is not a valid device

CUptiResult cuptiDeviceVirtualizationMode(

  CUdevice dev,
  CUpti_DeviceVirtualizationMode *mode,

)

  Query the virtualization mode of the device.

  This function is used to query the virtualization mode of the CUDA device.

  Parameters:

    - dev – The device handle returned by CUDA Driver API cuDeviceGet

    - mode – Pointer to an CUpti_DeviceVirtualizationMode to return the virtualization mode

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_DEVICE – if `dev` is not a valid device

    - CUPTI_ERROR_INVALID_PARAMETER – if `mode` is NULL

CUptiResult cuptiFinalize(void)

  Detach CUPTI from the running process.

  This API detaches the CUPTI from the running process. It destroys and cleans up all the resources associated with CUPTI in the current process. After CUPTI detaches from the process, the process will keep on running with no CUPTI attached to it. For safe operation of the API, it is recommended this API is invoked from the exit callsite of any of the CUDA Driver or Runtime API. Otherwise CUPTI client needs to make sure that required CUDA synchronization and CUPTI activity buffer flush is done before calling the API. Sample code showing the usage of the API in the cupti callback handler code:

      void CUPTIAPI
      cuptiCallbackHandler(void *userdata, CUpti_CallbackDomain domain,
          CUpti_CallbackId cbid, void *cbdata)
      {
        const CUpti_CallbackData *cbInfo = (CUpti_CallbackData *)cbdata;

        // Take this code path when CUPTI detach is requested
        if (detachCupti) {
          switch(domain)
          {
            case CUPTI_CB_DOMAIN_RUNTIME_API:
            case CUPTI_CB_DOMAIN_DRIVER_API:
              if (cbInfo->callbackSite == CUPTI_API_EXIT) {
                  // call the CUPTI detach API
                  cuptiFinalize();
              }
              break;
            default:
              break;
          }
        }
      }

CUptiResult cuptiGetAutoBoostState(

  CUcontext context,
  CUpti_ActivityAutoBoostState *state,

)

  Get auto boost state.

  The profiling results can be inconsistent in case auto boost is enabled. CUPTI tries to disable auto boost while profiling. It can fail to disable in cases where user does not have the permissions or CUDA_AUTO_BOOST env variable is set. The function can be used to query whether auto boost is enabled.

  Parameters:

    - context – A valid CUcontext.

    - state – A pointer to CUpti_ActivityAutoBoostState structure which contains the current state and the id of the process that has requested the current state

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `CUcontext` or `state` is NULL

    - CUPTI_ERROR_NOT_SUPPORTED – Indicates that the device does not support auto boost

    - CUPTI_ERROR_UNKNOWN – an internal error occurred

CUptiResult cuptiGetContextId(CUcontext context, uint32_t *contextId)

  Get the ID of a context.

  Get the ID of a context.

  Parameters:

    - context – The context

    - contextId – Returns a process-unique ID for the context

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_CONTEXT – The context is NULL or not valid.

    - CUPTI_ERROR_INVALID_PARAMETER – if `contextId` is NULL

CUptiResult cuptiGetDeviceId(CUcontext context, uint32_t *deviceId)

  Get the ID of a device.

  If `context` is NULL, returns the ID of the device that contains the currently active context. If `context` is non-NULL, returns the ID of the device which contains that context. Operates in a similar manner to cudaGetDevice() or cuCtxGetDevice() but may be called from within callback functions.

  Parameters:

    - context – The context, or NULL to indicate the current context.

    - deviceId – Returns the ID of the device that is current for the calling thread.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_DEVICE – if unable to get device ID

    - CUPTI_ERROR_INVALID_PARAMETER – if `deviceId` is NULL

CUptiResult cuptiGetGraphExecId(CUgraphExec graphExec, uint32_t *pId)

  Get the unique ID of executable graph.

  Returns the unique ID of executable CUDA graph.

  Parameters:

    - graphExec – The executable graph.

    - pId – Returns the unique ID of the executable graph

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `graph` is NULL

CUptiResult cuptiGetGraphId(CUgraph graph, uint32_t *pId)

  Get the unique ID of graph.

  Returns the unique ID of CUDA graph.

  Parameters:

    - graph – The graph.

    - pId – Returns the unique ID of the graph

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `graph` is NULL

CUptiResult cuptiGetGraphNodeId(CUgraphNode node, uint64_t *nodeId)

  Get the unique ID of a graph node.

  Returns the unique ID of the CUDA graph node.

  Parameters:

    - node – The graph node.

    - nodeId – Returns the unique ID of the node

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_PARAMETER – if `node` is NULL

CUptiResult cuptiGetLastError(void)

  Returns the last error from a cupti call or callback.

  Returns the last error that has been produced by any of the cupti api calls or the callback in the same host thread and resets it to CUPTI_SUCCESS.

CUptiResult cuptiGetStreamId(

  CUcontext context,
  CUstream stream,
  uint32_t *streamId,

)

  Get the ID of a stream.

  Get the ID of a stream. The stream ID is unique within a context (i.e. all streams within a context will have unique stream IDs).

  DEPRECATED This method is deprecated as of CUDA 8.0. Use method cuptiGetStreamIdEx instead.

  Parameters:

    - context – If non-NULL then the stream is checked to ensure that it belongs to this context. Typically this parameter should be null.

    - stream – The stream

    - streamId – Returns a context-unique ID for the stream

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_STREAM – if unable to get stream ID, or if `context` is non-NULL and `stream` does not belong to the context

    - CUPTI_ERROR_INVALID_PARAMETER – if `streamId` is NULL

CUptiResult cuptiGetStreamIdEx(

  CUcontext context,
  CUstream stream,
  uint8_t perThreadStream,
  uint32_t *streamId,

)

  Get the ID of a stream.

  Get the ID of a stream. The stream ID is unique within a context (i.e. all streams within a context will have unique stream IDs).

  Parameters:

    - context – If non-NULL then the stream is checked to ensure that it belongs to this context. Typically this parameter should be null.

    - stream – The stream

    - perThreadStream – Flag to indicate if program is compiled for per-thread streams

    - streamId – Returns a context-unique ID for the stream

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_INITIALIZED –

    - CUPTI_ERROR_INVALID_STREAM – if unable to get stream ID, or if `context` is non-NULL and `stream` does not belong to the context

    - CUPTI_ERROR_INVALID_PARAMETER – if `streamId` is NULL

CUptiResult cuptiGetThreadIdType(CUpti_ActivityThreadIdType *type)

  Get the thread-id type.

  Returns the thread-id type used in CUPTI This API is not supported when multiple subscribers are allowed. Use the corresponding attribute instead: CUPTI_ACTIVITY_ATTR_THREAD_ID_TYPE

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `type` is NULL

CUptiResult cuptiGetTimestamp(uint64_t *timestamp)

  Get the CUPTI timestamp.

  Returns a timestamp normalized to correspond with the start and end timestamps reported in the CUPTI activity records. The timestamp is reported in nanoseconds.

  Parameters:

    timestamp – Returns the CUPTI timestamp

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `timestamp` is NULL

CUptiResult cuptiGetTimestamp_v2(

  CUpti_SubscriberHandle subscriber,
  uint64_t *timestamp,

)

  Get the CUPTI timestamp (API currently in beta).

  If a subscriber registers a particular timestamp callback, this API will use that callback to get the timestamp. In CUDA 13.3, this will fall back to cuptiGetTimestamp(). In future versions, this will provide the timestamp callback registered by the requesting subscriber, and fallback to cuptiGetTimestamp() if no callback is registered.

  Returns a timestamp normalized to correspond with the start and end timestamps reported in the CUPTI activity records. The timestamp is reported in nanoseconds.

  Parameters:

    - subscriber – The subscriber handle

    - timestamp – Returns the CUPTI timestamp

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `timestamp` is NULL or `subscriber` is NULL

CUptiResult cuptiIsTracingSessionRunning(uint8_t *isRunning)

  Check whether a CUPTI tracing session is still running.

  This API returns true if a CUPTI library is already loaded by another CUPTI user by using any CUPTI API. This API returns false when CUPTI is finalized and there is no CUPTI currently loaded and active. Can be used to determine if it is safe to unload your CUPTI based tool. Note that this API itself does not load the CUPTI library, it merely checks if a CUPTI library is already loaded by another CUPTI user.

  Parameters:

    isRunning – Returns whether the tracing session is still running.

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_INVALID_PARAMETER – if `isRunning` is NULL.

    - CUPTI_ERROR_UNKNOWN – if an unknown error occurred.

CUptiResult cuptiSetThreadIdType(CUpti_ActivityThreadIdType type)

  Set the thread-id type.

  CUPTI uses the method corresponding to set type to generate the thread-id. See enum CUpti_ActivityThreadIdType for the list of methods. Activity records having thread-id field contain the same value. Thread id type must not be changed during the profiling session to avoid thread-id value mismatch across activity records. This API is not supported when multiple subscribers are allowed. Use the corresponding attribute instead: CUPTI_ACTIVITY_ATTR_THREAD_ID_TYPE

  Return values:

    - CUPTI_SUCCESS –

    - CUPTI_ERROR_NOT_SUPPORTED – if `type` is not supported on the platform

## 6.1.9. Typedefs

typedef void (*CUpti_BuffersCallbackCompleteFunc)(CUcontext context, uint32_t streamId, uint8_t *buffer, size_t size, size_t validSize)

  Function type for callback used by CUPTI to return a buffer of activity records.

  This callback function returns to the CUPTI client a buffer containing activity records. The buffer contains `validSize` bytes of activity records which should be read using cuptiActivityGetNextRecord. The number of dropped records can be read using cuptiActivityGetNumDroppedRecords. After this call CUPTI relinquished ownership of the buffer and will not use it anymore. The client may return the buffer to CUPTI using the CUpti_BuffersCallbackRequestFunc callback. Note: CUDA 6.0 onwards, all buffers returned by this callback are global buffers i.e. there is no context/stream specific buffer. User needs to parse the global buffer to extract the context/stream specific activity records.

  Param context:

    The context this buffer is associated with. If NULL, the buffer is associated with the global activities. This field is deprecated as of CUDA 6.0 and will always be NULL.

  Param streamId:

    The stream id this buffer is associated with. This field is deprecated as of CUDA 6.0 and will always be NULL.

  Param buffer:

    The activity record buffer.

  Param size:

    The total size of the buffer in bytes as set in CUpti_BuffersCallbackRequestFunc.

  Param validSize:

    The number of valid bytes in the buffer.

typedef void (*CUpti_BuffersCallbackCompleteFunc_v2)(uint8_t *buffer, size_t size, size_t validSize, CUpti_BufferCallbackCompleteInfo *pBufferCompleteInfo)

  Function type for callback used by CUPTI to return a buffer of activity records.

  This callback function returns to the CUPTI client a buffer containing activity records. The buffer contains `validSize` bytes of activity records which should be read using cuptiActivityGetNextRecord. The number of dropped records can be read using cuptiActivityGetNumDroppedRecords. After this call CUPTI relinquished ownership of the buffer and will not use it anymore. The client may return the buffer to CUPTI using the CUpti_BuffersCallbackRequestFunc callback. Note: CUDA 6.0 onwards, all buffers returned by this callback are global buffers i.e. there is no context/stream specific buffer. User needs to parse the global buffer to extract the context/stream specific activity records.

  Param buffer:

    The activity record buffer.

  Param size:

    The total size of the buffer in bytes as set in CUpti_BuffersCallbackRequestFunc.

  Param validSize:

    The number of valid bytes in the buffer.

  Param pBufferCompleteInfo:

    Additional information about the completed buffer.

typedef void (*CUpti_BuffersCallbackRequestFunc)(uint8_t **buffer, size_t *size, size_t *maxNumRecords)

  Function type for callback used by CUPTI to request an empty buffer for storing activity records.

  This callback function signals the CUPTI client that an activity buffer is needed by CUPTI. The activity buffer is used by CUPTI to store activity records. The callback function can decline the request by setting `*buffer` to NULL. In this case CUPTI may drop activity records.

  Param buffer:

    Returns the new buffer. If set to NULL then no buffer is returned.

  Param size:

    Returns the size of the returned buffer.

  Param maxNumRecords:

    Returns the maximum number of records that should be placed in the buffer. If 0 then the buffer is filled with as many records as possible. If > 0 the buffer is filled with at most that many records before it is returned.

typedef void (*CUpti_BuffersCallbackRequestFunc_v2)(uint8_t **buffer, size_t *size, size_t *maxNumRecords, CUpti_BufferCallbackRequestInfo *pBufferRequestInfo)

  Function type for callback used by CUPTI to request an empty buffer for storing activity records.

  This callback function signals the CUPTI client that an activity buffer is needed by CUPTI. The activity buffer is used by CUPTI to store activity records. The callback function can decline the request by setting `*buffer` to NULL. In this case CUPTI may drop activity records.

  Param buffer:

    Returns the new buffer. If set to NULL then no buffer is returned.

  Param size:

    Returns the size of the returned buffer.

  Param maxNumRecords:

    Returns the maximum number of records that should be placed in the buffer. If 0 then the buffer is filled with as many records as possible. If > 0 the buffer is filled with at most that many records before it is returned.

  Param pBufferRequestInfo:

    Additional information about the requested buffer.

typedef uint64_t (*CUpti_TimestampCallbackFunc)(void)

  Function type for callback used by CUPTI to request a timestamp to be used in activity records.

  This callback function signals the CUPTI client that a timestamp needs to be returned. This timestamp would be treated as normalized timestamp to be used for various purposes in CUPTI. For example to store start and end timestamps reported in the CUPTI activity records. The returned timestamp must be in nanoseconds.

  See also

  cuptiActivityRegisterTimestampCallback