Skip to main content
`Ctrl`+`K`

# 7.42. CUpti_ActivityGreenContext2

struct CUpti_ActivityGreenContext2

  The activity record for a green context (version 2).

  This activity record represents information about a green context (CUPTI_ACTIVITY_KIND_GREEN_CONTEXT). This is an enhanced version of CUpti_ActivityGreenContext that adds work queue configuration fields.

  The corresponding activity kind is CUPTI_ACTIVITY_KIND_GREEN_CONTEXT.

  Green contexts enable resource partitioning by allocating a subset of SMs (Streaming Multiprocessors) from the GPU to a context.

  TPC (Thread Processing Cluster)

    Thread Processing Clusters are hardware units within a GPC (Graphics Processing Cluster). Each TPC contains one or more SMs, along with texture units, L1 cache, instruction cache, and constant cache. Green contexts allocate resources at the TPC level.

  Public Members

  CUpti_ActivityKind kind

    The activity record kind, must be CUPTI_ACTIVITY_KIND_GREEN_CONTEXT.

  uint32_t contextId

    The context ID of the green context.

  uint32_t parentContextId

    The ID of the parent context.

  uint32_t deviceId

    The device ID associated with the green context.

  uint32_t numTpcs

    The number of TPCs allocated to the green context.

  uint16_t numMultiprocessors

    The number of multiprocessors (SMs) allocated to the green context.

  uint8_t logicalTpcMaskSize

    The size (in 32-bit words) of the logical TPC mask stored in logicalTpcMask[].

  uint8_t padding

    Undefined.

    Reserved for internal use.

  uint32_t logicalTpcMask[32]

    Bitset of allocated TPC IDs represented as 32-bit words.

    Valid words are specified by logicalTpcMaskSize; unused entries are zeroed. The array supports up to 1024 TPCs (32 words × 32 bits). Each bit represents a logical TPC ID assigned to the green context. For example, if bit k is set, logical TPC ID k is assigned to the context.

    Example: Interpreting the TPC Mask

      For a green context with numTpcs=3, logicalTpcMaskSize=8, and logicalTpcMask={66,8,0,0,0,0,0,0}:

      - Word 0: Value 66 (binary: …01000010, showing lowest 8 bits of 32-bit word) indicates TPCs 1 and 6

      - Word 1: Value 8 (binary: …00001000) indicates TPC 35 (bit 3 of word 1, i.e., global TPC ID 32+3)

      - Each word is 32 bits covering TPCs 0-31 (word 0), 32-63 (word 1), etc.

      - To check if TPC N is allocated: ``(logicalTpcMask[N/32] & (1U << (N%32)))

      - logicalTpcMaskSize indicates how many words in the array contain valid data

  uint64_t workqueueResourceId

    The work queue resource ID associated with the green context.

    This is a unique identifier for the work queue resource used by this green context.

  uint32_t workqueueConcurrencyLimit

    The concurrency limit for the work queue associated with the green context.

    This defines the maximum number of concurrent operations allowed on this work queue.

  uint32_t workqueueSharingScope

    The sharing scope for the work queue associated with the green context.

    This defines how the work queue can be shared across different contexts or processes. Refer

    Param CUdevWorkqueueConfigScope:

      in cuda.h for possible values.